<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="40.64" y2="0" width="0" layer="20"/>
<wire x1="40.64" y1="0" x2="40.64" y2="25.4" width="0" layer="20"/>
<wire x1="40.64" y1="25.4" x2="0" y2="25.4" width="0" layer="20"/>
<wire x1="0" y1="25.4" x2="0" y2="0" width="0" layer="20"/>
<hole x="2.54" y="22.86" drill="2"/>
<hole x="2.54" y="2.54" drill="2"/>
<hole x="38.1" y="22.86" drill="2"/>
<hole x="38.1" y="2.54" drill="2"/>
<text>(c) 2013 Wyvernworks</text>
<text>Reg DC Supply</text>
</plain>
<libraries>
<library name="SparkFun">
<packages>
<package name="TO220-IGO">
</package>
<package name="CPOL-RADIAL-100UF-25V">
</package>
<package name="AXIAL-5MM">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="E5-10,5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5.08 mm, diameter 10.5 mm</description>
</package>
</packages>
</library>
<library name="diode">
<packages>
<package name="DO41-10">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 2.54 mm, horizontal, grid 10.16 mm</description>
</package>
</packages>
</library>
<library name="wirepad">
<packages>
<package name="3,81/1,4">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.3">
</package>
</packages>
</library>
<library name="mylogos">
<description>My Logos</description>
<packages>
<package name="WYVERN-BOT-4MIL3">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="LM7805" library="SparkFun" package="TO220-IGO" value="7805"/>
<element name="C1" library="adafruit" package="E5-10,5" value="1000uf"/>
<element name="C2" library="SparkFun" package="AXIAL-5MM" value=".1uf"/>
<element name="LED1" library="SparkFun-LED" package="LED3MM" value="3mm red"/>
<element name="D1" library="diode" package="DO41-10" value="1N4004"/>
<element name="R1" library="SparkFun-Resistors" package="AXIAL-0.3" value="100ohm"/>
<element name="IN+" library="wirepad" package="3,81/1,4" value="IN+"/>
<element name="IN-" library="wirepad" package="3,81/1,4" value="IN-"/>
<element name="OUT+" library="wirepad" package="3,81/1,4" value="OUT+"/>
<element name="OUT-" library="wirepad" package="3,81/1,4" value="OUT-"/>
<element name="C3" library="SparkFun" package="CPOL-RADIAL-100UF-25V" value="10uf"/>
<element name="C4" library="SparkFun" package="CPOL-RADIAL-100UF-25V" value="100uf"/>
<element name="U$1" library="mylogos" package="WYVERN-BOT-4MIL3" value=""/>
</elements>
<signals>
<signal name="N$1">
<contactref element="IN+" pad="1"/>
<contactref element="C1" pad="+"/>
<contactref element="LM7805" pad="IN"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="LM7805" pad="OUT"/>
<contactref element="C2" pad="P$1"/>
<contactref element="LED1" pad="A"/>
<contactref element="OUT+" pad="1"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="IN-" pad="1"/>
<contactref element="D1" pad="C"/>
</signal>
<signal name="N$4">
<contactref element="R1" pad="P$1"/>
<contactref element="OUT-" pad="1"/>
<contactref element="C2" pad="P$2"/>
<contactref element="LM7805" pad="GND"/>
<contactref element="C1" pad="-"/>
<contactref element="D1" pad="A"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="LED1" pad="K"/>
<contactref element="R1" pad="P$2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
