<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="11.43" x2="0" y2="1.27" width="0" layer="20"/>
<wire x1="0" y1="1.27" x2="1.27" y2="0" width="0" layer="20" curve="90"/>
<wire x1="1.27" y1="0" x2="19.05" y2="0" width="0" layer="20"/>
<wire x1="19.05" y1="0" x2="20.32" y2="1.27" width="0" layer="20" curve="90"/>
<wire x1="20.32" y1="1.27" x2="20.32" y2="11.43" width="0" layer="20"/>
<wire x1="20.32" y1="11.43" x2="19.05" y2="12.7" width="0" layer="20" curve="90"/>
<wire x1="19.05" y1="12.7" x2="1.27" y2="12.7" width="0" layer="20"/>
<wire x1="1.27" y1="12.7" x2="0" y2="11.43" width="0" layer="20" curve="90"/>
<text>Breadboard ravine spacing
starts at 0.3", then every 0.1"</text>
<text>0</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>Gnd</text>
<text>SDA</text>
<text>SCL</text>
<text>Pwr</text>
<text>LP5810 
Breakout V1.1
Sept 2024
M Sandercock</text>
<text>Pwr</text>
<text>SCL</text>
<text>SDA</text>
<text>Gnd</text>
<text>0</text>
<text>1</text>
<text>2</text>
<text>3</text>
</plain>
<libraries>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun LEDs&lt;/h3&gt;
This library contains discrete LEDs for illumination or indication, but no displays.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-0603">
<description>&lt;B&gt;LED 0603 SMT&lt;/B&gt;&lt;p&gt;
0603, surface mount.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.075inch &lt;/li&gt;
&lt;li&gt;Area: 0.06" x 0.03"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;LED - BLUE&lt;/li&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DUMMY">
<description>NOTHING HERE!!! For when you want a symbol with no package as an option against symbols with a package.</description>
</package>
</packages>
</library>
<library name="SparkFun-PowerIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find drivers, regulators, and amplifiers.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DSD0008B">
<description>This is brought into the library for the LP5810_DSD_ LED driver chip.
&lt;p&gt;Texas Instruments uses DSD as the ordering code for this variant of the chip
&lt;br&gt;However they also call this a WSON package but it's 3x3mm, much bigger than the other WSON package we have in this library
&lt;br&gt;Based off MSO8-EP, which has the same pitch and package size but that has legs instead of the flank-pads this one has.</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X04-1MM-RA">
</package>
<package name="1X04_NO_SILK_ALL_ROUND">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun-Passives" package="0805" value="0.1uF"/>
<element name="D0" library="SparkFun-LED" package="LED-0603" value="RED">
<attribute name="PROD_ID" value="DIO-00819"/>
</element>
<element name="D1" library="SparkFun-LED" package="LED-0603" value="RED">
<attribute name="PROD_ID" value="DIO-00819"/>
</element>
<element name="D2" library="SparkFun-LED" package="LED-0603" value="RED">
<attribute name="PROD_ID" value="DIO-00819"/>
</element>
<element name="D3" library="SparkFun-LED" package="LED-0603" value="RED">
<attribute name="PROD_ID" value="DIO-00819"/>
</element>
<element name="FRAME1" library="SparkFun-Aesthetics" package="DUMMY" value="FRAME-LETTERNO_PACKAGE">
<attribute name="DESIGNER" value="Nobody"/>
<attribute name="VERSION" value="v01"/>
</element>
<element name="IC1" library="SparkFun-PowerIC" package="DSD0008B" value="LP5810_DSD"/>
<element name="J1" library="SparkFun-Connectors" package="1X04-1MM-RA" value="QWIIC">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="1X04_NO_SILK_ALL_ROUND" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="1X04_NO_SILK_ALL_ROUND" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="IC1" pad="EP"/>
<contactref element="J1" pad="1"/>
<contactref element="JP1" pad="1"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="3.3V">
<contactref element="IC1" pad="1"/>
<contactref element="D0" pad="A"/>
<contactref element="D1" pad="A"/>
<contactref element="D2" pad="A"/>
<contactref element="D3" pad="A"/>
<contactref element="J1" pad="2"/>
<contactref element="JP1" pad="4"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="SCL">
<contactref element="IC1" pad="3"/>
<contactref element="J1" pad="4"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="SDA">
<contactref element="IC1" pad="4"/>
<contactref element="J1" pad="3"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="OUT0">
<contactref element="IC1" pad="8"/>
<contactref element="D0" pad="C"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="OUT1">
<contactref element="IC1" pad="7"/>
<contactref element="D1" pad="C"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="OUT2">
<contactref element="IC1" pad="6"/>
<contactref element="D2" pad="C"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="OUT3">
<contactref element="IC1" pad="5"/>
<contactref element="D3" pad="C"/>
<contactref element="JP2" pad="4"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
