<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.5.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="1.27" x2="0" y2="26.67" width="0.1524" layer="20"/>
<wire x1="1.27" y1="27.94" x2="26.67" y2="27.94" width="0.1524" layer="20"/>
<wire x1="27.94" y1="26.67" x2="27.94" y2="1.27" width="0.1524" layer="20"/>
<text>COIL</text>
<text>ATTINY85
20SU</text>
<wire x1="26.67" y1="0" x2="1.27" y2="0" width="0.1524" layer="20"/>
<wire x1="0" y1="26.67" x2="1.27" y2="27.94" width="0.1524" layer="20" curve="-90"/>
<wire x1="26.67" y1="27.94" x2="27.94" y2="26.67" width="0.1524" layer="20" curve="-90"/>
<wire x1="1.27" y1="0" x2="0" y2="1.27" width="0.1524" layer="20" curve="-90"/>
<wire x1="27.94" y1="1.27" x2="26.67" y2="0" width="0.1524" layer="20" curve="-90"/>
<text>MagSpoof</text>
</plain>
<libraries>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun LEDs&lt;/h3&gt;
This library contains discrete LEDs for illumination or indication, but no displays.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED_3MM-NS">
<description>&lt;h3&gt;LED 3MM PTH- No Silk&lt;/h3&gt;

3 mm, round, no silk outline of package

&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.1inch&lt;/li&gt;
&lt;li&gt;Diameter: 3mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;LED&lt;/li&gt;&lt;/ul&gt;</description>
</package>
</packages>
</library>
<library name="st-microelectronics">
<description>&lt;b&gt;ST Microelectronics Devices&lt;/b&gt;&lt;p&gt;
Microcontrollers,  I2C components, linear devices&lt;p&gt;
http://www.st.com&lt;p&gt;
&lt;i&gt;Include st-microelectronics-2.lbr, st-microelectronics-3.lbr.&lt;p&gt;&lt;/i&gt;

&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL16">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.6">
<description>1W Resistor, 0.6" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.3">
<description>&lt;h3&gt;AXIAL-0.3&lt;/h3&gt;
&lt;p&gt;Commonly used for 1/4W through-hole resistors. 0.3" pitch between holes.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="Atmel">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 27/07/2012 14:02:49</description>
<packages>
<package name="SOIC127P798X216-8N">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="TACT_PANA-EVQ">
</package>
<package name="JST-PH-2-THM-RA">
<description>&lt;b&gt;S2B-PH-K-S&lt;/b&gt; 
&lt;p&gt;
JST PH 2-pin thru-home side entry</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Capacitors&lt;/h3&gt;
This library contains capacitors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CPOL-RADIAL-2.5MM-6.5MM">
<description>2.5 mm spaced PTHs with 6.5 mm diameter outline</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X3-NS">
<description>&lt;h3&gt;Plated Through Hole - 2x3 No Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="D1" library="SparkFun-LED" package="LED_3MM-NS" value="LED1">
<attribute name="VALUE"/>
</element>
<element name="IC2" library="st-microelectronics" package="DIL16" value="L293D">
<attribute name="MF" value=""/>
<attribute name="MPN" value="L293D"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="9589619"/>
<attribute name="OC_NEWARK" value="56P8249"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="SparkFun-Passives" package="AXIAL-0.6" value="COIL">
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="AXIAL-0.3" value="100Ω">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08380"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="Atmel" package="SOIC127P798X216-8N" value="ATTINY85-20SU">
<attribute name="MPN" value="ATTINY85-20SU"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="1455164"/>
<attribute name="OC_NEWARK" value="58M3797"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="Atmel"/>
</element>
<element name="SW1" library="adafruit" package="TACT_PANA-EVQ" value=""/>
<element name="C1" library="SparkFun-Capacitors" package="CPOL-RADIAL-2.5MM-6.5MM" value="100uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08439"/>
<attribute name="VALUE"/>
</element>
<element name="BAT" library="adafruit" package="JST-PH-2-THM-RA" value="">
<attribute name="NAME"/>
</element>
<element name="ICSP" library="SparkFun-Connectors" package="2X3-NS" value="AVR_SPI_PROG_3X2NS">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="GND3">
<contactref element="IC2" pad="13"/>
</signal>
<signal name="GND4">
<contactref element="IC2" pad="12"/>
</signal>
<signal name="VCC">
<contactref element="IC2" pad="16"/>
<contactref element="C1" pad="1"/>
<contactref element="IC2" pad="8"/>
<contactref element="IC1" pad="8"/>
<contactref element="BAT" pad="1"/>
<contactref element="ICSP" pad="2"/>
</signal>
<signal name="PB3">
<contactref element="IC1" pad="2"/>
<contactref element="D1" pad="A"/>
<contactref element="IC2" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="R1" pad="P$2"/>
<contactref element="D1" pad="K"/>
</signal>
<signal name="GND">
<contactref element="R1" pad="P$1"/>
<contactref element="C1" pad="2"/>
<contactref element="IC2" pad="4"/>
<contactref element="IC2" pad="5"/>
<contactref element="SW1" pad="P$1"/>
<contactref element="IC1" pad="4"/>
<contactref element="BAT" pad="2"/>
<contactref element="ICSP" pad="6"/>
</signal>
<signal name="N$5">
<contactref element="L1" pad="P$1"/>
<contactref element="IC2" pad="3"/>
</signal>
<signal name="N$6">
<contactref element="L1" pad="P$2"/>
<contactref element="IC2" pad="6"/>
</signal>
<signal name="PB1">
<contactref element="IC1" pad="6"/>
<contactref element="IC2" pad="7"/>
<contactref element="ICSP" pad="1"/>
</signal>
<signal name="PB0">
<contactref element="ICSP" pad="4"/>
<contactref element="IC1" pad="5"/>
<contactref element="IC2" pad="2"/>
</signal>
<signal name="PB5">
<contactref element="ICSP" pad="5"/>
<contactref element="IC1" pad="1"/>
</signal>
<signal name="PB2">
<contactref element="ICSP" pad="3"/>
<contactref element="IC1" pad="7"/>
<contactref element="SW1" pad="P$2"/>
</signal>
<signal name="PB4">
<contactref element="IC1" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
