<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.0.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="0" y2="44.45" width="0.2032" layer="20"/>
<wire x1="0" y1="44.45" x2="41.91" y2="44.45" width="0.2032" layer="20"/>
<wire x1="41.91" y1="44.45" x2="41.91" y2="0" width="0.2032" layer="20"/>
<wire x1="41.91" y1="0" x2="0" y2="0" width="0.2032" layer="20"/>
<text>Weather
Station v1</text>
<text>Inspired by https://goo.gl/YO0Epf</text>
</plain>
<libraries>
<library name="SparkFun-Sensors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find sensors- accelerometers, gyros, compasses, magnetometers, light sensors, imagers, temp sensors, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="PHOTOCELL">
</package>
</packages>
</library>
<library name="junkFromResistors">
<packages>
<package name="AXIAL-0.5">
<description>1/2W Resistor, 0.5" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
</packages>
</library>
<library name="Particle-Devices">
<description>&lt;h3&gt;Reference foot prints for Particle devices&lt;/h3&gt;
In this library you'll find foot prints to make circuit boards using the Particle devices: Spark Core, Photon and Electron.&lt;br&gt;&lt;br&gt;
There are for reference and you may need to adjust them for your application. See https://docs.particle.io for more details on the recommended layouts for Particle devices.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Designed by Particle. Distributed under a Creative Commons Attribution, Share-Alike license. Development kits based on this library should be distributed under a similar license. Commercial products using this library as a reference design need not comply with this license; further questions can be sent to hello@particle.io. Check license.txt for more information.</description>
<packages>
<package name="PHOTON">
</package>
</packages>
</library>
<library name="DHT11">
<packages>
<package name="DHT11-PION.">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="PHOTOCELL" library="SparkFun-Sensors" package="PHOTOCELL" value="PHOTOCELLPTH"/>
<element name="R2" library="junkFromResistors" package="AXIAL-0.5" value="4.7K"/>
<element name="R1" library="junkFromResistors" package="AXIAL-0.5" value="10K"/>
<element name="PARTICLE_PHOTON" library="Particle-Devices" package="PHOTON" value="PHOTON_WITH_HEADERS"/>
<element name="U$2" library="DHT11" package="DHT11-PION." value="DHT11-PION."/>
</elements>
<signals>
<signal name="VIN">
<contactref element="PARTICLE_PHOTON" pad="1"/>
</signal>
<signal name="GND">
<contactref element="PARTICLE_PHOTON" pad="2"/>
</signal>
<signal name="VBAT">
<contactref element="PARTICLE_PHOTON" pad="22"/>
</signal>
<signal name="N$1">
<contactref element="PARTICLE_PHOTON" pad="24"/>
<contactref element="U$2" pad="VCC"/>
<contactref element="R2" pad="P$1"/>
<contactref element="PHOTOCELL" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="R2" pad="P$2"/>
<contactref element="U$2" pad="DATA"/>
<contactref element="PARTICLE_PHOTON" pad="18"/>
</signal>
<signal name="N$6">
<contactref element="U$2" pad="GND"/>
<contactref element="PARTICLE_PHOTON" pad="21"/>
<contactref element="R1" pad="P$1"/>
</signal>
<signal name="N$2">
<contactref element="PHOTOCELL" pad="2"/>
<contactref element="R1" pad="P$2"/>
<contactref element="PARTICLE_PHOTON" pad="12"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
