<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.4.3">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="31.75" y2="0" width="0" layer="20"/>
<wire x1="31.75" y1="0" x2="31.75" y2="25.4" width="0" layer="20"/>
<wire x1="31.75" y1="25.4" x2="0" y2="25.4" width="0" layer="20"/>
<wire x1="0" y1="25.4" x2="0" y2="0" width="0" layer="20"/>
<text>Geppetto
Electronics</text>
<text>NMEA</text>
<text>DIAG</text>
<text>TX SEL</text>
<text>GPSDO&lt;-&gt;USB</text>
</plain>
<libraries>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="74xx-little-us">
<description>&lt;b&gt;Single and Dual Gates Family, US symbols&lt;/b&gt;&lt;p&gt;
Little logic devices from Texas Instruments&lt;br&gt;
TinyLogic(R) from FAIRCHILD Semiconductor TM
&lt;p&gt;
&lt;author&gt;Created by evgeni@eniks.com&lt;/author&gt;&lt;br&gt;
&lt;author&gt;Extended by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;&lt;p&gt;
SOT753 - Philips Semiconductors&lt;br&gt;
Source: http://www.semiconductors.philips.com/acrobat_download/datasheets/74HC_HCT1G66_3.pdf</description>
</package>
</packages>
</library>
<library name="CUI-VSK-S10">
<packages>
<package name="MD-60S">
</package>
</packages>
</library>
<library name="SparkFun-Connectors-new">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X03">
</package>
</packages>
</library>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SSOP28DB">
<description>&lt;b&gt;Small Shrink Outline Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="USB-MICROB">
<description>Micro USB Package</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun-Capacitors" package="0805" value="0.1µF">
<attribute name="NAME"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0805" value="0.1µF">
<attribute name="NAME"/>
</element>
<element name="C6" library="SparkFun-Capacitors" package="0805" value="4700pF">
<attribute name="NAME"/>
</element>
<element name="IC2" library="74xx-little-us" package="SOT23-5" value="74AHC1GU04DBV">
<attribute name="NAME"/>
</element>
<element name="JP1" library="CUI-VSK-S10" package="MD-60S" value="MD-60S"/>
<element name="JP2" library="SparkFun-Connectors-new" package="1X03" value="M03PTH"/>
<element name="IC1" library="SparkFun-DigitalIC" package="SSOP28DB" value="CY7C65213">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="IC-12487"/>
</element>
<element name="U$1" library="SparkFun-Connectors" package="USB-MICROB" value="USB-5PIN-MICROB"/>
<element name="R1" library="SparkFun-Resistors" package="0805" value="4.7kΩ">
<attribute name="NAME"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0805" value="10kΩ">
<attribute name="NAME"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="0805" value="1MΩ">
<attribute name="NAME"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="0805" value="0.1µF">
<attribute name="NAME"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="0805" value="0.1µF">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="PPS">
<contactref element="JP1" pad="1"/>
<contactref element="IC2" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="IC2" pad="4"/>
<contactref element="IC1" pad="10"/>
</signal>
<signal name="N$6">
<contactref element="JP1" pad="3"/>
<contactref element="IC1" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="JP2" pad="2"/>
<contactref element="IC1" pad="5"/>
</signal>
<signal name="G_TX">
<contactref element="JP1" pad="2"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="N$9">
<contactref element="JP1" pad="4"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="GND">
<contactref element="JP1" pad="5"/>
<contactref element="JP1" pad="TAB"/>
<contactref element="IC2" pad="3"/>
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="IC1" pad="21"/>
<contactref element="IC1" pad="18"/>
<contactref element="IC1" pad="7"/>
<contactref element="U$1" pad="GND"/>
<contactref element="R2" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="C6" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
</signal>
<signal name="+5V">
<contactref element="JP1" pad="6"/>
<contactref element="IC2" pad="5"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="IC1" pad="4"/>
</signal>
<signal name="NC1">
<contactref element="IC1" pad="25"/>
</signal>
<signal name="N$1">
<contactref element="IC1" pad="16"/>
<contactref element="U$1" pad="D-"/>
</signal>
<signal name="N$2">
<contactref element="U$1" pad="D+"/>
<contactref element="IC1" pad="15"/>
</signal>
<signal name="N$5">
<contactref element="IC1" pad="20"/>
<contactref element="U$1" pad="VBUS"/>
<contactref element="R1" pad="2"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="IC1" pad="19"/>
<contactref element="R1" pad="1"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="U$1" pad="MT2"/>
<contactref element="U$1" pad="MT3"/>
<contactref element="U$1" pad="MT1"/>
<contactref element="U$1" pad="MT4"/>
<contactref element="R3" pad="2"/>
<contactref element="C6" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="IC1" pad="17"/>
<contactref element="C3" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
