<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="0" y1="12.705" x2="0" y2="0.79375" width="0" layer="20"/>
<wire x1="0" y1="0.79375" x2="0.635" y2="0.15875" width="0" layer="20" curve="90"/>
<wire x1="0.635" y1="0.15875" x2="7.585" y2="0.15875" width="0" layer="20"/>
<wire x1="7.585" y1="0.15875" x2="8.22" y2="0.79375" width="0" layer="20" curve="90"/>
<wire x1="8.22" y1="0.79375" x2="8.22" y2="12.705" width="0" layer="20"/>
<wire x1="8.22" y1="12.705" x2="7.585" y2="13.34" width="0" layer="20" curve="90"/>
<wire x1="7.585" y1="13.34" x2="0.635" y2="13.34" width="0" layer="20"/>
<wire x1="0.635" y1="13.34" x2="0" y2="12.705" width="0" layer="20" curve="90"/>
<text>1</text>
<text>protofusion.org</text>
<text>Rev. 0</text>
<text>2013</text>
<text>VCC</text>
</plain>
<libraries>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X3_LOCK">
</package>
<package name="SJ_2S-NO">
<description>Small solder jumper with no paste layer so it will open after reflow.</description>
</package>
<package name="LED-0603">
</package>
</packages>
</library>
<library name="Protofusion">
<packages>
<package name="POGOPROG-BACKMOUNT">
</package>
<package name="POGOPROG_LOGO">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="SparkFun" package="2X3_LOCK" value="AVR_SPI_PRG_62X3_LOCK"/>
<element name="J2" library="Protofusion" package="POGOPROG-BACKMOUNT" value="POGOPIN-BACKBOARD"/>
<element name="SJ1" library="SparkFun" package="SJ_2S-NO" value="SOLDERJUMPERNO"/>
<element name="LED1" library="SparkFun" package="LED-0603" value=""/>
<element name="R1" library="adafruit" package="R0603" value=""/>
<element name="U$2" library="Protofusion" package="POGOPROG_LOGO" value=""/>
</elements>
<signals>
<signal name="MOSI">
<contactref element="J2" pad="6"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="MISO">
<contactref element="J2" pad="5"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="SCK">
<contactref element="J2" pad="4"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="RST">
<contactref element="J2" pad="7"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="GND">
<contactref element="J2" pad="3"/>
<contactref element="J1" pad="6"/>
<contactref element="LED1" pad="C"/>
</signal>
<signal name="N$2">
<contactref element="SJ1" pad="2"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="R1" pad="1"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="VCC">
<contactref element="J1" pad="2"/>
<contactref element="SJ1" pad="1"/>
<contactref element="R1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
