<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.6.0">
<drawing>
<board>
<plain>
<wire x1="-0.512128125" y1="4.05" x2="-1.5" y2="4.05" width="0" layer="20"/>
<wire x1="-1.5" y1="4.05" x2="-2.25" y2="4.8" width="0" layer="20" curve="-90"/>
<wire x1="-2.25" y1="4.8" x2="-2.25" y2="8.4" width="0" layer="20"/>
<wire x1="-0.512128125" y1="4.05" x2="0" y2="3.537871875" width="0" layer="20" curve="-90"/>
<wire x1="0" y1="3.537871875" x2="0" y2="0.15" width="0" layer="20"/>
<wire x1="0" y1="0.15" x2="0.15" y2="0" width="0" layer="20" curve="90"/>
<wire x1="0.15" y1="0" x2="12.6" y2="0" width="0" layer="20"/>
<wire x1="12.6" y1="0" x2="12.6" y2="3.537871875" width="0" layer="20"/>
<wire x1="12.6" y1="3.537871875" x2="13.112128125" y2="4.05" width="0" layer="20" curve="-90"/>
<wire x1="13.112128125" y1="4.05" x2="14.337871875" y2="4.05" width="0" layer="20"/>
<wire x1="14.337871875" y1="4.05" x2="14.85" y2="4.562128125" width="0" layer="20" curve="90"/>
<wire x1="14.85" y1="4.562128125" x2="14.85" y2="8.637871875" width="0" layer="20"/>
<wire x1="14.85" y1="8.637871875" x2="14.337871875" y2="9.15" width="0" layer="20" curve="90"/>
<wire x1="-2.25" y1="8.4" x2="-1.5" y2="9.15" width="0" layer="20" curve="-90"/>
<wire x1="-1.5" y1="9.15" x2="14.337871875" y2="9.15" width="0" layer="20"/>
</plain>
<libraries>
<library name="FH35C-41S-0.3SHW(50)">
<packages>
<package name="FH35C-41S-0.3SHW(50)">
</package>
</packages>
</library>
<library name="solderpad">
<packages>
<package name="SOLDERPAD">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-CAP">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="FH35C-41S-0.3SHW(50)" package="FH35C-41S-0.3SHW(50)" value="FH35C-41S-0.3SHW(50)"/>
<element name="U$2" library="solderpad" package="SOLDERPAD" value="SOLDERPAD"/>
<element name="U$3" library="solderpad" package="SOLDERPAD" value="SOLDERPAD"/>
<element name="U$4" library="solderpad" package="SOLDERPAD" value="SOLDERPAD"/>
<element name="U$5" library="solderpad" package="SOLDERPAD" value="SOLDERPAD"/>
<element name="U$6" library="solderpad" package="SOLDERPAD" value="SOLDERPAD"/>
<element name="U$7" library="solderpad" package="SOLDERPAD" value="SOLDERPAD"/>
<element name="U$8" library="solderpad" package="SOLDERPAD" value="SOLDERPAD"/>
<element name="U$9" library="solderpad" package="SOLDERPAD" value="SOLDERPAD"/>
<element name="U$10" library="solderpad" package="SOLDERPAD" value="SOLDERPAD"/>
<element name="U$11" library="solderpad" package="SOLDERPAD" value="SOLDERPAD"/>
<element name="U$12" library="solderpad" package="SOLDERPAD" value="SOLDERPAD"/>
<element name="U$13" library="solderpad" package="SOLDERPAD" value="SOLDERPAD"/>
<element name="U$14" library="solderpad" package="SOLDERPAD" value="SOLDERPAD"/>
<element name="U$15" library="solderpad" package="SOLDERPAD" value="SOLDERPAD"/>
<element name="U$16" library="solderpad" package="SOLDERPAD" value="SOLDERPAD"/>
<element name="U$17" library="solderpad" package="SOLDERPAD" value="SOLDERPAD"/>
<element name="U$18" library="solderpad" package="SOLDERPAD" value="SOLDERPAD"/>
<element name="U$19" library="solderpad" package="SOLDERPAD" value="SOLDERPAD"/>
<element name="C1" library="SparkFun-Capacitors" package="0603-CAP" value="10uF">
<attribute name="PROD_ID" value="CAP-11015"/>
</element>
</elements>
<signals>
<signal name="I2C2SCL">
<contactref element="U$1" pad="P$10"/>
<contactref element="U$3" pad="P$1"/>
</signal>
<signal name="I2C2SDA">
<contactref element="U$1" pad="P$11"/>
<contactref element="U$2" pad="P$1"/>
</signal>
<signal name="3.3V">
<contactref element="U$1" pad="P$37"/>
<contactref element="U$1" pad="P$38"/>
<contactref element="U$1" pad="P$39"/>
<contactref element="U$1" pad="P$40"/>
<contactref element="U$1" pad="P$41"/>
<contactref element="U$18" pad="P$1"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="DDI0_TX0_P">
<contactref element="U$1" pad="P$16"/>
<contactref element="U$4" pad="P$1"/>
</signal>
<signal name="DDI0_TX0_N">
<contactref element="U$1" pad="P$17"/>
<contactref element="U$5" pad="P$1"/>
</signal>
<signal name="DDI0_TX1_P">
<contactref element="U$1" pad="P$19"/>
<contactref element="U$6" pad="P$1"/>
</signal>
<signal name="DDI0_TX1_N">
<contactref element="U$1" pad="P$20"/>
<contactref element="U$7" pad="P$1"/>
</signal>
<signal name="DDI0_TX2_P">
<contactref element="U$1" pad="P$22"/>
<contactref element="U$8" pad="P$1"/>
</signal>
<signal name="DDI0_TX2_N">
<contactref element="U$1" pad="P$23"/>
<contactref element="U$9" pad="P$1"/>
</signal>
<signal name="DDI0_TX3_P">
<contactref element="U$1" pad="P$25"/>
<contactref element="U$10" pad="P$1"/>
</signal>
<signal name="DDI0_TX3_N">
<contactref element="U$1" pad="P$26"/>
<contactref element="U$11" pad="P$1"/>
</signal>
<signal name="DDI0_AUX_P">
<contactref element="U$1" pad="P$28"/>
<contactref element="U$12" pad="P$1"/>
</signal>
<signal name="DDI0_AUX_N">
<contactref element="U$1" pad="P$29"/>
<contactref element="U$13" pad="P$1"/>
</signal>
<signal name="DDI0_HPD_CONN">
<contactref element="U$1" pad="P$31"/>
<contactref element="U$14" pad="P$1"/>
</signal>
<signal name="DDI0_BCKLT_R_CTRL">
<contactref element="U$1" pad="P$32"/>
<contactref element="U$15" pad="P$1"/>
</signal>
<signal name="DDI0_VDD_EN">
<contactref element="U$1" pad="P$33"/>
<contactref element="U$16" pad="P$1"/>
</signal>
<signal name="DDI0_BCKL_EN">
<contactref element="U$1" pad="P$34"/>
<contactref element="U$17" pad="P$1"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="P$18"/>
<contactref element="U$1" pad="P$30"/>
<contactref element="U$1" pad="P$27"/>
<contactref element="U$1" pad="P$24"/>
<contactref element="U$1" pad="P$21"/>
<contactref element="U$19" pad="P$1"/>
<contactref element="C1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
