<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="15.367" y2="0" width="0" layer="20"/>
<wire x1="15.367" y1="0" x2="15.367" y2="29.972" width="0" layer="20"/>
<wire x1="15.367" y1="29.972" x2="0" y2="29.972" width="0" layer="20"/>
<wire x1="0" y1="29.972" x2="0" y2="0" width="0" layer="20"/>
<text>R2</text>
<text>R1</text>
<text>GI</text>
<text>^OUT</text>
<text>^IN</text>
<text>www.dkpinball.com</text>
<text>www.dkpinball.com</text>
<text>+</text>
<text>LED</text>
</plain>
<libraries>
<library name="relays">
<packages>
<package name="SOP04">
<description>&lt;b&gt;SOP 04 - 4.3x4.4mm RM 2.54mm&lt;/b&gt; AQY21, AQY22, AQY61 Series NAiS&lt;p&gt;Source: http://www.mew-europe.com/..  pti_en.pdf</description>
</package>
</packages>
</library>
<library name="led">
<packages>
<package name="FKIT-LED-1206">
</package>
</packages>
</library>
<library name="passives">
<packages>
<package name="1206">
</package>
</packages>
</library>
<library name="Mike_Rectifier">
<packages>
<package name="SOIC-4">
<description>&lt;b&gt;SOIC-4 Package&lt;/b&gt;&lt;p&gt;
Source: http://www.fairchildsemi.com/products/discrete/pdf/soic4_dim.pdf</description>
</package>
</packages>
</library>
<library name="con-molex">
<description>&lt;b&gt;Molex Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="22-23-2021">
<description>.100" (2.54mm) Center Headers - 2 Pin</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="EIA3216">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="K1" library="relays" package="SOP04" value="AQY21SOP">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
</element>
<element name="LED" library="led" package="FKIT-LED-1206" value="">
<attribute name="VALUE"/>
</element>
<element name="R1" library="passives" package="1206" value="200"/>
<element name="R2" library="passives" package="1206" value="200"/>
<element name="B1" library="Mike_Rectifier" package="SOIC-4" value="MB2S">
<attribute name="NAME"/>
</element>
<element name="X1" library="con-molex" package="22-23-2021" value="22-23-2021">
<attribute name="OC_NEWARK" value="25C3832"/>
<attribute name="MPN" value="22-23-2021"/>
<attribute name="MF" value="MOLEX"/>
<attribute name="OC_FARNELL" value="1462926"/>
</element>
<element name="OUT" library="con-molex" package="22-23-2021" value="22-23-2021">
<attribute name="OC_NEWARK" value="25C3832"/>
<attribute name="MPN" value="22-23-2021"/>
<attribute name="MF" value="MOLEX"/>
<attribute name="OC_FARNELL" value="1462926"/>
</element>
<element name="IN" library="con-molex" package="22-23-2021" value="22-23-2021">
<attribute name="OC_NEWARK" value="25C3832"/>
<attribute name="MPN" value="22-23-2021"/>
<attribute name="MF" value="MOLEX"/>
<attribute name="OC_FARNELL" value="1462926"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="EIA3216" value="10uF">
<attribute name="PROD_ID" value="CAP-00811"/>
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="DC-">
<contactref element="B1" pad="-"/>
<contactref element="R1" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="C1" pad="C"/>
</signal>
<signal name="N$1">
<contactref element="B1" pad="~1"/>
<contactref element="X1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="B1" pad="~2"/>
<contactref element="X1" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="B1" pad="+"/>
<contactref element="LED" pad="A"/>
<contactref element="K1" pad="1"/>
<contactref element="C1" pad="A"/>
</signal>
<signal name="N$4">
<contactref element="K1" pad="2"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="LED" pad="C"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="K1" pad="3"/>
<contactref element="OUT" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="K1" pad="4"/>
<contactref element="IN" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="IN" pad="2"/>
<contactref element="OUT" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
