<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.4.0">
<drawing>
<board>
<plain>
<circle x="25" y="25" radius="25" width="0.4064" layer="20"/>
</plain>
<libraries>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-CAP">
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-0603">
</package>
</packages>
</library>
<library name="efm8SB">
<packages>
<package name="EFM8SB2">
<description>&lt;b&gt;EFM8SB2&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 44&lt;/i&gt;&lt;br&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-RES">
</package>
</packages>
</library>
<library name="prog_conn">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X03_LOCK">
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="BATTCON_20MM_4LEGS">
</package>
</packages>
</library>
<library name="SparkFun-FreqCtrl">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find crystals and oscillators and other things that go "tick".&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CRYSTAL-32KHZ-SMD_EPSON_MC146">
</package>
</packages>
</library>
<library name="SparkFun-Retired">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of retired footprints for resistors, capacitors, board names, ICs, etc., that are no longer used in our catalog.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt;Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE-SWITCH-SMD">
</package>
</packages>
</library>
</libraries>
<attributes>
<attribute name="CIRCULAR-LAYOUT-SETTINGS" value="0.984252 0.984252 0.767717 180.000000 0 1"/>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun-Passives" package="0603-CAP" value=""/>
<element name="C2" library="SparkFun-Passives" package="0603-CAP" value=""/>
<element name="D2" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="D3" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="D4" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="D5" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="D6" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="IC1" library="efm8SB" package="EFM8SB2" value="EFM8SB2"/>
<element name="R1" library="SparkFun-Resistors" package="0603-RES" value=""/>
<element name="R2" library="SparkFun-Resistors" package="0603-RES" value=""/>
<element name="R3" library="SparkFun-Resistors" package="0603-RES" value=""/>
<element name="R4" library="SparkFun-Resistors" package="0603-RES" value=""/>
<element name="R5" library="SparkFun-Resistors" package="0603-RES" value=""/>
<element name="R6" library="SparkFun-Resistors" package="0603-RES" value=""/>
<element name="JP1" library="prog_conn" package="1X03_LOCK" value=""/>
<element name="BAT1" library="SparkFun-Electromechanical" package="BATTCON_20MM_4LEGS" value="20mm coincell">
<attribute name="VALUE" value="20mm coincell"/>
<attribute name="PROD_ID" value="BATT-10373"/>
</element>
<element name="D1" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="D7" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="D8" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="D9" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="D10" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="D11" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="D12" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="D13" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="D14" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="D15" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="D16" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="D17" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="D18" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="D19" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="D20" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="D21" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="D22" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="D23" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="D24" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="D25" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="D26" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="D27" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="D28" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="D29" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="D30" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="D31" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="D32" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="D33" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="D34" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="D35" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="D36" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="D37" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="D38" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="D39" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="D40" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="D41" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="D42" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="D43" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="D44" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="D45" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="D46" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="D47" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="D48" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="D49" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="D50" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="D51" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="D52" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="D53" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="D54" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="D55" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="D56" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="D57" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="D58" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="D59" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="D60" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="D61" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="D62" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="D63" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="D64" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="D65" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="D66" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="D67" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="D68" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="D69" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="D70" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="D71" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="D72" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="Y1" library="SparkFun-FreqCtrl" package="CRYSTAL-32KHZ-SMD_EPSON_MC146" value=""/>
<element name="S1" library="SparkFun-Retired" package="TACTILE-SWITCH-SMD" value="TAC_SWITCHSMD">
<attribute name="PROD_ID" value="SWCH-08247"/>
</element>
<element name="S2" library="SparkFun-Retired" package="TACTILE-SWITCH-SMD" value="TAC_SWITCHSMD">
<attribute name="PROD_ID" value="SWCH-08247"/>
</element>
<element name="R7" library="SparkFun-Resistors" package="0603-RES" value=""/>
<element name="R8" library="SparkFun-Resistors" package="0603-RES" value=""/>
<element name="R9" library="SparkFun-Resistors" package="0603-RES" value=""/>
<element name="R10" library="SparkFun-Resistors" package="0603-RES" value=""/>
<element name="D73" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="D74" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="R11" library="SparkFun-Resistors" package="0603-RES" value=""/>
<element name="R12" library="SparkFun-Resistors" package="0603-RES" value=""/>
</elements>
<signals>
<signal name="SM1">
<contactref element="D2" pad="C"/>
<contactref element="R1" pad="2"/>
<contactref element="D7" pad="C"/>
<contactref element="D12" pad="C"/>
<contactref element="D17" pad="C"/>
<contactref element="D22" pad="C"/>
<contactref element="D27" pad="C"/>
<contactref element="D32" pad="C"/>
<contactref element="D37" pad="C"/>
<contactref element="D42" pad="C"/>
<contactref element="D47" pad="C"/>
<contactref element="D52" pad="C"/>
<contactref element="D57" pad="C"/>
</signal>
<signal name="H">
<contactref element="R6" pad="2"/>
<contactref element="D61" pad="C"/>
<contactref element="D62" pad="C"/>
<contactref element="D63" pad="C"/>
<contactref element="D64" pad="C"/>
<contactref element="D65" pad="C"/>
<contactref element="D66" pad="C"/>
<contactref element="D67" pad="C"/>
<contactref element="D68" pad="C"/>
<contactref element="D69" pad="C"/>
<contactref element="D70" pad="C"/>
<contactref element="D71" pad="C"/>
<contactref element="D72" pad="C"/>
</signal>
<signal name="SM2">
<contactref element="D3" pad="C"/>
<contactref element="R2" pad="2"/>
<contactref element="D8" pad="C"/>
<contactref element="D13" pad="C"/>
<contactref element="D18" pad="C"/>
<contactref element="D23" pad="C"/>
<contactref element="D28" pad="C"/>
<contactref element="D33" pad="C"/>
<contactref element="D38" pad="C"/>
<contactref element="D43" pad="C"/>
<contactref element="D48" pad="C"/>
<contactref element="D53" pad="C"/>
<contactref element="D58" pad="C"/>
</signal>
<signal name="HS1">
<contactref element="D2" pad="A"/>
<contactref element="D3" pad="A"/>
<contactref element="D4" pad="A"/>
<contactref element="D5" pad="A"/>
<contactref element="D6" pad="A"/>
<contactref element="D62" pad="A"/>
<contactref element="IC1" pad="21"/>
</signal>
<signal name="SM3">
<contactref element="D4" pad="C"/>
<contactref element="R3" pad="2"/>
<contactref element="D9" pad="C"/>
<contactref element="D14" pad="C"/>
<contactref element="D19" pad="C"/>
<contactref element="D24" pad="C"/>
<contactref element="D29" pad="C"/>
<contactref element="D34" pad="C"/>
<contactref element="D39" pad="C"/>
<contactref element="D44" pad="C"/>
<contactref element="D49" pad="C"/>
<contactref element="D54" pad="C"/>
<contactref element="D59" pad="C"/>
</signal>
<signal name="SM4">
<contactref element="D5" pad="C"/>
<contactref element="R4" pad="2"/>
<contactref element="D10" pad="C"/>
<contactref element="D15" pad="C"/>
<contactref element="D20" pad="C"/>
<contactref element="D25" pad="C"/>
<contactref element="D30" pad="C"/>
<contactref element="D35" pad="C"/>
<contactref element="D40" pad="C"/>
<contactref element="D45" pad="C"/>
<contactref element="D50" pad="C"/>
<contactref element="D55" pad="C"/>
<contactref element="D60" pad="C"/>
</signal>
<signal name="SM5">
<contactref element="D6" pad="C"/>
<contactref element="R5" pad="2"/>
<contactref element="D1" pad="C"/>
<contactref element="D11" pad="C"/>
<contactref element="D16" pad="C"/>
<contactref element="D21" pad="C"/>
<contactref element="D26" pad="C"/>
<contactref element="D31" pad="C"/>
<contactref element="D36" pad="C"/>
<contactref element="D41" pad="C"/>
<contactref element="D46" pad="C"/>
<contactref element="D51" pad="C"/>
<contactref element="D56" pad="C"/>
</signal>
<signal name="GND">
<contactref element="IC1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="BAT1" pad="2"/>
<contactref element="JP1" pad="3"/>
<contactref element="R8" pad="2"/>
<contactref element="R10" pad="2"/>
<contactref element="R11" pad="1"/>
<contactref element="R12" pad="1"/>
</signal>
<signal name="VDD">
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="IC1" pad="3"/>
<contactref element="BAT1" pad="1"/>
<contactref element="S1" pad="1"/>
<contactref element="S1" pad="2"/>
<contactref element="S2" pad="1"/>
<contactref element="S2" pad="2"/>
</signal>
<signal name="C2D">
<contactref element="IC1" pad="7"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="C2CK">
<contactref element="IC1" pad="6"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="DRV_SM1">
<contactref element="R1" pad="1"/>
<contactref element="IC1" pad="15"/>
</signal>
<signal name="DRV_SM2">
<contactref element="R2" pad="1"/>
<contactref element="IC1" pad="14"/>
</signal>
<signal name="DRV_SM3">
<contactref element="R3" pad="1"/>
<contactref element="IC1" pad="13"/>
</signal>
<signal name="DRV_SM4">
<contactref element="R4" pad="1"/>
<contactref element="IC1" pad="12"/>
</signal>
<signal name="DRV_SM5">
<contactref element="R5" pad="1"/>
<contactref element="IC1" pad="11"/>
</signal>
<signal name="DRV_H">
<contactref element="R6" pad="1"/>
<contactref element="IC1" pad="16"/>
</signal>
<signal name="HS2">
<contactref element="D7" pad="A"/>
<contactref element="D8" pad="A"/>
<contactref element="D9" pad="A"/>
<contactref element="D10" pad="A"/>
<contactref element="D11" pad="A"/>
<contactref element="D63" pad="A"/>
<contactref element="IC1" pad="20"/>
</signal>
<signal name="HS3">
<contactref element="D12" pad="A"/>
<contactref element="D13" pad="A"/>
<contactref element="D14" pad="A"/>
<contactref element="D15" pad="A"/>
<contactref element="D16" pad="A"/>
<contactref element="D64" pad="A"/>
<contactref element="IC1" pad="19"/>
</signal>
<signal name="HS4">
<contactref element="D17" pad="A"/>
<contactref element="D18" pad="A"/>
<contactref element="D19" pad="A"/>
<contactref element="D20" pad="A"/>
<contactref element="D21" pad="A"/>
<contactref element="D65" pad="A"/>
<contactref element="IC1" pad="18"/>
</signal>
<signal name="HS5">
<contactref element="D22" pad="A"/>
<contactref element="D23" pad="A"/>
<contactref element="D24" pad="A"/>
<contactref element="D25" pad="A"/>
<contactref element="D26" pad="A"/>
<contactref element="D66" pad="A"/>
<contactref element="IC1" pad="17"/>
</signal>
<signal name="HS6">
<contactref element="D27" pad="A"/>
<contactref element="D28" pad="A"/>
<contactref element="D29" pad="A"/>
<contactref element="D30" pad="A"/>
<contactref element="D31" pad="A"/>
<contactref element="D67" pad="A"/>
<contactref element="IC1" pad="8"/>
</signal>
<signal name="HS7">
<contactref element="D32" pad="A"/>
<contactref element="D33" pad="A"/>
<contactref element="D34" pad="A"/>
<contactref element="D35" pad="A"/>
<contactref element="D36" pad="A"/>
<contactref element="D68" pad="A"/>
<contactref element="IC1" pad="32"/>
</signal>
<signal name="HS8">
<contactref element="D37" pad="A"/>
<contactref element="D38" pad="A"/>
<contactref element="D39" pad="A"/>
<contactref element="D40" pad="A"/>
<contactref element="D41" pad="A"/>
<contactref element="D69" pad="A"/>
<contactref element="IC1" pad="31"/>
</signal>
<signal name="HS9">
<contactref element="D42" pad="A"/>
<contactref element="D43" pad="A"/>
<contactref element="D44" pad="A"/>
<contactref element="D45" pad="A"/>
<contactref element="D46" pad="A"/>
<contactref element="D70" pad="A"/>
<contactref element="IC1" pad="30"/>
</signal>
<signal name="HS10">
<contactref element="D47" pad="A"/>
<contactref element="D48" pad="A"/>
<contactref element="D49" pad="A"/>
<contactref element="D50" pad="A"/>
<contactref element="D51" pad="A"/>
<contactref element="D71" pad="A"/>
<contactref element="IC1" pad="29"/>
</signal>
<signal name="HS11">
<contactref element="D52" pad="A"/>
<contactref element="D53" pad="A"/>
<contactref element="D54" pad="A"/>
<contactref element="D55" pad="A"/>
<contactref element="D56" pad="A"/>
<contactref element="D72" pad="A"/>
<contactref element="IC1" pad="28"/>
</signal>
<signal name="HS12">
<contactref element="D1" pad="A"/>
<contactref element="D57" pad="A"/>
<contactref element="D58" pad="A"/>
<contactref element="D59" pad="A"/>
<contactref element="D60" pad="A"/>
<contactref element="D61" pad="A"/>
<contactref element="IC1" pad="27"/>
</signal>
<signal name="XTAL4">
<contactref element="Y1" pad="P$1"/>
<contactref element="IC1" pad="9"/>
</signal>
<signal name="XTAL3">
<contactref element="IC1" pad="10"/>
<contactref element="Y1" pad="P$2"/>
</signal>
<signal name="BTN2">
<contactref element="IC1" pad="26"/>
<contactref element="R9" pad="2"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="BTN1">
<contactref element="IC1" pad="25"/>
<contactref element="R7" pad="2"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="S1" pad="4"/>
<contactref element="S1" pad="3"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="S2" pad="4"/>
<contactref element="S2" pad="3"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="D73" pad="C"/>
<contactref element="R11" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="D74" pad="C"/>
<contactref element="R12" pad="2"/>
</signal>
<signal name="AMPM">
<contactref element="D73" pad="A"/>
<contactref element="IC1" pad="24"/>
</signal>
<signal name="SEC">
<contactref element="D74" pad="A"/>
<contactref element="IC1" pad="23"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
