<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="0.635" y1="0.254" x2="18.415" y2="0.254" width="0.2032" layer="20"/>
<wire x1="18.415" y1="17.78" x2="0.635" y2="17.78" width="0.2032" layer="20"/>
<wire x1="0.635" y1="17.78" x2="0.635" y2="0.254" width="0.2032" layer="20"/>
<text>GND</text>
<text>RST</text>
<text>VCC</text>
<text>MISO</text>
<text>MOSI</text>
<text>SCK</text>
<text>AVR ICSP V1.0</text>
<wire x1="18.415" y1="17.78" x2="18.415" y2="0.254" width="0.2032" layer="20"/>
<text>GND</text>
<text>VCC</text>
<text>VCC</text>
<text>GND</text>
<text>AVR ICSP V1.0</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X3_POGO">
</package>
<package name="2X3-NS">
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="STAND-OFF">
<description>&lt;b&gt;Stand Off&lt;/b&gt;&lt;p&gt;
This is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components. SKU : PRT-00447</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="SparkFun-Connectors" package="2X3_POGO" value="">
<attribute name="PROD_ID" value="HW-11044"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="2X3-NS" value="AVR_SPI_PRG_6NS"/>
<element name="JP2" library="SparkFun-Electromechanical" package="STAND-OFF" value="STAND-OFF"/>
<element name="JP3" library="SparkFun-Electromechanical" package="STAND-OFF" value="STAND-OFF"/>
</elements>
<signals>
<signal name="MISO">
<contactref element="J1" pad="P$1"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="SCK">
<contactref element="J1" pad="P$3"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="RESET">
<contactref element="J1" pad="P$5"/>
<contactref element="J2" pad="5"/>
</signal>
<signal name="+5">
<contactref element="J1" pad="P$2"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="MOSI">
<contactref element="J1" pad="P$4"/>
<contactref element="J2" pad="4"/>
</signal>
<signal name="GND">
<contactref element="J1" pad="P$6"/>
<contactref element="J2" pad="6"/>
</signal>
<signal name="N$1">
</signal>
<signal name="N$2">
</signal>
</signals>
</board>
</drawing>
</eagle>
