<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="41.275" y1="11.43" x2="24.765" y2="11.43" width="0" layer="20"/>
<wire x1="24.765" y1="11.43" x2="24.13" y2="12.065" width="0" layer="20" curve="-90"/>
<wire x1="24.13" y1="12.065" x2="24.13" y2="26.035" width="0" layer="20"/>
<wire x1="24.13" y1="26.035" x2="24.765" y2="26.67" width="0" layer="20" curve="-90"/>
<wire x1="24.765" y1="26.67" x2="41.275" y2="26.67" width="0" layer="20"/>
<wire x1="41.275" y1="26.67" x2="41.91" y2="26.035" width="0" layer="20" curve="-90"/>
<wire x1="41.91" y1="26.035" x2="41.91" y2="12.065" width="0" layer="20"/>
<wire x1="41.91" y1="12.065" x2="41.275" y2="11.43" width="0" layer="20" curve="-90"/>
<text>V</text>
<text>V</text>
<text>G</text>
<text>G</text>
<text>30Sep17</text>
<text>V 1</text>
<text>USB</text>
<text>USB</text>
<text>D+</text>
<text>D-</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X06_NO_SILK">
</package>
</packages>
</library>
<library name="Wurth">
<packages>
<package name="629105136821">
<description>micro USB receptacle&lt;br&gt;
horizontal SMT&lt;br&gt;
http://katalog.we-online.de/em/datasheet/629105136821.pdf&lt;br&gt;
75% cream coverage</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="SparkFun-Connectors" package="1X06_NO_SILK" value="">
<attribute name="PROD_ID" value="CONN-08437"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X06_NO_SILK" value="">
<attribute name="PROD_ID" value="CONN-08437"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="Wurth" package="629105136821" value="USB"/>
</elements>
<signals>
<signal name="PWR">
<contactref element="J1" pad="5"/>
<contactref element="J2" pad="5"/>
<contactref element="J1" pad="6"/>
<contactref element="J2" pad="6"/>
<contactref element="J3" pad="1"/>
</signal>
<signal name="GND">
<contactref element="J1" pad="1"/>
<contactref element="J2" pad="1"/>
<contactref element="J1" pad="2"/>
<contactref element="J3" pad="5"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="D+">
<contactref element="J3" pad="3"/>
<contactref element="J1" pad="4"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="D-">
<contactref element="J3" pad="2"/>
<contactref element="J2" pad="3"/>
<contactref element="J2" pad="4"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
