<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.3.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="27.864" y2="0" width="0" layer="20"/>
<wire x1="27.864" y1="0" x2="27.864" y2="29.708" width="0" layer="20"/>
<wire x1="27.864" y1="29.708" x2="0" y2="29.708" width="0" layer="20"/>
<wire x1="0" y1="29.708" x2="0" y2="0" width="0" layer="20"/>
<text>PedalTile</text>
<text>PedalTile v0.1</text>
<text>Daniel Garcia
ЯDaneel /  dgarcia@dgarcia.net</text>
<text>G</text>
<text>+</text>
<text>-</text>
</plain>
<libraries>
<library name="thonkiconn">
<packages>
<package name="WQP-PJ301M-12_JACK">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X03">
<description>&lt;h3&gt;Plated Through Hole - 3 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="GATE1" library="thonkiconn" package="WQP-PJ301M-12_JACK" value="WQP-PJ301M-12_JACK">
<attribute name="NAME"/>
</element>
<element name="GATE2" library="thonkiconn" package="WQP-PJ301M-12_JACK" value="WQP-PJ301M-12_JACK">
<attribute name="NAME"/>
</element>
<element name="PEDAL1" library="thonkiconn" package="WQP-PJ301M-12_JACK" value="WQP-PJ301M-12_JACK">
<attribute name="NAME"/>
</element>
<element name="PEDAL2" library="thonkiconn" package="WQP-PJ301M-12_JACK" value="WQP-PJ301M-12_JACK">
<attribute name="NAME"/>
</element>
<element name="POWER" library="SparkFun-Connectors" package="1X03" value="P1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="GATE2" pad="P$3"/>
<contactref element="GATE1" pad="P$3"/>
<contactref element="POWER" pad="1"/>
</signal>
<signal name="+12V">
<contactref element="POWER" pad="2"/>
<contactref element="PEDAL1" pad="P$3"/>
<contactref element="PEDAL2" pad="P$3"/>
<contactref element="PEDAL1" pad="P$2"/>
<contactref element="PEDAL2" pad="P$2"/>
</signal>
<signal name="N$1">
<contactref element="PEDAL2" pad="P$1"/>
<contactref element="GATE2" pad="P$1"/>
</signal>
<signal name="N$2">
<contactref element="PEDAL1" pad="P$1"/>
<contactref element="GATE1" pad="P$1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
