<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.4.0">
<drawing>
<board>
<plain>
<wire x1="10.16" y1="0" x2="10.16" y2="10.16" width="0" layer="20"/>
<wire x1="10.16" y1="10.16" x2="0" y2="10.16" width="0" layer="20"/>
<wire x1="0" y1="10.16" x2="0" y2="53.34" width="0" layer="20"/>
<wire x1="0" y1="53.34" x2="10.16" y2="53.34" width="0" layer="20"/>
<wire x1="10.16" y1="53.34" x2="10.16" y2="63.5" width="0" layer="20"/>
<wire x1="10.16" y1="63.5" x2="97.79" y2="63.5" width="0" layer="20"/>
<wire x1="97.79" y1="63.5" x2="97.79" y2="53.34" width="0" layer="20"/>
<wire x1="97.79" y1="53.34" x2="107.95" y2="53.34" width="0" layer="20"/>
<wire x1="107.95" y1="53.34" x2="107.95" y2="10.16" width="0" layer="20"/>
<wire x1="107.95" y1="10.16" x2="97.79" y2="10.16" width="0" layer="20"/>
<wire x1="97.79" y1="10.16" x2="97.79" y2="0" width="0" layer="20"/>
<wire x1="97.79" y1="0" x2="10.16" y2="0" width="0" layer="20"/>
<hole x="16.51" y="6.985" drill="3.2"/>
<hole x="16.51" y="55.88" drill="3.2"/>
<hole x="91.44" y="55.88" drill="3.2"/>
<hole x="91.44" y="6.985" drill="3.2"/>
<hole x="78.74" y="36.83" drill="6.35"/>
<text>Benjamin Koch
AccuTrigger
REV-C</text>
<text>SUP800 GPS</text>
</plain>
<libraries>
<library name="SparkFun-PowerIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find drivers, regulators, and amplifiers.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TO-220-ALT">
</package>
</packages>
</library>
<library name="Ben_relay1">
<packages>
<package name="BENS_SS_RELAY">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X16">
</package>
<package name="MICRO-SD-SOCKET-PP">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.3">
</package>
</packages>
</library>
<library name="RJ45_VERT">
<packages>
<package name="RJ45">
</package>
</packages>
</library>
<library name="SparkFun-Retired">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of retired footprints for resistors, capacitors, board names, ICs, etc., that are no longer used in our catalog.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt;Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE-PTH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="Teensy_3_Series_Board_v1.0">
<packages>
<package name="TEENSY_3.1+4">
</package>
</packages>
</library>
<library name="SUP800F">
<packages>
<package name="SUP800F">
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED5MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
5 mm, round</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="5V_REG" library="SparkFun-PowerIC" package="TO-220-ALT" value="">
<attribute name="SF_ID" value="COM-00107"/>
<attribute name="PROD_ID" value="VREG-08450"/>
</element>
<element name="CAMERA1" library="Ben_relay1" package="BENS_SS_RELAY" value="CPC1218"/>
<element name="CAMERA2" library="Ben_relay1" package="BENS_SS_RELAY" value="CPC1218"/>
<element name="LCD" library="SparkFun-Connectors" package="1X16" value=""/>
<element name="LED1" library="SparkFun-LED" package="LED5MM" value=""/>
<element name="R1" library="SparkFun-Passives" package="AXIAL-0.3" value=""/>
<element name="RJ45" library="RJ45_VERT" package="RJ45" value="RJ45_VERTICAL_DIGI"/>
<element name="S1" library="SparkFun-Retired" package="TACTILE-PTH" value=""/>
<element name="S2" library="SparkFun-Retired" package="TACTILE-PTH" value=""/>
<element name="S3" library="SparkFun-Retired" package="TACTILE-PTH" value=""/>
<element name="S4" library="SparkFun-Retired" package="TACTILE-PTH" value=""/>
<element name="TEENSY_3.1" library="Teensy_3_Series_Board_v1.0" package="TEENSY_3.1+4" value="TEENSY_3.1+4"/>
<element name="U$1" library="SUP800F" package="SUP800F" value="SUP800F_GPS"/>
<element name="U1" library="SparkFun-Connectors" package="MICRO-SD-SOCKET-PP" value="USD-SOCKETNEW">
<attribute name="PROD_ID" value="CONN-07820"/>
</element>
</elements>
<signals>
<signal name="AGND">
<contactref element="TEENSY_3.1" pad="AGND"/>
</signal>
<signal name="VBAT">
<contactref element="TEENSY_3.1" pad="VBAT"/>
</signal>
<signal name="AREF">
<contactref element="TEENSY_3.1" pad="A14"/>
</signal>
<signal name="VUSB">
<contactref element="TEENSY_3.1" pad="VUSB"/>
</signal>
<signal name="LCD1">
<contactref element="LCD" pad="4"/>
<contactref element="TEENSY_3.1" pad="23/A9"/>
</signal>
<signal name="LCD2">
<contactref element="LCD" pad="5"/>
<contactref element="TEENSY_3.1" pad="22/A8"/>
</signal>
<signal name="LCD3">
<contactref element="LCD" pad="6"/>
<contactref element="TEENSY_3.1" pad="21/A7"/>
</signal>
<signal name="LCD7">
<contactref element="LCD" pad="14"/>
<contactref element="TEENSY_3.1" pad="17/A3"/>
</signal>
<signal name="LCD6">
<contactref element="LCD" pad="13"/>
<contactref element="TEENSY_3.1" pad="18/A4"/>
</signal>
<signal name="LCD5">
<contactref element="LCD" pad="12"/>
<contactref element="TEENSY_3.1" pad="19/A5"/>
</signal>
<signal name="LCD4">
<contactref element="LCD" pad="11"/>
<contactref element="TEENSY_3.1" pad="20/A6"/>
</signal>
<signal name="5V">
<contactref element="5V_REG" pad="OUT"/>
<contactref element="TEENSY_3.1" pad="VIN"/>
</signal>
<signal name="GND">
<contactref element="LCD" pad="1"/>
<contactref element="5V_REG" pad="GND"/>
<contactref element="U1" pad="GND3"/>
<contactref element="U1" pad="GND1"/>
<contactref element="U1" pad="CD2"/>
<contactref element="U1" pad="6"/>
<contactref element="TEENSY_3.1" pad="GND"/>
<contactref element="TEENSY_3.1" pad="GND1"/>
<contactref element="U$1" pad="GND"/>
<contactref element="U$1" pad="P$1"/>
<contactref element="U$1" pad="P$2"/>
<contactref element="LED1" pad="K"/>
<contactref element="S4" pad="3"/>
<contactref element="S4" pad="4"/>
<contactref element="S3" pad="3"/>
<contactref element="S3" pad="4"/>
<contactref element="S2" pad="3"/>
<contactref element="S2" pad="4"/>
<contactref element="S1" pad="3"/>
<contactref element="S1" pad="4"/>
<contactref element="RJ45" pad="GND1"/>
<contactref element="RJ45" pad="GND2"/>
<contactref element="RJ45" pad="2"/>
<contactref element="CAMERA2" pad="GND"/>
<contactref element="CAMERA1" pad="GND"/>
<contactref element="CAMERA1" pad="CONN1"/>
</signal>
<signal name="12V">
<contactref element="5V_REG" pad="IN"/>
<contactref element="RJ45" pad="1"/>
</signal>
<signal name="CS">
<contactref element="U1" pad="2"/>
<contactref element="TEENSY_3.1" pad="15/A1"/>
</signal>
<signal name="MOSI">
<contactref element="U1" pad="3"/>
<contactref element="TEENSY_3.1" pad="11"/>
</signal>
<signal name="SCK">
<contactref element="U1" pad="5"/>
<contactref element="TEENSY_3.1" pad="13"/>
</signal>
<signal name="MISO">
<contactref element="U1" pad="7"/>
<contactref element="TEENSY_3.1" pad="12"/>
</signal>
<signal name="3.3V">
<contactref element="U1" pad="4"/>
<contactref element="TEENSY_3.1" pad="3.3V"/>
<contactref element="TEENSY_3.1" pad="3.3V1"/>
<contactref element="U$1" pad="VIN"/>
<contactref element="U$1" pad="VBAT"/>
<contactref element="LCD" pad="2"/>
</signal>
<signal name="GPS_RX">
<contactref element="TEENSY_3.1" pad="8"/>
<contactref element="U$1" pad="RX"/>
<contactref element="RJ45" pad="8"/>
</signal>
<signal name="GPS_TX">
<contactref element="TEENSY_3.1" pad="7"/>
<contactref element="U$1" pad="TX"/>
<contactref element="RJ45" pad="7"/>
</signal>
<signal name="SW1">
<contactref element="S1" pad="1"/>
<contactref element="S1" pad="2"/>
<contactref element="TEENSY_3.1" pad="2"/>
</signal>
<signal name="SW2">
<contactref element="S2" pad="1"/>
<contactref element="S2" pad="2"/>
<contactref element="TEENSY_3.1" pad="3"/>
</signal>
<signal name="SW3">
<contactref element="S3" pad="1"/>
<contactref element="S3" pad="2"/>
<contactref element="TEENSY_3.1" pad="4"/>
</signal>
<signal name="SW4">
<contactref element="S4" pad="1"/>
<contactref element="S4" pad="2"/>
<contactref element="TEENSY_3.1" pad="5"/>
</signal>
<signal name="N$9">
<contactref element="R1" pad="P$2"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="LED">
<contactref element="R1" pad="P$1"/>
<contactref element="TEENSY_3.1" pad="6"/>
</signal>
<signal name="N$1">
<contactref element="TEENSY_3.1" pad="A10"/>
</signal>
<signal name="N$2">
<contactref element="TEENSY_3.1" pad="AREF"/>
</signal>
<signal name="CAM1SNS">
<contactref element="RJ45" pad="3"/>
<contactref element="CAMERA1" pad="CONN2"/>
<contactref element="TEENSY_3.1" pad="14/A0"/>
</signal>
<signal name="CAM2SNS">
<contactref element="RJ45" pad="5"/>
<contactref element="CAMERA2" pad="CONN2"/>
</signal>
<signal name="CAM2GND">
<contactref element="RJ45" pad="4"/>
<contactref element="CAMERA2" pad="CONN1"/>
</signal>
<signal name="YOKE_SWITCH">
<contactref element="RJ45" pad="6"/>
<contactref element="TEENSY_3.1" pad="16/A2"/>
</signal>
<signal name="CAMERA_RELAY">
<contactref element="CAMERA2" pad="VIN"/>
<contactref element="CAMERA1" pad="VIN"/>
<contactref element="TEENSY_3.1" pad="9"/>
</signal>
<signal name="N$6">
<contactref element="TEENSY_3.1" pad="A11"/>
</signal>
<signal name="N$7">
<contactref element="TEENSY_3.1" pad="10"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
