<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="68.25" y2="0" width="0" layer="20"/>
<wire x1="68.25" y1="0" x2="68.25" y2="33.01" width="0" layer="20"/>
<wire x1="68.25" y1="33.01" x2="0" y2="33.01" width="0" layer="20"/>
<wire x1="0" y1="33.01" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SCREWTERMINAL-3.5MM-2">
</package>
<package name="1X08_ROUND">
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TO-92">
<description>&lt;b&gt;TO 92&lt;/b&gt;</description>
</package>
<package name="TO220V">
<description>&lt;b&gt;TO 220 Vertical&lt;/b&gt; Package works with various parts including N-Channel MOSFET SparkFun SKU: COM-10213</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.3">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-2" value="">
<attribute name="PROD_ID" value="CONN-08399"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-2" value="">
<attribute name="PROD_ID" value="CONN-08399"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-2" value="">
<attribute name="PROD_ID" value="CONN-08399"/>
</element>
<element name="J4" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-2" value="">
<attribute name="PROD_ID" value="CONN-08399"/>
</element>
<element name="J5" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-2" value="">
<attribute name="PROD_ID" value="CONN-08399"/>
</element>
<element name="J6" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-2" value="">
<attribute name="PROD_ID" value="CONN-08399"/>
</element>
<element name="J8" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-2" value="">
<attribute name="PROD_ID" value="CONN-08399"/>
</element>
<element name="Q1" library="SparkFun-DiscreteSemi" package="TO-92" value="MOSFET-NCHANNEL2N7000"/>
<element name="Q10" library="SparkFun-DiscreteSemi" package="TO220V" value="MOSFET-NCHANNELFQP30N06L">
<attribute name="PROD_ID" value="TRANS-10060"/>
<attribute name="NAME"/>
</element>
<element name="Q11" library="SparkFun-DiscreteSemi" package="TO-92" value="MOSFET-NCHANNEL2N7000"/>
<element name="Q12" library="SparkFun-DiscreteSemi" package="TO220V" value="MOSFET-NCHANNELFQP30N06L">
<attribute name="PROD_ID" value="TRANS-10060"/>
<attribute name="NAME"/>
</element>
<element name="Q2" library="SparkFun-DiscreteSemi" package="TO220V" value="MOSFET-NCHANNELFQP30N06L">
<attribute name="PROD_ID" value="TRANS-10060"/>
<attribute name="NAME"/>
</element>
<element name="Q3" library="SparkFun-DiscreteSemi" package="TO-92" value="MOSFET-NCHANNEL2N7000"/>
<element name="Q4" library="SparkFun-DiscreteSemi" package="TO220V" value="MOSFET-NCHANNELFQP30N06L">
<attribute name="PROD_ID" value="TRANS-10060"/>
<attribute name="NAME"/>
</element>
<element name="Q5" library="SparkFun-DiscreteSemi" package="TO-92" value="MOSFET-NCHANNEL2N7000"/>
<element name="Q6" library="SparkFun-DiscreteSemi" package="TO220V" value="MOSFET-NCHANNELFQP30N06L">
<attribute name="PROD_ID" value="TRANS-10060"/>
<attribute name="NAME"/>
</element>
<element name="Q7" library="SparkFun-DiscreteSemi" package="TO-92" value="MOSFET-NCHANNEL2N7000"/>
<element name="Q8" library="SparkFun-DiscreteSemi" package="TO220V" value="MOSFET-NCHANNELFQP30N06L">
<attribute name="PROD_ID" value="TRANS-10060"/>
<attribute name="NAME"/>
</element>
<element name="Q9" library="SparkFun-DiscreteSemi" package="TO-92" value="MOSFET-NCHANNEL2N7000"/>
<element name="R1" library="SparkFun-Resistors" package="AXIAL-0.3" value="1K">
<attribute name="PROD_ID" value="RES-12182"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="AXIAL-0.3" value="1K">
<attribute name="PROD_ID" value="RES-12182"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="AXIAL-0.3" value="1K">
<attribute name="PROD_ID" value="RES-12182"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="AXIAL-0.3" value="1K">
<attribute name="PROD_ID" value="RES-12182"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="AXIAL-0.3" value="1K">
<attribute name="PROD_ID" value="RES-12182"/>
</element>
<element name="R6" library="SparkFun-Resistors" package="AXIAL-0.3" value="1K">
<attribute name="PROD_ID" value="RES-12182"/>
</element>
<element name="J7" library="SparkFun-Connectors" package="1X08_ROUND" value="">
<attribute name="PROD_ID" value="CONN-08437"/>
</element>
</elements>
<signals>
<signal name="12V">
<contactref element="J1" pad="1"/>
<contactref element="R1" pad="P$2"/>
<contactref element="J2" pad="1"/>
<contactref element="R2" pad="P$2"/>
<contactref element="J3" pad="1"/>
<contactref element="R3" pad="P$2"/>
<contactref element="J4" pad="1"/>
<contactref element="R4" pad="P$2"/>
<contactref element="J5" pad="1"/>
<contactref element="R5" pad="P$2"/>
<contactref element="J6" pad="1"/>
<contactref element="R6" pad="P$2"/>
<contactref element="J8" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="J1" pad="2"/>
<contactref element="Q2" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="Q2" pad="1"/>
<contactref element="Q1" pad="3"/>
<contactref element="R1" pad="P$1"/>
</signal>
<signal name="3.3V">
<contactref element="Q1" pad="2"/>
<contactref element="Q3" pad="2"/>
<contactref element="Q5" pad="2"/>
<contactref element="Q7" pad="2"/>
<contactref element="Q9" pad="2"/>
<contactref element="Q11" pad="2"/>
<contactref element="J7" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="J2" pad="2"/>
<contactref element="Q4" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="Q4" pad="1"/>
<contactref element="Q3" pad="3"/>
<contactref element="R2" pad="P$1"/>
</signal>
<signal name="N$7">
<contactref element="J3" pad="2"/>
<contactref element="Q6" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="Q6" pad="1"/>
<contactref element="Q5" pad="3"/>
<contactref element="R3" pad="P$1"/>
</signal>
<signal name="N$10">
<contactref element="J4" pad="2"/>
<contactref element="Q8" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="Q8" pad="1"/>
<contactref element="Q7" pad="3"/>
<contactref element="R4" pad="P$1"/>
</signal>
<signal name="N$13">
<contactref element="J5" pad="2"/>
<contactref element="Q10" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="Q10" pad="1"/>
<contactref element="Q9" pad="3"/>
<contactref element="R5" pad="P$1"/>
</signal>
<signal name="N$16">
<contactref element="J6" pad="2"/>
<contactref element="Q12" pad="2"/>
</signal>
<signal name="N$17">
<contactref element="Q12" pad="1"/>
<contactref element="Q11" pad="3"/>
<contactref element="R6" pad="P$1"/>
</signal>
<signal name="GND">
<contactref element="Q2" pad="3"/>
<contactref element="Q4" pad="3"/>
<contactref element="Q6" pad="3"/>
<contactref element="Q8" pad="3"/>
<contactref element="Q10" pad="3"/>
<contactref element="Q12" pad="3"/>
<contactref element="J8" pad="2"/>
<contactref element="J7" pad="8"/>
</signal>
<signal name="C1">
<contactref element="Q1" pad="1"/>
<contactref element="J7" pad="7"/>
</signal>
<signal name="C2">
<contactref element="Q3" pad="1"/>
<contactref element="J7" pad="6"/>
</signal>
<signal name="C3">
<contactref element="Q5" pad="1"/>
<contactref element="J7" pad="5"/>
</signal>
<signal name="C4">
<contactref element="Q7" pad="1"/>
<contactref element="J7" pad="4"/>
</signal>
<signal name="C5">
<contactref element="Q9" pad="1"/>
<contactref element="J7" pad="3"/>
</signal>
<signal name="C6">
<contactref element="Q11" pad="1"/>
<contactref element="J7" pad="2"/>
</signal>
<signal name="N$3">
</signal>
<signal name="N$6">
</signal>
<signal name="N$9">
</signal>
</signals>
</board>
</drawing>
</eagle>
