<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="16.51" x2="0" y2="3.81" width="0" layer="20"/>
<wire x1="0" y1="3.81" x2="3.81" y2="0" width="0" layer="20" curve="90"/>
<wire x1="3.81" y1="0" x2="33.02" y2="0" width="0" layer="20"/>
<wire x1="33.02" y1="0" x2="35.56" y2="2.54" width="0" layer="20" curve="90"/>
<wire x1="35.56" y1="2.54" x2="35.56" y2="17.78" width="0" layer="20"/>
<wire x1="35.56" y1="17.78" x2="33.02" y2="20.32" width="0" layer="20" curve="90"/>
<wire x1="33.02" y1="20.32" x2="3.81" y2="20.32" width="0" layer="20"/>
<wire x1="3.81" y1="20.32" x2="0" y2="16.51" width="0" layer="20" curve="90"/>
<text>R0</text>
<text>T1</text>
<text>X2</text>
<text>X3</text>
<text>RST</text>
<text>4</text>
<text>5</text>
<text>6</text>
<text>7</text>
<text>8</text>
<text>9</text>
<text>10</text>
<text>11</text>
<text>12</text>
<text>13</text>
<text>14</text>
<text>15</text>
<text>16</text>
<text>V+</text>
<text>GND</text>
<text>Pixie</text>
<text>2313</text>
<text>Barbary</text>
<text>Enterprises</text>
<text>ATtiny2313</text>
</plain>
<libraries>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DIL20">
</package>
</packages>
</library>
<library name="barbary_enterprises">
<packages>
<package name="2X3-NS">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X10">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="SparkFun-DigitalIC" package="DIL20" value="">
<attribute name="VALUE"/>
</element>
<element name="J1" library="barbary_enterprises" package="2X3-NS" value="AVR_SPI_PRG_6LABELED"/>
<element name="JP1" library="SparkFun-Connectors" package="1X10" value="M10&quot;"/>
<element name="JP2" library="SparkFun-Connectors" package="1X10" value="M10&quot;"/>
</elements>
<signals>
<signal name="VCC">
<contactref element="U1" pad="20"/>
<contactref element="J1" pad="2"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="GND">
<contactref element="U1" pad="10"/>
<contactref element="J1" pad="6"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="RST">
<contactref element="U1" pad="1"/>
<contactref element="J1" pad="5"/>
<contactref element="JP1" pad="10"/>
</signal>
<signal name="0">
<contactref element="U1" pad="2"/>
<contactref element="JP1" pad="9"/>
</signal>
<signal name="1">
<contactref element="U1" pad="3"/>
<contactref element="JP1" pad="8"/>
</signal>
<signal name="X2">
<contactref element="U1" pad="4"/>
<contactref element="JP1" pad="7"/>
</signal>
<signal name="X1">
<contactref element="U1" pad="5"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="2">
<contactref element="U1" pad="6"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="3">
<contactref element="U1" pad="7"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="4">
<contactref element="U1" pad="8"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="5">
<contactref element="U1" pad="9"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="6">
<contactref element="U1" pad="11"/>
<contactref element="JP2" pad="10"/>
</signal>
<signal name="7">
<contactref element="U1" pad="12"/>
<contactref element="JP2" pad="9"/>
</signal>
<signal name="8">
<contactref element="U1" pad="13"/>
<contactref element="JP2" pad="8"/>
</signal>
<signal name="9">
<contactref element="U1" pad="14"/>
<contactref element="JP2" pad="7"/>
</signal>
<signal name="10">
<contactref element="U1" pad="15"/>
<contactref element="JP2" pad="6"/>
</signal>
<signal name="11">
<contactref element="U1" pad="16"/>
<contactref element="JP2" pad="5"/>
</signal>
<signal name="12">
<contactref element="U1" pad="17"/>
<contactref element="J1" pad="4"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="13">
<contactref element="U1" pad="18"/>
<contactref element="J1" pad="1"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="14">
<contactref element="U1" pad="19"/>
<contactref element="J1" pad="3"/>
<contactref element="JP2" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
