<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.3.1">
<drawing>
<board>
<plain>
<polygon width="0.0762" layer="20">
<vertex x="19.05" y="9.525"/>
<vertex x="18.415" y="9.525" curve="90"/>
<vertex x="17.78" y="8.89"/>
<vertex x="17.78" y="5.08"/>
<vertex x="17.78" y="2.54" curve="90"/>
<vertex x="18.415" y="1.905"/>
<vertex x="19.05" y="1.905"/>
<vertex x="19.685" y="1.905" curve="90"/>
<vertex x="20.32" y="2.54"/>
<vertex x="20.32" y="5.715"/>
<vertex x="20.32" y="8.89" curve="90"/>
<vertex x="19.685" y="9.525"/>
</polygon>
<polygon width="0.0762" layer="20">
<vertex x="29.21" y="9.525"/>
<vertex x="28.575" y="9.525" curve="90"/>
<vertex x="27.94" y="8.89"/>
<vertex x="27.94" y="5.08"/>
<vertex x="27.94" y="2.54" curve="90"/>
<vertex x="28.575" y="1.905"/>
<vertex x="29.21" y="1.905"/>
<vertex x="29.845" y="1.905" curve="90"/>
<vertex x="30.48" y="2.54"/>
<vertex x="30.48" y="8.89" curve="90"/>
<vertex x="29.845" y="9.525"/>
</polygon>
<polygon width="0.0762" layer="20">
<vertex x="34.925" y="9.525"/>
<vertex x="34.29" y="9.525" curve="90"/>
<vertex x="33.655" y="8.89"/>
<vertex x="33.655" y="5.08"/>
<vertex x="33.655" y="2.54" curve="90"/>
<vertex x="34.29" y="1.905"/>
<vertex x="34.925" y="1.905"/>
<vertex x="35.56" y="1.905" curve="90"/>
<vertex x="36.195" y="2.54"/>
<vertex x="36.195" y="6.35"/>
<vertex x="36.195" y="8.89" curve="90"/>
<vertex x="35.56" y="9.525"/>
</polygon>
<polygon width="0.0762" layer="20">
<vertex x="47.625" y="9.525"/>
<vertex x="46.99" y="9.525" curve="90"/>
<vertex x="46.355" y="8.89"/>
<vertex x="46.355" y="5.715"/>
<vertex x="46.355" y="2.54" curve="90"/>
<vertex x="46.99" y="1.905"/>
<vertex x="47.625" y="1.905"/>
<vertex x="48.26" y="1.905" curve="90"/>
<vertex x="48.895" y="2.54"/>
<vertex x="48.895" y="6.985"/>
<vertex x="48.895" y="8.89" curve="90"/>
<vertex x="48.26" y="9.525"/>
</polygon>
<wire x1="5.08" y1="0" x2="0" y2="5.08" width="0" layer="20" curve="-90"/>
<wire x1="0" y1="5.08" x2="0" y2="34.29" width="0" layer="20"/>
<wire x1="0" y1="34.29" x2="5.715" y2="40.64" width="0" layer="20" curve="-90"/>
<wire x1="5.715" y1="40.64" x2="59.69" y2="40.64" width="0" layer="20"/>
<wire x1="59.69" y1="40.64" x2="64.77" y2="34.925" width="0" layer="20" curve="-90"/>
<wire x1="64.77" y1="34.925" x2="64.77" y2="5.08" width="0" layer="20"/>
<wire x1="64.77" y1="5.08" x2="59.69" y2="0" width="0" layer="20" curve="-90"/>
<wire x1="59.69" y1="0" x2="5.08" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X4">
</package>
<package name="1X04_LOCK">
</package>
</packages>
</library>
<library name="SRG">
<description>Components Scott made</description>
<packages>
<package name="DIGISPARK">
<description>DigiSpark &lt;br&gt;</description>
</package>
</packages>
</library>
<library name="Rembrandt Electronics - JST XH Connectors v1-0">
<packages>
<package name="JST-XH-08-PACKAGE-ROUND-PAD">
<description>&lt;b&gt;JST XH Connector Round Pads (Package)&lt;/b&gt;&lt;p&gt;

Wire to board connector.

Pitch: 2,54 mm, (0.100")&lt;p&gt;
Number of pins: &lt;b&gt;8&lt;/b&gt;&lt;b&gt;&lt;P&gt;

&lt;b&gt;Created by Rembrandt Electronics&lt;/b&gt;&lt;p&gt;
&lt;b&gt;www.rembrandtelectronics.com&lt;/b&gt;&lt;p&gt;</description>
</package>
</packages>
</library>
<library name="TMP36">
<packages>
<package name="SOT-23">
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT323">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1206">
</package>
</packages>
</library>
<library name="holes">
<description>&lt;b&gt;Mounting Holes and Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="3,6">
<description>&lt;b&gt;MOUNTING HOLE&lt;/b&gt; 3.6 mm with drill center</description>
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="ML-E">
<description>&lt;b&gt;Cree® XLamp® ML-E LEDs&lt;/b&gt; 1/2 watt, 3.5 x 3.5 mm&lt;p&gt;
Source: &lt;a href="http://www.cree.com/products/pdf/XLampML-E.pdf"&gt; Data sheet &lt;/a&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1206">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="FAN" library="SparkFun-Connectors" package="2X4" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="SRG" package="DIGISPARK" value="DIGISPARK">
<attribute name="NAME"/>
</element>
<element name="U$2" library="TMP36" package="SOT-23" value="TMP36"/>
<element name="Q1" library="SparkFun-DiscreteSemi" package="SOT323" value="MOSFET-NCHANNEL2N7002PW">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="TRANS-11151"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="1206" value="1.5ohm">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="H1" library="holes" package="3,6" value="MOUNT-HOLE3.6"/>
<element name="H2" library="holes" package="3,6" value="MOUNT-HOLE3.6"/>
<element name="H3" library="holes" package="3,6" value="MOUNT-HOLE3.6"/>
<element name="H4" library="holes" package="3,6" value="MOUNT-HOLE3.6"/>
<element name="LED3" library="led" package="ML-E" value="ML-E"/>
<element name="LED4" library="led" package="ML-E" value="ML-E"/>
<element name="X2" library="Rembrandt Electronics - JST XH Connectors v1-0" package="JST-XH-08-PACKAGE-ROUND-PAD" value="JST-XH-08-PIN-ROUND-PAD"/>
<element name="C1" library="SparkFun-Capacitors" package="1206" value=""/>
<element name="JP2" library="SparkFun-Connectors" package="1X04_LOCK" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="U$1" pad="GND"/>
<contactref element="FAN" pad="8"/>
<contactref element="U$2" pad="5"/>
<contactref element="Q1" pad="2"/>
<contactref element="X2" pad="8"/>
<contactref element="X2" pad="4"/>
<contactref element="X2" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="RAW">
<contactref element="U$1" pad="VIN"/>
<contactref element="X2" pad="7"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="5V">
<contactref element="U$1" pad="5V"/>
<contactref element="U$2" pad="2"/>
<contactref element="LED3" pad="A@1"/>
<contactref element="X2" pad="6"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="SW1">
<contactref element="U$1" pad="P4"/>
<contactref element="X2" pad="3"/>
</signal>
<signal name="LEDSW">
<contactref element="U$1" pad="P3"/>
<contactref element="X2" pad="1"/>
</signal>
<signal name="PWM">
<contactref element="FAN" pad="2"/>
<contactref element="U$1" pad="P1"/>
</signal>
<signal name="TACH">
<contactref element="FAN" pad="4"/>
</signal>
<signal name="12V">
<contactref element="FAN" pad="6"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="POT">
<contactref element="U$1" pad="P2"/>
<contactref element="X2" pad="5"/>
</signal>
<signal name="TMP">
<contactref element="U$1" pad="P5"/>
<contactref element="U$2" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="LED3" pad="C@1"/>
<contactref element="LED4" pad="A@1"/>
</signal>
<signal name="N$5">
<contactref element="U$2" pad="4"/>
</signal>
<signal name="N$3">
<contactref element="Q1" pad="3"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="R1" pad="2"/>
<contactref element="LED4" pad="C@1"/>
</signal>
<signal name="GATE">
<contactref element="U$1" pad="P0"/>
<contactref element="Q1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
