<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.4.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="50.8" y2="0" width="0" layer="20"/>
<wire x1="50.8" y1="0" x2="50.8" y2="33.01" width="0" layer="20"/>
<wire x1="50.8" y1="33.01" x2="0" y2="33.01" width="0" layer="20"/>
<wire x1="0" y1="33.01" x2="0" y2="0" width="0" layer="20"/>
<text>IC2</text>
<text>CPT-O r0.1 09/02/2016
Made in El Salvador
</text>
<text>A0</text>
<text>A1</text>
<text>A2</text>
<text>A3</text>
<text>A4</text>
<text>A5</text>
<text>D1</text>
<text>D0</text>
<text>D2</text>
<text>D3</text>
<text>D4</text>
<text>D5</text>
<text>GND</text>
<text>AREF</text>
<text>5V</text>
<text>HWB</text>
<text>D13</text>
<text>D12</text>
<text>D11</text>
<text>D10</text>
<text>D9</text>
<text>D8</text>
<text>D7</text>
<text>D6</text>
<text>Designed by TeUbi.co in 
collaboration with MicroCode
for the OpenHardware.sv
community in El Salvador.</text>
</plain>
<libraries>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SPARKFUN-DIGITALIC_TQFP44">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="USB-MINIB">
<description>&lt;b&gt;USB Series Mini-B Surface Mounted&lt;/b&gt;</description>
</package>
<package name="1X12">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE_SWITCH_SMD">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="AVRISP">
</package>
<package name="CTS406">
<description>&lt;b&gt;Model 406 6.0x3.5mm Low Cost Surface Mount Crystal&lt;/b&gt;&lt;p&gt;
Source: 008-0260-0_E.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-1206">
</package>
</packages>
</library>
<library name="custom_components">
<packages>
<package name="RPI-1031">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="SparkFun-DigitalIC" package="SPARKFUN-DIGITALIC_TQFP44" value="ATMEGA32U4TQFP">
<attribute name="NAME"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0805" value="22">
<attribute name="NAME"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0805" value="22">
<attribute name="NAME"/>
</element>
<element name="USB_CONN" library="SparkFun-Connectors" package="USB-MINIB" value="USB-MINIB-5PIN">
<attribute name="NAME"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="0805" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="Q1" library="adafruit" package="CTS406" value="16Mhz">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0805" value="18pF">
<attribute name="NAME"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="0805" value="18pF">
<attribute name="NAME"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="0805" value="10k">
<attribute name="NAME"/>
</element>
<element name="ISP1" library="adafruit" package="AVRISP" value="AVRISP-6">
<attribute name="NAME"/>
</element>
<element name="RX_LED" library="SparkFun-LED" package="LED-1206" value="BLUE">
<attribute name="PROD_ID" value="DIO-09955"/>
<attribute name="VALUE" value="WHITE"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TX_LED" library="SparkFun-LED" package="LED-1206" value="RED">
<attribute name="PROD_ID" value="DIO-09955"/>
<attribute name="VALUE" value="WHITE"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="0805" value="85">
<attribute name="NAME"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="0805" value="150">
<attribute name="NAME"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="1X12" value="M12PTH">
<attribute name="NAME"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="1X12" value="M12PTH">
<attribute name="NAME"/>
</element>
<element name="IC2" library="custom_components" package="RPI-1031" value="RPI-1031"/>
<element name="R6" library="SparkFun-Resistors" package="0805" value="10k">
<attribute name="NAME"/>
</element>
<element name="R7" library="SparkFun-Resistors" package="0805" value="22k">
<attribute name="NAME"/>
</element>
<element name="R8" library="SparkFun-Resistors" package="0805" value="22k">
<attribute name="NAME"/>
</element>
<element name="LED3" library="SparkFun-LED" package="LED-1206" value="YELLOW">
<attribute name="PROD_ID" value="DIO-09955"/>
<attribute name="VALUE" value="WHITE"/>
<attribute name="NAME"/>
</element>
<element name="LED4" library="SparkFun-LED" package="LED-1206" value="BLUE">
<attribute name="PROD_ID" value="DIO-09955"/>
<attribute name="VALUE" value="WHITE"/>
<attribute name="NAME"/>
</element>
<element name="LED5" library="SparkFun-LED" package="LED-1206" value="GREEN">
<attribute name="PROD_ID" value="DIO-09955"/>
<attribute name="VALUE" value="WHITE"/>
<attribute name="NAME"/>
</element>
<element name="LED6" library="SparkFun-LED" package="LED-1206" value="RED">
<attribute name="PROD_ID" value="DIO-09955"/>
<attribute name="VALUE" value="WHITE"/>
<attribute name="NAME"/>
</element>
<element name="R16" library="SparkFun-Resistors" package="0805" value="150">
<attribute name="NAME"/>
</element>
<element name="R17" library="SparkFun-Resistors" package="0805" value="85">
<attribute name="NAME"/>
</element>
<element name="R18" library="SparkFun-Resistors" package="0805" value="150">
<attribute name="NAME"/>
</element>
<element name="R19" library="SparkFun-Resistors" package="0805" value="150">
<attribute name="NAME"/>
</element>
<element name="S2" library="SparkFun-Electromechanical" package="TACTILE_SWITCH_SMD" value="SWITCH-MOMENTARY-2SMD">
<attribute name="NAME"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="0805" value="0.1uF"/>
</elements>
<signals>
<signal name="D_USBRD+">
<contactref element="R2" pad="2"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="D_USBRD-">
<contactref element="IC1" pad="4"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="D_USBD-">
<contactref element="R1" pad="1"/>
<contactref element="USB_CONN" pad="D+"/>
</signal>
<signal name="GND">
<contactref element="USB_CONN" pad="GND"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="IC1" pad="5"/>
<contactref element="IC1" pad="15"/>
<contactref element="IC1" pad="23"/>
<contactref element="IC1" pad="35"/>
<contactref element="IC1" pad="43"/>
<contactref element="ISP1" pad="6"/>
<contactref element="RX_LED" pad="C"/>
<contactref element="TX_LED" pad="C"/>
<contactref element="JP2" pad="12"/>
<contactref element="IC2" pad="3"/>
<contactref element="R7" pad="1"/>
<contactref element="R8" pad="1"/>
<contactref element="LED6" pad="C"/>
<contactref element="LED5" pad="C"/>
<contactref element="LED4" pad="C"/>
<contactref element="LED3" pad="C"/>
<contactref element="S2" pad="1"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="D_USBD+">
<contactref element="USB_CONN" pad="D-"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="IC1" pad="6"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="IC1" pad="16"/>
<contactref element="Q1" pad="3"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="IC1" pad="17"/>
<contactref element="Q1" pad="1"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="5V">
<contactref element="IC1" pad="7"/>
<contactref element="IC1" pad="14"/>
<contactref element="IC1" pad="2"/>
<contactref element="IC1" pad="34"/>
<contactref element="IC1" pad="24"/>
<contactref element="IC1" pad="44"/>
<contactref element="USB_CONN" pad="VBUS"/>
<contactref element="R3" pad="2"/>
<contactref element="ISP1" pad="2"/>
<contactref element="JP2" pad="10"/>
<contactref element="R6" pad="2"/>
<contactref element="IC2" pad="2"/>
<contactref element="IC2" pad="5"/>
<contactref element="C4" pad="2"/>
</signal>
<signal name="RST_SIG">
<contactref element="IC1" pad="13"/>
<contactref element="R3" pad="1"/>
<contactref element="ISP1" pad="5"/>
<contactref element="S2" pad="3"/>
</signal>
<signal name="MISO_SIG">
<contactref element="IC1" pad="11"/>
<contactref element="ISP1" pad="1"/>
</signal>
<signal name="MOSI_SIG">
<contactref element="IC1" pad="10"/>
<contactref element="ISP1" pad="4"/>
</signal>
<signal name="SCK_SIG">
<contactref element="IC1" pad="9"/>
<contactref element="ISP1" pad="3"/>
</signal>
<signal name="N$11">
<contactref element="R4" pad="1"/>
<contactref element="RX_LED" pad="A"/>
</signal>
<signal name="N$12">
<contactref element="R5" pad="1"/>
<contactref element="TX_LED" pad="A"/>
</signal>
<signal name="A0">
<contactref element="IC1" pad="36"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="A1">
<contactref element="IC1" pad="37"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="A2">
<contactref element="IC1" pad="38"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="A3">
<contactref element="IC1" pad="39"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="A4">
<contactref element="IC1" pad="40"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="A5">
<contactref element="IC1" pad="41"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="D0">
<contactref element="IC1" pad="20"/>
<contactref element="JP1" pad="7"/>
</signal>
<signal name="D1">
<contactref element="IC1" pad="21"/>
<contactref element="JP1" pad="8"/>
</signal>
<signal name="D6">
<contactref element="IC1" pad="27"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="D8">
<contactref element="IC1" pad="28"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="D9">
<contactref element="IC1" pad="29"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="D10">
<contactref element="IC1" pad="30"/>
<contactref element="JP2" pad="5"/>
<contactref element="R16" pad="2"/>
</signal>
<signal name="D11">
<contactref element="IC1" pad="12"/>
<contactref element="JP2" pad="6"/>
<contactref element="R17" pad="2"/>
</signal>
<signal name="D12">
<contactref element="IC1" pad="26"/>
<contactref element="JP2" pad="7"/>
<contactref element="R18" pad="2"/>
</signal>
<signal name="D13">
<contactref element="IC1" pad="32"/>
<contactref element="JP2" pad="8"/>
<contactref element="R19" pad="2"/>
</signal>
<signal name="RXL_SIG">
<contactref element="IC1" pad="8"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="TXL_SIG">
<contactref element="IC1" pad="22"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="HWB_SIG">
<contactref element="IC1" pad="33"/>
<contactref element="JP2" pad="9"/>
</signal>
<signal name="AREF_SIG">
<contactref element="IC1" pad="42"/>
<contactref element="JP2" pad="11"/>
</signal>
<signal name="N$30">
<contactref element="IC2" pad="6"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="D4">
<contactref element="IC2" pad="4"/>
<contactref element="R7" pad="2"/>
<contactref element="IC1" pad="25"/>
<contactref element="JP1" pad="11"/>
</signal>
<signal name="D2">
<contactref element="IC1" pad="19"/>
<contactref element="JP1" pad="9"/>
</signal>
<signal name="D3">
<contactref element="IC1" pad="18"/>
<contactref element="JP1" pad="10"/>
</signal>
<signal name="D7">
<contactref element="IC1" pad="1"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="R16" pad="1"/>
<contactref element="LED3" pad="A"/>
</signal>
<signal name="N$21">
<contactref element="R17" pad="1"/>
<contactref element="LED4" pad="A"/>
</signal>
<signal name="N$22">
<contactref element="R18" pad="1"/>
<contactref element="LED5" pad="A"/>
</signal>
<signal name="N$23">
<contactref element="R19" pad="1"/>
<contactref element="LED6" pad="A"/>
</signal>
<signal name="D5">
<contactref element="JP1" pad="12"/>
<contactref element="IC1" pad="31"/>
<contactref element="IC2" pad="1"/>
<contactref element="R8" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
