<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.0.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="13.97" x2="0" y2="1.27" width="0" layer="20"/>
<wire x1="0" y1="13.97" x2="1.27" y2="15.24" width="0" layer="20"/>
<wire x1="1.27" y1="15.24" x2="13.97" y2="15.24" width="0" layer="20"/>
<wire x1="13.97" y1="15.24" x2="15.24" y2="13.97" width="0" layer="20"/>
<wire x1="15.24" y1="13.97" x2="15.24" y2="1.27" width="0" layer="20"/>
<wire x1="15.24" y1="1.27" x2="13.97" y2="0" width="0" layer="20"/>
<wire x1="13.97" y1="0" x2="1.27" y2="0" width="0" layer="20"/>
<wire x1="1.27" y1="0" x2="0" y2="1.27" width="0" layer="20"/>
<text>R</text>
<text>U</text>
<text>G</text>
<text>B</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X4">
<description>&lt;h3&gt;Plated Through Hole - 2x4&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:8&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="Richard">
<packages>
<package name="STEPPER_ONBOARD">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="Richard" package="STEPPER_ONBOARD" value="STEPPERW_HOLES"/>
<element name="J2" library="SparkFun-Connectors" package="2X4" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="RED">
<contactref element="U$1" pad="RED"/>
<contactref element="J2" pad="5"/>
<contactref element="J2" pad="7"/>
</signal>
<signal name="BLUE">
<contactref element="U$1" pad="BLUE"/>
<contactref element="J2" pad="6"/>
<contactref element="J2" pad="8"/>
</signal>
<signal name="GREEN">
<contactref element="U$1" pad="GREEN"/>
<contactref element="J2" pad="2"/>
<contactref element="J2" pad="4"/>
</signal>
<signal name="BLACK">
<contactref element="U$1" pad="BLACK"/>
<contactref element="J2" pad="3"/>
<contactref element="J2" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
