<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<text>VIDEO GRAPHICS CARD</text>
<text>(C) 2018 Marco Maccaferri</text>
<wire x1="0" y1="0" x2="99.106" y2="0" width="0" layer="20"/>
<wire x1="99.106" y1="0" x2="99.106" y2="44.76" width="0" layer="20"/>
<wire x1="99.106" y1="44.76" x2="94.006" y2="49.86" width="0" layer="20" curve="90"/>
<wire x1="94.006" y1="49.86" x2="15.011" y2="49.86" width="0" layer="20"/>
<wire x1="15.011" y1="49.86" x2="0" y2="34.849" width="0" layer="20"/>
<wire x1="0" y1="34.849" x2="0" y2="0" width="0" layer="20"/>
<text>Designed for RC2014 Computer</text>
<hole x="5.029" y="33.122" drill="3.2"/>
<text>VGA / RGB</text>
<text>PROP-PLUG</text>
<text>5V</text>
<text>3.3V</text>
<text>!WAIT!</text>
<text>https://www.github.com/maccasoft</text>
</plain>
<libraries>
<library name="rc2014-vga">
<description>Generated from &lt;b&gt;rc2014-vga.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="HEADER_PRG_1X05">
</package>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="HC49/S">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="TO92">
<description>&lt;b&gt;TO 92&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="rc2014-graphics-card">
<description>Generated from &lt;b&gt;rc2014-vga.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="DIL40">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="0204/7">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 7.5 mm</description>
</package>
<package name="RC2014BUS">
</package>
<package name="1X01">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="DO35-7">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 2 mm, horizontal, grid 7.62 mm</description>
</package>
<package name="VGA">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
</package>
<package name="0207/10">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 10 mm</description>
</package>
<package name="C050-025X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 2.5 x 7.5 mm</description>
</package>
<package name="E2,5-6">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.54 mm, diameter 6 mm</description>
</package>
<package name="1X02">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="p8x-2016-propplug">
<description>Generated from &lt;b&gt;p8x-2016-propplug.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="TO92">
<description>&lt;b&gt;TO 92&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="CN1" library="rc2014-graphics-card" package="RC2014BUS" value="RC2014BUS">
<attribute name="MPN" value="PRPC040SBAN-M71RC"/>
</element>
<element name="IC2" library="rc2014-graphics-card" package="DIL40" value="P8X32A-B-D40">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MPN" value="P8X32A-D40"/>
</element>
<element name="XTAL1" library="rc2014-vga" package="HC49/S" value="5MHz">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MPN" value="ECS-50-20-4X"/>
</element>
<element name="C3" library="rc2014-graphics-card" package="C050-025X075" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MPN" value="R82EC3100AA70J"/>
</element>
<element name="C2" library="rc2014-graphics-card" package="C050-025X075" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MPN" value="R82EC3100AA70J"/>
</element>
<element name="R11" library="rc2014-graphics-card" package="0207/10" value="240 1%">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MPN" value="RNMF14FTC240R"/>
</element>
<element name="R12" library="rc2014-graphics-card" package="0207/10" value="240 1%">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MPN" value="RNMF14FTC240R"/>
</element>
<element name="R5" library="rc2014-graphics-card" package="0207/10" value="510 1%">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MPN" value="RNMF14FTC510R"/>
</element>
<element name="R6" library="rc2014-graphics-card" package="0207/10" value="240 1%">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MPN" value="RNMF14FTC240R"/>
</element>
<element name="R7" library="rc2014-graphics-card" package="0207/10" value="510 1%">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MPN" value="RNMF14FTC510R"/>
</element>
<element name="R8" library="rc2014-graphics-card" package="0207/10" value="240 1%">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MPN" value="RNMF14FTC240R"/>
</element>
<element name="R9" library="rc2014-graphics-card" package="0207/10" value="510 1%">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MPN" value="RNMF14FTC510R"/>
</element>
<element name="R10" library="rc2014-graphics-card" package="0207/10" value="240 1%">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MPN" value="RNMF14FTC240R"/>
</element>
<element name="R15" library="rc2014-graphics-card" package="0207/10" value="130 1%">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MPN" value="RNMF14FTC130R"/>
</element>
<element name="R14" library="rc2014-graphics-card" package="0207/10" value="130 1%">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MPN" value="RNMF14FTC130R"/>
</element>
<element name="R13" library="rc2014-graphics-card" package="0207/10" value="130 1%">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MPN" value="RNMF14FTC130R"/>
</element>
<element name="C1" library="rc2014-graphics-card" package="E2,5-6" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MPN" value="ESK105M050AC3AA"/>
</element>
<element name="IC1" library="rc2014-vga" package="TO92" value="MCP1700">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MPN" value="MCP1700-3302E/TO"/>
</element>
<element name="CN2" library="rc2014-graphics-card" package="VGA" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value="1734344-1"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="rc2014-graphics-card" package="0207/10" value="4k7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MPN" value="CFR-25JB-52-4K7"/>
</element>
<element name="R1" library="rc2014-graphics-card" package="0207/10" value="4k7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MPN" value="CFR-25JB-52-4K7"/>
</element>
<element name="IC3" library="rc2014-vga" package="DIL08" value="24LC512-I/P">
<attribute name="NAME"/>
<attribute name="MPN" value="24LC256-I/P"/>
</element>
<element name="C4" library="rc2014-graphics-card" package="C050-025X075" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MPN" value="R82EC3100AA70J"/>
</element>
<element name="CN4" library="rc2014-vga" package="HEADER_PRG_1X05" value="PROPELLER_ICSP_HEADER">
<attribute name="MPN" value="PRPC005SAAN-RC"/>
</element>
<element name="R16" library="rc2014-graphics-card" package="0204/7" value="4k7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R17" library="rc2014-graphics-card" package="0204/7" value="4k7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R18" library="rc2014-graphics-card" package="0204/7" value="4k7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R19" library="rc2014-graphics-card" package="0204/7" value="4k7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R20" library="rc2014-graphics-card" package="0204/7" value="4k7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R21" library="rc2014-graphics-card" package="0204/7" value="4k7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R22" library="rc2014-graphics-card" package="0204/7" value="4k7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R23" library="rc2014-graphics-card" package="0204/7" value="4k7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="rc2014-graphics-card" package="DO35-7" value="1N4148DO35-7">
<attribute name="NAME"/>
</element>
<element name="D3" library="rc2014-graphics-card" package="DO35-7" value="1N4148DO35-7">
<attribute name="NAME"/>
</element>
<element name="D4" library="rc2014-graphics-card" package="DO35-7" value="1N4148DO35-7">
<attribute name="NAME"/>
</element>
<element name="D5" library="rc2014-graphics-card" package="DO35-7" value="1N4148DO35-7">
<attribute name="NAME"/>
</element>
<element name="R26" library="rc2014-graphics-card" package="0204/7" value="4k7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R28" library="rc2014-graphics-card" package="0204/7" value="4k7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R27" library="rc2014-graphics-card" package="0204/7" value="4k7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R25" library="rc2014-graphics-card" package="0204/7" value="4k7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R30" library="rc2014-graphics-card" package="0204/7" value="4k7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R29" library="rc2014-graphics-card" package="0204/7" value="4k7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R31" library="rc2014-graphics-card" package="0204/7" value="4k7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="rc2014-graphics-card" package="DO35-7" value="1N4148DO35-7">
<attribute name="NAME"/>
</element>
<element name="R32" library="rc2014-graphics-card" package="0204/7" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R24" library="rc2014-graphics-card" package="0204/7" value="4k7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="rc2014-graphics-card" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="rc2014-graphics-card" package="E2,5-6" value="1uF">
<attribute name="MPN" value="ESK105M050AC3AA"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TR1" library="p8x-2016-propplug" package="TO92" value="BC547A">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="rc2014-graphics-card" package="0204/7" value="33k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="rc2014-graphics-card" package="1X01" value="">
<attribute name="VALUE"/>
</element>
<element name="R3" library="rc2014-graphics-card" package="0207/10" value="1k2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP3" library="rc2014-graphics-card" package="1X02" value="">
<attribute name="NAME"/>
</element>
<element name="JP4" library="rc2014-graphics-card" package="1X02" value="">
<attribute name="NAME"/>
</element>
<element name="R33" library="rc2014-graphics-card" package="0207/10" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R34" library="rc2014-graphics-card" package="0207/10" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="IC2" pad="30"/>
<contactref element="XTAL1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="IC2" pad="31"/>
<contactref element="XTAL1" pad="2"/>
</signal>
<signal name="GND">
<contactref element="IC2" pad="9"/>
<contactref element="IC2" pad="29"/>
<contactref element="IC2" pad="10"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="R15" pad="1"/>
<contactref element="R13" pad="1"/>
<contactref element="R14" pad="1"/>
<contactref element="IC1" pad="1"/>
<contactref element="C1" pad="-"/>
<contactref element="CN2" pad="5"/>
<contactref element="CN2" pad="4"/>
<contactref element="CN2" pad="10"/>
<contactref element="CN2" pad="11"/>
<contactref element="CN2" pad="6"/>
<contactref element="CN2" pad="7"/>
<contactref element="CN2" pad="8"/>
<contactref element="CN1" pad="GND"/>
<contactref element="IC3" pad="1"/>
<contactref element="IC3" pad="4"/>
<contactref element="IC3" pad="3"/>
<contactref element="IC3" pad="2"/>
<contactref element="IC3" pad="7"/>
<contactref element="C4" pad="2"/>
<contactref element="CN4" pad="1"/>
<contactref element="R32" pad="1"/>
<contactref element="C5" pad="-"/>
<contactref element="R4" pad="2"/>
<contactref element="TR1" pad="3"/>
<contactref element="JP3" pad="2"/>
<contactref element="JP4" pad="2"/>
</signal>
<signal name="B">
<contactref element="R9" pad="2"/>
<contactref element="R10" pad="2"/>
<contactref element="R15" pad="2"/>
<contactref element="CN2" pad="3"/>
</signal>
<signal name="HSYNC">
<contactref element="R12" pad="2"/>
<contactref element="CN2" pad="13"/>
</signal>
<signal name="VSYNC">
<contactref element="R11" pad="2"/>
<contactref element="CN2" pad="14"/>
</signal>
<signal name="G">
<contactref element="R7" pad="2"/>
<contactref element="R8" pad="2"/>
<contactref element="R14" pad="2"/>
<contactref element="CN2" pad="2"/>
</signal>
<signal name="R">
<contactref element="R5" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="R13" pad="2"/>
<contactref element="CN2" pad="1"/>
</signal>
<signal name="P16">
<contactref element="IC2" pad="21"/>
<contactref element="R11" pad="1"/>
</signal>
<signal name="P17">
<contactref element="IC2" pad="22"/>
<contactref element="R12" pad="1"/>
</signal>
<signal name="P18">
<contactref element="IC2" pad="23"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="P19">
<contactref element="IC2" pad="24"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="P20">
<contactref element="IC2" pad="25"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="P21">
<contactref element="IC2" pad="26"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="P22">
<contactref element="IC2" pad="27"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="P23">
<contactref element="IC2" pad="28"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="+3.3V">
<contactref element="C1" pad="+"/>
<contactref element="IC1" pad="3"/>
<contactref element="IC2" pad="32"/>
<contactref element="IC2" pad="12"/>
<contactref element="C3" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="IC3" pad="8"/>
<contactref element="C4" pad="1"/>
<contactref element="CN4" pad="5"/>
<contactref element="JP1" pad="1"/>
<contactref element="R33" pad="1"/>
<contactref element="R34" pad="1"/>
</signal>
<signal name="GPU_SCL">
<contactref element="IC2" pad="37"/>
<contactref element="R1" pad="1"/>
<contactref element="IC3" pad="6"/>
</signal>
<signal name="GPU_SDA">
<contactref element="IC2" pad="38"/>
<contactref element="R2" pad="1"/>
<contactref element="IC3" pad="5"/>
</signal>
<signal name="+5V">
<contactref element="CN1" pad="+5V"/>
<contactref element="IC1" pad="2"/>
<contactref element="JP1" pad="3"/>
<contactref element="C5" pad="+"/>
</signal>
<signal name="N$11">
<contactref element="IC2" pad="11"/>
<contactref element="CN4" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="IC2" pad="40"/>
<contactref element="CN4" pad="3"/>
</signal>
<signal name="N$14">
<contactref element="IC2" pad="39"/>
<contactref element="CN4" pad="4"/>
</signal>
<signal name="N$3">
<contactref element="CN1" pad="D3"/>
<contactref element="R19" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="CN1" pad="D2"/>
<contactref element="R18" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="CN1" pad="D1"/>
<contactref element="R17" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="CN1" pad="D0"/>
<contactref element="R16" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="CN1" pad="D4"/>
<contactref element="R20" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="CN1" pad="D5"/>
<contactref element="R21" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="CN1" pad="D6"/>
<contactref element="R22" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="CN1" pad="D7"/>
<contactref element="R23" pad="2"/>
</signal>
<signal name="D0">
<contactref element="IC2" pad="13"/>
<contactref element="R16" pad="1"/>
</signal>
<signal name="D1">
<contactref element="IC2" pad="14"/>
<contactref element="R17" pad="1"/>
</signal>
<signal name="D2">
<contactref element="IC2" pad="15"/>
<contactref element="R18" pad="1"/>
</signal>
<signal name="D3">
<contactref element="IC2" pad="16"/>
<contactref element="R19" pad="1"/>
</signal>
<signal name="D4">
<contactref element="IC2" pad="17"/>
<contactref element="R20" pad="1"/>
</signal>
<signal name="D5">
<contactref element="IC2" pad="18"/>
<contactref element="R21" pad="1"/>
</signal>
<signal name="D6">
<contactref element="IC2" pad="19"/>
<contactref element="R22" pad="1"/>
</signal>
<signal name="D7">
<contactref element="IC2" pad="20"/>
<contactref element="R23" pad="1"/>
</signal>
<signal name="N$22">
<contactref element="CN1" pad="A3"/>
<contactref element="D2" pad="A"/>
</signal>
<signal name="N$23">
<contactref element="CN1" pad="A4"/>
<contactref element="D3" pad="A"/>
</signal>
<signal name="N$24">
<contactref element="CN1" pad="A5"/>
<contactref element="D4" pad="A"/>
</signal>
<signal name="N$26">
<contactref element="CN1" pad="A7"/>
<contactref element="D5" pad="A"/>
</signal>
<signal name="N$27">
<contactref element="D5" pad="C"/>
<contactref element="D2" pad="C"/>
<contactref element="D3" pad="C"/>
<contactref element="D4" pad="C"/>
<contactref element="D1" pad="C"/>
<contactref element="R26" pad="2"/>
<contactref element="R32" pad="2"/>
</signal>
<signal name="N$29">
<contactref element="CN1" pad="A1"/>
<contactref element="R28" pad="2"/>
</signal>
<signal name="N$30">
<contactref element="CN1" pad="A0"/>
<contactref element="R27" pad="2"/>
</signal>
<signal name="N$35">
<contactref element="CN1" pad="!IOREQ!"/>
<contactref element="R25" pad="2"/>
</signal>
<signal name="N$28">
<contactref element="CN1" pad="A2"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="N$31">
<contactref element="CN1" pad="!RD!"/>
<contactref element="R30" pad="2"/>
</signal>
<signal name="N$32">
<contactref element="CN1" pad="!WR!"/>
<contactref element="R29" pad="2"/>
</signal>
<signal name="N$33">
<contactref element="R31" pad="2"/>
<contactref element="CN1" pad="!M1!"/>
</signal>
<signal name="!RD!">
<contactref element="R30" pad="1"/>
<contactref element="IC2" pad="7"/>
</signal>
<signal name="!WR!">
<contactref element="IC2" pad="6"/>
<contactref element="R29" pad="1"/>
</signal>
<signal name="ADDR">
<contactref element="R26" pad="1"/>
<contactref element="IC2" pad="2"/>
</signal>
<signal name="N$25">
<contactref element="CN1" pad="A6"/>
<contactref element="R24" pad="1"/>
</signal>
<signal name="A1">
<contactref element="R28" pad="1"/>
<contactref element="IC2" pad="5"/>
</signal>
<signal name="A0">
<contactref element="R27" pad="1"/>
<contactref element="IC2" pad="4"/>
</signal>
<signal name="!IOREQ!">
<contactref element="IC2" pad="1"/>
<contactref element="R25" pad="1"/>
</signal>
<signal name="A6">
<contactref element="R24" pad="2"/>
<contactref element="IC2" pad="3"/>
</signal>
<signal name="!M1!">
<contactref element="R31" pad="1"/>
<contactref element="IC2" pad="8"/>
</signal>
<signal name="N$43">
<contactref element="CN2" pad="9"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="N$44">
<contactref element="TR1" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="!WAIT!">
<contactref element="TR1" pad="1"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="N$45">
<contactref element="R3" pad="2"/>
<contactref element="IC2" pad="36"/>
</signal>
<signal name="N$46">
<contactref element="JP3" pad="1"/>
<contactref element="R33" pad="2"/>
<contactref element="IC2" pad="33"/>
</signal>
<signal name="N$47">
<contactref element="JP4" pad="1"/>
<contactref element="R34" pad="2"/>
<contactref element="IC2" pad="34"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
