<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.3.0">
<drawing>
<board>
<plain>
<wire x1="-2.54" y1="19.05" x2="23.8" y2="19.05" width="0" layer="20"/>
<wire x1="23.8" y1="19.05" x2="23.8" y2="60.95" width="0" layer="20"/>
<wire x1="23.8" y1="60.95" x2="-2.54" y2="60.95" width="0" layer="20"/>
<wire x1="-2.54" y1="60.95" x2="-2.54" y2="19.05" width="0" layer="20"/>
<text>Charles Dysert
EVG2000</text>
<text>Joystick Y
Version 2.0</text>
<text>Charles Dysert
EVG2000</text>
<text>Joystick Y
Version 2.0</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DB9">
<description>&lt;h3&gt;9 Pin Serial Connector - Female PCB Mount Right Angle&lt;/h3&gt;
0.318" style. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:11&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Connectors/DB9-PCB.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;DB9&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="Headers">
<description>&lt;h3&gt; PCBLayout.com - Frequently Used &lt;i&gt;Headers&lt;/i&gt;&lt;/h3&gt;

Visit us at &lt;a href="http://www.PCBLayout.com"&gt;PCBLayout.com&lt;/a&gt; for quick and hassle-free PCB Layout/Manufacturing ordering experience.
&lt;BR&gt;
&lt;BR&gt;
This library has been generated by our experienced pcb layout engineers using current IPC and/or industry standards. We &lt;b&gt;believe&lt;/b&gt; the content to be accurate, complete and current. But, this content is provided as a courtesy and &lt;u&gt;user assumes all risk and responsiblity of it's usage&lt;/u&gt;.
&lt;BR&gt;
&lt;BR&gt;
Feel free to contact us at &lt;a href="mailto:Support@PCBLayout.com"&gt;Support@PCBLayout.com&lt;/a&gt; if you have any questions/concerns regarding any of our content or services.</description>
<packages>
<package name="61300911121">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JOYSTICK1-IN" library="SparkFun-Connectors" package="DB9" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-08194"/>
<attribute name="VALUE"/>
</element>
<element name="JOYSTICK2-IN" library="SparkFun-Connectors" package="DB9" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-08194"/>
<attribute name="VALUE"/>
</element>
<element name="JOYSTICKOUT" library="Headers" package="61300911121" value="61300911121">
<attribute name="CREATED_BY" value="PCBLayout.com"/>
<attribute name="DIGI_KEY_PART_NUMBER" value="732-5322-ND"/>
<attribute name="MANUFACTURER" value="Wurth Electronics Inc."/>
<attribute name="MPN" value="61300911121"/>
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="JOYSTICKOUT" pad="1"/>
<contactref element="JOYSTICK1-IN" pad="1"/>
<contactref element="JOYSTICK2-IN" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="JOYSTICK1-IN" pad="2"/>
<contactref element="JOYSTICKOUT" pad="2"/>
<contactref element="JOYSTICK2-IN" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="JOYSTICK1-IN" pad="3"/>
<contactref element="JOYSTICKOUT" pad="3"/>
<contactref element="JOYSTICK2-IN" pad="3"/>
</signal>
<signal name="N$7">
<contactref element="JOYSTICK1-IN" pad="4"/>
<contactref element="JOYSTICKOUT" pad="4"/>
<contactref element="JOYSTICK2-IN" pad="4"/>
</signal>
<signal name="N$9">
<contactref element="JOYSTICK1-IN" pad="5"/>
<contactref element="JOYSTICKOUT" pad="5"/>
<contactref element="JOYSTICK2-IN" pad="5"/>
</signal>
<signal name="N$12">
<contactref element="JOYSTICK1-IN" pad="7"/>
<contactref element="JOYSTICKOUT" pad="7"/>
<contactref element="JOYSTICK2-IN" pad="7"/>
</signal>
<signal name="N$14">
<contactref element="JOYSTICK1-IN" pad="8"/>
<contactref element="JOYSTICKOUT" pad="8"/>
<contactref element="JOYSTICK2-IN" pad="8"/>
</signal>
<signal name="N$16">
<contactref element="JOYSTICK1-IN" pad="9"/>
<contactref element="JOYSTICKOUT" pad="9"/>
<contactref element="JOYSTICK2-IN" pad="9"/>
</signal>
<signal name="N$2">
<contactref element="JOYSTICK1-IN" pad="6"/>
<contactref element="JOYSTICKOUT" pad="6"/>
<contactref element="JOYSTICK2-IN" pad="6"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
