<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="20.26" y2="0" width="0" layer="20"/>
<wire x1="20.26" y1="0" x2="20.26" y2="20.39" width="0" layer="20"/>
<wire x1="20.26" y1="20.39" x2="0" y2="20.39" width="0" layer="20"/>
<wire x1="0" y1="20.39" x2="0" y2="0" width="0" layer="20"/>
<text>Henry Fehr</text>
<text>Henry Fehr</text>
<text>12/10/16</text>
<text>12/10/16</text>
<text>REV 3.1</text>
<text>REV 3.1</text>
</plain>
<libraries>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="EIA3216">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="JST-2-SMD">
<description>2mm SMD side-entry connector. tDocu layer indicates the actual physical plastic housing. +/- indicate SparkFun standard batteries and wiring.</description>
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LUXEON">
</package>
</packages>
</library>
<library name="zetex">
<description>&lt;b&gt;Zetex Power MOS FETs, Bridges, Diodes&lt;/b&gt;&lt;p&gt;
http://www.zetex.com&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT89">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun-Capacitors" package="EIA3216" value="10uF">
<attribute name="PROD_ID" value="CAP-00811"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="EIA3216" value="10uF">
<attribute name="PROD_ID" value="CAP-00811"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="JST-2-SMD" value="6V Max">
<attribute name="PROD_ID" value="CONN-11443"/>
<attribute name="TOP_POS" value="+"/>
<attribute name="BTM_NEG" value="-"/>
<attribute name="BTM_POS" value="+"/>
<attribute name="TOP_NEG" value="-"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="SparkFun-LED" package="LUXEON" value="LUXEONSMD"/>
<element name="U$2" library="zetex" package="SOT89" value="L7135">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U$2" pad="2@1"/>
<contactref element="U$1" pad="S"/>
<contactref element="J1" pad="1"/>
<contactref element="C2" pad="C"/>
<contactref element="C1" pad="C"/>
</signal>
<signal name="VCC">
<contactref element="J1" pad="2"/>
<contactref element="U$2" pad="3"/>
<contactref element="U$1" pad="A"/>
<contactref element="C2" pad="A"/>
</signal>
<signal name="N$1">
<contactref element="U$1" pad="C"/>
<contactref element="U$2" pad="1"/>
<contactref element="C1" pad="A"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
