<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="8.89" x2="50.47" y2="8.89" width="0" layer="20"/>
<wire x1="50.47" y1="8.89" x2="50.47" y2="31.74" width="0" layer="20"/>
<wire x1="50.47" y1="31.74" x2="0" y2="31.74" width="0" layer="20"/>
<wire x1="0" y1="31.74" x2="0" y2="8.89" width="0" layer="20"/>
<text>gNerduino</text>
<text>rev1</text>
<text>gnd</text>
<text>gnd</text>
<text>r1 330</text>
<text>r2 330</text>
<text>16mhz</text>
<text>VCC</text>
<text>GND</text>
<text>22pf</text>
<text>22pf</text>
<text>gNerduino r1 - John Z Black</text>
</plain>
<libraries>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Capacitors&lt;/h3&gt;
This library contains capacitors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CAP-PTH-2.54">
<description>2 PTH spaced 0.1" apart</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="HC49/S">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="atmega328p-pu">
<packages>
<package name="DIP254P762X457-28">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X01_OFFSET">
<description>&lt;h3&gt;Plated Through Hole - Long Pad w/ Offset Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:1&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_01&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X01">
<description>&lt;h3&gt;Plated Through Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:1&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_01&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun LEDs&lt;/h3&gt;
This library contains discrete LEDs for illumination or indication, but no displays.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED_3MM">
<description>&lt;h3&gt;LED 3MM PTH&lt;/h3&gt;

3 mm, round.

&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.1inch&lt;/li&gt;
&lt;li&gt;Diameter: 3mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;LED&lt;/li&gt;&lt;/ul&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.3">
<description>&lt;h3&gt;AXIAL-0.3&lt;/h3&gt;
&lt;p&gt;Commonly used for 1/4W through-hole resistors. 0.3" pitch between holes.&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun-Capacitors" package="CAP-PTH-2.54" value="22pF">
<attribute name="PROD_ID" value="CAP-09128"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="CAP-PTH-2.54" value="22pF">
<attribute name="PROD_ID" value="CAP-09128"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="adafruit" package="HC49/S" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="OC_FARNELL" value="1667008"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="atmega328p-pu" package="DIP254P762X457-28" value="">
<attribute name="SUPPLIER" value="Atmel"/>
<attribute name="PACKAGE" value="PDIP-28"/>
<attribute name="MPN" value="ATMEGA328P-PU"/>
<attribute name="OC_NEWARK" value="68T2944"/>
<attribute name="OC_FARNELL" value="1715487"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="VCC" library="SparkFun-Connectors" package="1X01_OFFSET" value="VCC">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X01_OFFSET" value="GND">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D5" library="SparkFun-Connectors" package="1X01" value=""/>
<element name="D6" library="SparkFun-Connectors" package="1X01" value=""/>
<element name="D7" library="SparkFun-Connectors" package="1X01" value=""/>
<element name="D8" library="SparkFun-Connectors" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D9" library="SparkFun-Connectors" package="1X01" value=""/>
<element name="D10" library="SparkFun-Connectors" package="1X01" value=""/>
<element name="D11" library="SparkFun-Connectors" package="1X01" value=""/>
<element name="D12" library="SparkFun-Connectors" package="1X01" value=""/>
<element name="D13" library="SparkFun-LED" package="LED_3MM" value="">
<attribute name="PROD_ID" value="DIO-08794"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="AXIAL-0.3" value="330">
<attribute name="PROD_ID" value="RES-8371"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="AXIAL-0.3" value="330">
<attribute name="PROD_ID" value="RES-8371"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PWR" library="SparkFun-LED" package="LED_3MM" value="">
<attribute name="PROD_ID" value="DIO-08794"/>
</element>
<element name="+" library="SparkFun-Connectors" package="1X01" value="+">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J12" library="SparkFun-Connectors" package="1X01" value="-">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RST" library="SparkFun-Connectors" package="1X01" value=""/>
<element name="RX" library="SparkFun-Connectors" package="1X01" value=""/>
<element name="TX" library="SparkFun-Connectors" package="1X01" value=""/>
<element name="J16" library="SparkFun-Connectors" package="1X01" value="GND">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J17" library="SparkFun-Connectors" package="1X01" value="GND">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J18" library="SparkFun-Connectors" package="1X01" value="GND">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="GND" library="SparkFun-Connectors" package="1X01" value="GND">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="AI4" library="SparkFun-Connectors" package="1X01" value=""/>
<element name="AI3" library="SparkFun-Connectors" package="1X01" value=""/>
<element name="AI1" library="SparkFun-Connectors" package="1X01" value=""/>
<element name="AI2" library="SparkFun-Connectors" package="1X01" value=""/>
<element name="D14" library="SparkFun-Connectors" package="1X01" value=""/>
<element name="AI0" library="SparkFun-Connectors" package="1X01" value=""/>
</elements>
<signals>
<signal name="AVCC">
<contactref element="U1" pad="20"/>
</signal>
<signal name="VCC">
<contactref element="U1" pad="7"/>
<contactref element="VCC" pad="1"/>
<contactref element="R2" pad="P$1"/>
<contactref element="+" pad="1"/>
</signal>
<signal name="GND">
<contactref element="U1" pad="8"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="J2" pad="1"/>
<contactref element="U1" pad="22"/>
<contactref element="D13" pad="K"/>
<contactref element="PWR" pad="K"/>
<contactref element="J12" pad="1"/>
<contactref element="GND" pad="1"/>
<contactref element="J18" pad="1"/>
<contactref element="J16" pad="1"/>
<contactref element="J17" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="U1" pad="10"/>
<contactref element="Q1" pad="1"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="U1" pad="9"/>
<contactref element="Q1" pad="2"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="U1" pad="11"/>
<contactref element="D5" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="U1" pad="12"/>
<contactref element="D6" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="U1" pad="13"/>
<contactref element="D7" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="U1" pad="14"/>
<contactref element="D8" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="U1" pad="15"/>
<contactref element="D9" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="U1" pad="16"/>
<contactref element="D10" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="U1" pad="17"/>
<contactref element="D11" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="U1" pad="18"/>
<contactref element="D12" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="U1" pad="19"/>
<contactref element="R1" pad="P$1"/>
</signal>
<signal name="N$13">
<contactref element="D13" pad="A"/>
<contactref element="R1" pad="P$2"/>
</signal>
<signal name="N$14">
<contactref element="R2" pad="P$2"/>
<contactref element="PWR" pad="A"/>
</signal>
<signal name="N$15">
<contactref element="U1" pad="1"/>
<contactref element="RST" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="RX" pad="1"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="N$17">
<contactref element="U1" pad="3"/>
<contactref element="TX" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="U1" pad="28"/>
<contactref element="D14" pad="1"/>
</signal>
<signal name="N$18">
<contactref element="U1" pad="27"/>
<contactref element="AI4" pad="1"/>
</signal>
<signal name="N$20">
<contactref element="U1" pad="26"/>
<contactref element="AI3" pad="1"/>
</signal>
<signal name="N$21">
<contactref element="U1" pad="25"/>
<contactref element="AI2" pad="1"/>
</signal>
<signal name="N$19">
<contactref element="U1" pad="24"/>
<contactref element="AI1" pad="1"/>
</signal>
<signal name="N$22">
<contactref element="U1" pad="23"/>
<contactref element="AI0" pad="1"/>
</signal>
<signal name="N$23">
</signal>
</signals>
</board>
</drawing>
</eagle>
