<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="6.457" y2="0" width="0" layer="20"/>
<wire x1="6.457" y1="0" x2="6.457" y2="6.528" width="0" layer="20"/>
<wire x1="6.457" y1="6.528" x2="0" y2="6.528" width="0" layer="20"/>
<wire x1="0" y1="6.528" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X01">
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="CHIPLED_0603">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_LY Q971.pdf</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="ANODE1" library="SparkFun-Connectors" package="1X01" value="M01PTH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="ANODE2" library="SparkFun-Connectors" package="1X01" value="M01PTH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CATHODE1" library="SparkFun-Connectors" package="1X01" value="M01PTH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CATHODE2" library="SparkFun-Connectors" package="1X01" value="M01PTH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="led" package="CHIPLED_0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="ANODE1" pad="1"/>
<contactref element="LED1" pad="A"/>
<contactref element="ANODE2" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="CATHODE1" pad="1"/>
<contactref element="LED1" pad="C"/>
<contactref element="CATHODE2" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
