<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="5" y1="0" x2="58.4" y2="0" width="0" layer="20"/>
<wire x1="58.4" y1="0" x2="58.329584375" y2="49.984078125" width="0" layer="20"/>
<wire x1="0" y1="45" x2="0" y2="5" width="0" layer="20"/>
<wire x1="0" y1="5" x2="5" y2="0" width="0.001" layer="20" curve="90"/>
<wire x1="5" y1="50" x2="0" y2="45" width="0.001" layer="20" curve="90"/>
<wire x1="4.93936875" y1="49.999778125" x2="58.32940625" y2="49.98380625" width="0.0001" layer="20"/>
<hole x="5" y="5" drill="3.2"/>
<hole x="5" y="45" drill="3.2"/>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="1X01-CLEANBIG">
</package>
</packages>
</library>
<library name="Connector">
<packages>
<package name="4P-2.0-90D">
</package>
</packages>
</library>
<library name="Particle-Devices">
<description>&lt;h3&gt;Reference foot prints for Particle devices&lt;/h3&gt;
In this library you'll find foot prints to make circuit boards using the Particle devices: Spark Core, Photon and Electron.&lt;br&gt;&lt;br&gt;
There are for reference and you may need to adjust them for your application. See https://docs.particle.io for more details on the recommended layouts for Particle devices.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Designed by Particle. Distributed under a Creative Commons Attribution, Share-Alike license. Development kits based on this library should be distributed under a similar license. Commercial products using this library as a reference design need not comply with this license; further questions can be sent to hello@particle.io. Check license.txt for more information.</description>
<packages>
<package name="ARGON">
<description>&lt;b&gt;ARGON&lt;/b&gt;&lt;p&gt;

Footprint and formfactor based on &lt;a href="https://www.adafruit.com/feather"&gt;Adafruit Feather.&lt;/a&gt;&lt;br&gt;
More information: &lt;a href="https://docs.particle.io/argon/"&gt;https://docs.particle.io/argon/&lt;/a&gt;&lt;/p&gt;
Please pay attention to the keepout areas under the antenna to get good RF performance.</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X06_2.54MM_SCREWPIN">
<description>&lt;h3&gt;Plated Through Hole - 6 Pin No Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="Connector" package="4P-2.0-90D" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="Connector" package="4P-2.0-90D" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="adafruit" package="1X01-CLEANBIG" value="">
<attribute name="VALUE"/>
</element>
<element name="U1" library="Particle-Devices" package="ARGON" value="ARGON"/>
<element name="J3" library="SparkFun-Connectors" package="1X06_2.54MM_SCREWPIN" value="">
<attribute name="PROD_ID" value="CONN-14885"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U1" pad="4"/>
<contactref element="J1" pad="4"/>
<contactref element="J2" pad="4"/>
<contactref element="J3" pad="6"/>
</signal>
<signal name="VCC">
<contactref element="U1" pad="26"/>
<contactref element="J2" pad="3"/>
<contactref element="J3" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="J1" pad="2"/>
<contactref element="U1" pad="17"/>
</signal>
<signal name="N$6">
<contactref element="U1" pad="18"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="U1" pad="19"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="U1" pad="21"/>
<contactref element="J3" pad="4"/>
</signal>
<signal name="N$3">
<contactref element="U1" pad="20"/>
<contactref element="J3" pad="5"/>
</signal>
<signal name="N$7">
<contactref element="J2" pad="1"/>
<contactref element="U1" pad="5"/>
</signal>
<signal name="N$8">
<contactref element="U1" pad="11"/>
<contactref element="J3" pad="3"/>
</signal>
<signal name="LI+">
<contactref element="U1" pad="28"/>
</signal>
<signal name="N$4">
<contactref element="U1" pad="13"/>
<contactref element="J3" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="J1" pad="3"/>
<contactref element="U1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
