<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.0.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="36.195" y2="0" width="0" layer="20"/>
<wire x1="36.195" y1="0" x2="36.195" y2="21.59" width="0" layer="20"/>
<wire x1="36.195" y1="21.59" x2="0" y2="21.59" width="0" layer="20"/>
<wire x1="0" y1="21.59" x2="0" y2="0" width="0" layer="20"/>
<hole x="2.54" y="2.54" drill="2.8"/>
<hole x="33.655" y="19.05" drill="2.8"/>
<text>MONOLITH</text>
<text>MAIN</text>
<text>REV 1.0.0</text>
<text>20170210</text>
<text>COREY HOARD</text>
<text>CHILD BOARD</text>
<text>G</text>
<text>R</text>
</plain>
<libraries>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Aesthetics&lt;/h3&gt;
This library contiains non-functional items such as logos, build/ordering notes, frame blocks, etc. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CREATIVE_COMMONS">
<description>&lt;h3&gt;Creative Commons License Template&lt;/h3&gt;
&lt;p&gt;CC BY-SA 4.0 License with &lt;a href="https://creativecommons.org/licenses/by-sa/4.0/"&gt;link to license&lt;/a&gt; and placeholder for designer name.&lt;/p&gt;
&lt;p&gt;Devices using:
&lt;ul&gt;&lt;li&gt;FRAME_LEDGER&lt;/li&gt;
&lt;li&gt;FRAME_LETTER&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X3-SHROUDED">
<description>&lt;h3&gt;Plated Through Hole - 2x3 Shrouded Header&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Shrouded-10pin.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Switches">
<description>&lt;h3&gt;SparkFun Switches, Buttons, Encoders&lt;/h3&gt;
In this library you'll find switches, buttons, joysticks, and anything that moves to create or disrupt an electrical connection.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="ENCODER_LED_2">
<description>&lt;h3&gt;Illuminated Rotary Encoder w/ 2 LEDs&lt;/h3&gt;
&lt;p&gt;Rotary encoders rotate similarly to potentiometers, but they’re different from potentiometers in that an encoder has full rotation without limits. They output gray code so that you can tell how much and in which direction the encoder has been turned.&lt;/p&gt;
&lt;p&gt;This encoder has a red/green LED built-in, which shines through the encoder shaft.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://cdn.sparkfun.com/datasheets/Components/LED/EC12PLRVF-D-24K-24-24C-0206-6H%28SPEC%29.pdf"&gt;Datasheet&lt;/a&gt; (EC12PLGRSDVF-D-25K-24-32/07-6H)&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Capacitors&lt;/h3&gt;
This library contains capacitors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CAP-PTH-SMALL-KIT">
<description>&lt;h3&gt;CAP-PTH-SMALL-KIT&lt;/h3&gt;
Commonly used for small ceramic capacitors. Like our 0.1uF (http://www.sparkfun.com/products/8375) or 22pF caps (http://www.sparkfun.com/products/8571).&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Warning:&lt;/b&gt; This is the KIT version of this package. This package has a smaller diameter top stop mask, which doesn't cover the diameter of the pad. This means only the bottom side of the pads' copper will be exposed. You'll only be able to solder to the bottom side.</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="0207/2V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 2.5 mm</description>
</package>
</packages>
</library>
<library name="SparkFun-Jumpers">
<description>&lt;h3&gt;SparkFun Jumpers&lt;/h3&gt;
In this library you'll find jumpers, or other semipermanent means of changing current paths. The least permanent form is the solder jumper. These can be changed by adding, removing, or moving solder. In cases that are less likely to be changed we have jumpers that are connected with traces. These can be cut with a razor, or reconnected with solder. Reference designator JP.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SMT-JUMPER_3_NO_SILK">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="FRAME1" library="SparkFun-Aesthetics" package="CREATIVE_COMMONS" value="FRAME-LETTER"/>
<element name="MAIN" library="SparkFun-Connectors" package="2X3-SHROUDED" value="">
<attribute name="SF_ID" value="PRT_10877"/>
<attribute name="PROD_ID" value="CONN-10681"/>
<attribute name="VALUE"/>
</element>
<element name="S2" library="SparkFun-Switches" package="ENCODER_LED_2" value="ENCODER-2LED">
<attribute name="SF_SKU" value="COM-10596"/>
<attribute name="PROD_ID" value="COMP-11113"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="CAP-PTH-SMALL-KIT" value="0.1uF">
<attribute name="PROD_ID" value="CAP-08370"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="CAP-PTH-SMALL-KIT" value="0.1uF">
<attribute name="PROD_ID" value="CAP-08370"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="CAP-PTH-SMALL-KIT" value="0.1uF">
<attribute name="PROD_ID" value="CAP-08370"/>
</element>
<element name="R1" library="adafruit" package="0207/2V" value="10k">
<attribute name="VALUE"/>
</element>
<element name="R2" library="adafruit" package="0207/2V" value="330">
<attribute name="VALUE"/>
</element>
<element name="R3" library="adafruit" package="0207/2V" value="330">
<attribute name="VALUE"/>
</element>
<element name="R4" library="adafruit" package="0207/2V" value="10k">
<attribute name="VALUE"/>
</element>
<element name="R5" library="adafruit" package="0207/2V" value="10k">
<attribute name="VALUE"/>
</element>
<element name="R6" library="adafruit" package="0207/2V" value="330">
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun-Jumpers" package="SMT-JUMPER_3_NO_SILK" value="JUMPER-SMT_3_NO_SILK">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="ENC_A">
<contactref element="MAIN" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="ENC_B">
<contactref element="MAIN" pad="3"/>
<contactref element="R3" pad="1"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="ENC_S">
<contactref element="MAIN" pad="5"/>
<contactref element="C3" pad="1"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="AUX">
<contactref element="MAIN" pad="4"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="+3V3">
<contactref element="MAIN" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="GND">
<contactref element="MAIN" pad="6"/>
<contactref element="S2" pad="C"/>
<contactref element="S2" pad="GND"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="R2" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="S2" pad="A"/>
</signal>
<signal name="N$3">
<contactref element="S2" pad="B"/>
<contactref element="R3" pad="2"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="R5" pad="1"/>
<contactref element="S2" pad="SW"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="LED_R">
<contactref element="S2" pad="+R"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="LED_G">
<contactref element="S2" pad="+G"/>
<contactref element="JP1" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
