<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="45" y1="32" x2="3" y2="32" width="0" layer="20"/>
<wire x1="3" y1="32" x2="0" y2="29" width="0" layer="20" curve="90"/>
<wire x1="0" y1="29" x2="0" y2="-58" width="0" layer="20"/>
<wire x1="0" y1="-58" x2="3" y2="-61" width="0" layer="20" curve="90"/>
<wire x1="3" y1="-61" x2="45" y2="-61" width="0" layer="20"/>
<wire x1="45" y1="-61" x2="48" y2="-58" width="0" layer="20" curve="90"/>
<wire x1="48" y1="-58" x2="48" y2="29" width="0" layer="20"/>
<wire x1="48" y1="29" x2="45" y2="32" width="0" layer="20" curve="90"/>
<text>Lesser sooty owl</text>
</plain>
<libraries>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-CAP">
</package>
</packages>
</library>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-RES">
</package>
</packages>
</library>
<library name="odroid-u3">
<packages>
<package name="U3V05">
<description>ODROID U3 v0.5 outline and I/O</description>
</package>
<package name="SOT223">
<description>&lt;b&gt;Smal Outline Transistor&lt;/b&gt;</description>
</package>
<package name="SO14">
</package>
</packages>
</library>
<library name="con-harting-ml">
<description>&lt;b&gt;Harting  &amp; 3M Connectors&lt;/b&gt;&lt;p&gt;
Low profile connectors, straight&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="ML26">
<description>&lt;b&gt;HARTING&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun-Capacitors" package="0603-CAP" value="0.1uF">
<attribute name="PROD_ID" value="CAP-00810"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0603-CAP" value="0.1uF">
<attribute name="PROD_ID" value="CAP-00810"/>
</element>
<element name="U1" library="odroid-u3" package="SO14" value="TXB0104">
<attribute name="PROD_ID" value="IC-11329"/>
</element>
<element name="SV1" library="con-harting-ml" package="ML26" value="7i90">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="R1" library="SparkFun" package="0603-RES" value="82"/>
<element name="C3" library="SparkFun-Capacitors" package="0603-CAP" value="0.1uF">
<attribute name="PROD_ID" value="CAP-00810"/>
</element>
<element name="R2" library="SparkFun" package="0603-RES" value="82"/>
<element name="R3" library="SparkFun" package="0603-RES" value="82"/>
<element name="U$4" library="odroid-u3" package="U3V05" value="ODROID-U3"/>
<element name="IC2" library="odroid-u3" package="SOT223" value="REG1117-3.3">
<attribute name="OC_NEWARK" value="14P6981"/>
<attribute name="MPN" value="REG1117"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1097566"/>
</element>
</elements>
<signals>
<signal name="CLK_A">
<contactref element="U1" pad="5"/>
<contactref element="U$4" pad="P$1"/>
</signal>
<signal name="MOSI_A">
<contactref element="U1" pad="4"/>
<contactref element="U$4" pad="P$3"/>
</signal>
<signal name="MISO_A">
<contactref element="U1" pad="3"/>
<contactref element="U$4" pad="P$4"/>
</signal>
<signal name="CSN_A">
<contactref element="U1" pad="2"/>
<contactref element="U$4" pad="P$2"/>
</signal>
<signal name="GND">
<contactref element="U1" pad="7"/>
<contactref element="SV1" pad="10"/>
<contactref element="SV1" pad="12"/>
<contactref element="SV1" pad="14"/>
<contactref element="SV1" pad="16"/>
<contactref element="SV1" pad="18"/>
<contactref element="SV1" pad="20"/>
<contactref element="SV1" pad="22"/>
<contactref element="SV1" pad="24"/>
<contactref element="C3" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="U$4" pad="P$11"/>
<contactref element="IC2" pad="1"/>
</signal>
<signal name="1.8V">
<contactref element="U1" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="U1" pad="8"/>
<contactref element="U$4" pad="P$6"/>
</signal>
<signal name="5V">
<contactref element="C2" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="U$4" pad="P$12"/>
<contactref element="IC2" pad="3"/>
</signal>
<signal name="MOSI_B">
<contactref element="SV1" pad="13"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="MISO_B">
<contactref element="SV1" pad="15"/>
<contactref element="U1" pad="12"/>
</signal>
<signal name="CSN_B">
<contactref element="SV1" pad="17"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="CLK_B">
<contactref element="SV1" pad="11"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="U1" pad="10"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="3.3V">
<contactref element="C3" pad="1"/>
<contactref element="U1" pad="14"/>
<contactref element="IC2" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="R3" pad="1"/>
<contactref element="U1" pad="13"/>
</signal>
<signal name="N$3">
<contactref element="U1" pad="11"/>
<contactref element="R2" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
