<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="2.54" y1="-0.254" x2="45.72" y2="-0.254" width="0" layer="20"/>
<text>USB Line Voltage Inducer</text>
<text>v1.8
1/1/2017</text>
<text>CT-220/330pF
C0-4.7/6.8uF
L-100/82uH</text>
<wire x1="48.26" y1="2.286" x2="48.26" y2="31.75" width="0" layer="20"/>
<wire x1="45.72" y1="34.29" x2="2.54" y2="34.29" width="0" layer="20"/>
<wire x1="0" y1="31.75" x2="0" y2="2.286" width="0" layer="20"/>
<wire x1="0" y1="2.286" x2="2.54" y2="-0.254" width="0" layer="20" curve="90"/>
<wire x1="0" y1="31.75" x2="2.54" y2="34.29" width="0" layer="20" curve="-90"/>
<wire x1="48.26" y1="31.75" x2="45.72" y2="34.29" width="0" layer="20" curve="90"/>
<wire x1="45.72" y1="-0.254" x2="48.26" y2="2.286" width="0" layer="20" curve="90"/>
<text>9v/18v</text>
<text>RSC-1.5/0.68ohm
R1-1K/5.6Kohm
R2-6.2K/75Kohm</text>
</plain>
<libraries>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CAP-PTH-SMALL">
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DIODE-1N4148">
</package>
</packages>
</library>
<library name="#mine">
<packages>
<package name="6P6C_JACK">
<description>Footprint for a 6P6C jack</description>
</package>
<package name="USB_VERT">
<description>Footprint for a vertical USB mount, based on Amphenol FCI's 73725-0110BLF.</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="RLB0912">
</package>
<package name="AXIAL-0.4">
<description>1/4W Resistor, 0.4" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.3">
<description>&lt;h3&gt;AXIAL-0.3&lt;/h3&gt;
&lt;p&gt;Commonly used for 1/4W through-hole resistors. 0.3" pitch between holes.&lt;/p&gt;</description>
</package>
<package name="AXIAL-0.5">
<description>1/2W Resistor, 0.5" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
</packages>
</library>
<library name="CEDTv77">
<description>&lt;b&gt;Center for Electronics Design and Technology&lt;/b&gt;&lt;br&gt;
at&lt;br&gt;
Netaji Subhas Institute of Technology&lt;br&gt;
Dwarka,&lt;br&gt;
New Delhi, India&lt;br&gt;
&lt;br&gt;
Data Modified : 18-July-2013&lt;br&gt;
&lt;br&gt;
CEDT is Managed by Dhananjay V. Gadre (dvgadre@gmail.com)&lt;br&gt;&lt;br&gt;
&lt;br&gt;
Get the latest version from &lt;a href="https://github.com/IndianTinker/CEDT-EagleLibrary"&gt;here&lt;/a&gt;
&lt;br&gt;&lt;br&gt;
&lt;author&gt;This library was created by Anurag Chugh, Rohit Dureja and Shanjit Singh Jajmann&lt;/author&gt;</description>
<packages>
<package name="DIL8">
<description>&lt;B&gt;Dual In Line&lt;/B&gt;&lt;p&gt;
package type P</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C0" library="SparkFun-Capacitors" package="CAP-PTH-SMALL" value="4.7UF / 6.8UF">
<attribute name="NAME"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="CAP-PTH-SMALL" value="100UF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="CAP-PTH-SMALL" value="0.47UF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CT" library="SparkFun-Capacitors" package="CAP-PTH-SMALL" value="220PF / 330PF">
<attribute name="NAME"/>
</element>
<element name="D1" library="SparkFun-DiscreteSemi" package="DIODE-1N4148" value="1N4148">
<attribute name="PROD_ID" value="DIO-08378"/>
<attribute name="NAME"/>
</element>
<element name="J1" library="#mine" package="6P6C_JACK" value="SS-6466S-A-PG1DIP">
<attribute name="NAME"/>
</element>
<element name="J2" library="#mine" package="6P6C_JACK" value="SS-6466S-A-PG1DIP">
<attribute name="NAME"/>
</element>
<element name="J3" library="#mine" package="USB_VERT" value="USB">
<attribute name="NAME"/>
</element>
<element name="L" library="SparkFun-Passives" package="RLB0912" value="100UH / 82UH">
<attribute name="NAME"/>
</element>
<element name="R" library="SparkFun-Resistors" package="AXIAL-0.3" value="180OHM">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Passives" package="AXIAL-0.4" value="1K OHM / 5.6K OHM">
<attribute name="NAME"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="AXIAL-0.3" value="6.2K OHM / 75K OHM">
<attribute name="NAME"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="AXIAL-0.3" value="330OHM">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RSC" library="SparkFun-Resistors" package="AXIAL-0.5" value="1.5OHM / 0.68OHM">
<attribute name="NAME"/>
</element>
<element name="U$1" library="CEDTv77" package="DIL8" value="U1">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$5">
<contactref element="CT" pad="2"/>
<contactref element="R1" pad="P$1"/>
<contactref element="C0" pad="2"/>
<contactref element="R3" pad="P$2"/>
<contactref element="J3" pad="PIN4"/>
<contactref element="C1" pad="2"/>
<contactref element="U$1" pad="2"/>
<contactref element="U$1" pad="4"/>
</signal>
<signal name="N$6">
<contactref element="C1" pad="1"/>
<contactref element="RSC" pad="P$1"/>
<contactref element="J3" pad="PIN1"/>
<contactref element="U$1" pad="6"/>
</signal>
<signal name="N$8">
<contactref element="U$1" pad="7"/>
<contactref element="RSC" pad="P$2"/>
<contactref element="R" pad="P$1"/>
<contactref element="L" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="U$1" pad="8"/>
<contactref element="R" pad="P$2"/>
</signal>
<signal name="N$9">
<contactref element="L" pad="1"/>
<contactref element="U$1" pad="1"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="N$11">
<contactref element="CT" pad="1"/>
<contactref element="U$1" pad="3"/>
</signal>
<signal name="N$13">
<contactref element="U$1" pad="5"/>
<contactref element="R1" pad="P$2"/>
<contactref element="R2" pad="P$2"/>
</signal>
<signal name="N$14">
<contactref element="R2" pad="P$1"/>
<contactref element="C0" pad="1"/>
<contactref element="D1" pad="C"/>
<contactref element="C2" pad="2"/>
<contactref element="J1" pad="PIN3"/>
</signal>
<signal name="N$4">
<contactref element="C2" pad="1"/>
<contactref element="R3" pad="P$1"/>
<contactref element="J2" pad="PIN3"/>
</signal>
<signal name="N$1">
<contactref element="J2" pad="PIN2"/>
<contactref element="J1" pad="PIN2"/>
</signal>
<signal name="N$2">
<contactref element="J2" pad="PIN1"/>
<contactref element="J1" pad="PIN1"/>
</signal>
<signal name="N$3">
<contactref element="J1" pad="PIN4"/>
<contactref element="J2" pad="PIN4"/>
</signal>
<signal name="N$10">
<contactref element="J1" pad="PIN5"/>
<contactref element="J2" pad="PIN5"/>
</signal>
<signal name="N$12">
<contactref element="J2" pad="PIN6"/>
<contactref element="J1" pad="PIN6"/>
</signal>
<signal name="S$1">
</signal>
<signal name="S$2">
</signal>
<signal name="S$3">
</signal>
<signal name="S$4">
</signal>
</signals>
</board>
</drawing>
</eagle>
