<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="15.164" y2="0" width="0" layer="20"/>
<wire x1="15.164" y1="0" x2="15.164" y2="10.912" width="0" layer="20"/>
<wire x1="15.164" y1="10.912" x2="0" y2="10.912" width="0" layer="20"/>
<wire x1="0" y1="10.912" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SO08">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt; Fits JEDEC packages (narrow SOIC-8)</description>
</package>
</packages>
</library>
<library name="aaronMiratron">
<packages>
<package name="M1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.25 W</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X03_LONGPADS">
</package>
<package name="1X06_NO_SILK_YES_STOP">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1206">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="SparkFun-DigitalIC" package="SO08" value="TJA1040">
<attribute name="NAME"/>
</element>
<element name="R1" library="aaronMiratron" package="M1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Passives" package="1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X03_LONGPADS" value="">
<attribute name="VALUE"/>
</element>
<element name="J4" library="SparkFun-Connectors" package="1X06_NO_SILK_YES_STOP" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="RD1">
<contactref element="U$1" pad="4"/>
<contactref element="J4" pad="5"/>
</signal>
<signal name="TD1">
<contactref element="U$1" pad="1"/>
<contactref element="J4" pad="4"/>
</signal>
<signal name="GND">
<contactref element="C1" pad="2"/>
<contactref element="U$1" pad="2"/>
<contactref element="J2" pad="3"/>
<contactref element="J4" pad="6"/>
</signal>
<signal name="+3V3">
<contactref element="C1" pad="1"/>
<contactref element="U$1" pad="3"/>
<contactref element="J4" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="R1" pad="1"/>
<contactref element="J2" pad="2"/>
<contactref element="U$1" pad="6"/>
</signal>
<signal name="N$2">
<contactref element="U$1" pad="7"/>
<contactref element="J2" pad="1"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$3">
</signal>
<signal name="N$4">
</signal>
</signals>
</board>
</drawing>
</eagle>
