<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="-93.98" y1="0" x2="93.98" y2="0" width="0" layer="20"/>
<wire x1="93.98" y1="0" x2="93.98" y2="123.698" width="0" layer="20"/>
<wire x1="93.98" y1="123.698" x2="-93.98" y2="123.698" width="0" layer="20"/>
<wire x1="-93.98" y1="123.698" x2="-93.98" y2="0" width="0" layer="20"/>
<text>PMT2</text>
<text>PMT1</text>
<text>Vctl
(Gain)</text>
<text>Vctl
(Gain)</text>
<text>TTL
HV CTL</text>
<text>Trip
Reset</text>
<text>Power</text>
<text>HV On</text>
<text>Tripped</text>
<text>L</text>
<text>N</text>
<text>E</text>
<text>LINE 
VOLTAGE!</text>
<text>POWER SUPPLY
ON BOTTOM</text>
<text>GROUND</text>
<text>PMT CONTROLLER</text>
<text>J002028REVC</text>
<text>S</text>
<text>S</text>
<text>LEVEL</text>
<text>LEVEL</text>
<text>DELAY</text>
<text>DELAY</text>
<text>TRIP I/O</text>
<text>MANUAL</text>
<text>EXT</text>
<text>PMT1 GAIN</text>
<text>PMT1 IN</text>
<text>PMT2 IN</text>
<text>HV CNTRL</text>
<text>PMT2 GAIN</text>
<text>20160622</text>
</plain>
<libraries>
<library name="STEVES_BU">
<packages>
<package name="TO220V">
</package>
<package name="1206S">
</package>
<package name="0805S">
</package>
<package name="1045_TESTPOINT">
</package>
<package name="SWITCH_7000_SPDT_VRA">
</package>
<package name="SWITCH_NKK_MS_DPDT40">
</package>
<package name="ACOPIAN_ES-10">
</package>
<package name="POT_BOURNS3590">
</package>
<package name="SO-16">
</package>
<package name="SWITCH-3PDT-VRA">
</package>
<package name="LED-TRI-DIA-540-0X00">
</package>
<package name="HEATSINK-7019B-MTG">
</package>
<package name="3362M">
</package>
<package name="DUAL-BNC">
</package>
<package name="LOGO_JANELIA_2014">
</package>
</packages>
</library>
<library name="heatsink">
<description>&lt;b&gt;Heatsinks&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SK129-HOLE">
<description>&lt;b&gt;HEATSINK&lt;/b&gt;&lt;p&gt; manufacturer Fischer/distributor Buerklin</description>
</package>
</packages>
</library>
<library name="linear">
<description>&lt;b&gt;Linear Devices&lt;/b&gt;&lt;p&gt;
Operational amplifiers,  comparators, voltage regulators, ADCs, DACs, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SO08">
<description>&lt;b&gt;Small Outline Package 8&lt;/b&gt;&lt;br&gt;
NS Package M08A</description>
</package>
</packages>
</library>
<library name="74xx-us">
<description>&lt;b&gt;TTL Devices, 74xx Series with US Symbols&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Texas Instruments &lt;i&gt;TTL Data Book&lt;/i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;Volume 1, 1996.
&lt;li&gt;TTL Data Book, Volume 2 , 1993
&lt;li&gt;National Seminconductor Databook 1990, ALS/LS Logic
&lt;li&gt;ttl 74er digital data dictionary, ECA Electronic + Acustic GmbH, ISBN 3-88109-032-0
&lt;li&gt;http://icmaster.com/ViewCompare.asp
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SO16">
<description>&lt;b&gt;Small Outline package&lt;/b&gt; 150 mil</description>
</package>
</packages>
</library>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X12">
</package>
<package name="BNC">
<description>Fits Mouser Part#5227161</description>
</package>
</packages>
</library>
<library name="74xx-little-us">
<description>&lt;b&gt;Single and Dual Gates Family, US symbols&lt;/b&gt;&lt;p&gt;
Little logic devices from Texas Instruments&lt;br&gt;
TinyLogic(R) from FAIRCHILD Semiconductor TM
&lt;p&gt;
&lt;author&gt;Created by evgeni@eniks.com&lt;/author&gt;&lt;br&gt;
&lt;author&gt;Extended by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;&lt;p&gt;
SOT753 - Philips Semiconductors&lt;br&gt;
Source: http://www.semiconductors.philips.com/acrobat_download/datasheets/74HC_HCT1G66_3.pdf</description>
</package>
</packages>
</library>
<library name="74xx-little-de">
<description>&lt;b&gt;Single and Dual Gates Family, US symbols&lt;/b&gt;&lt;p&gt;
Little logic devices from Texas Instruments&lt;br&gt;
TinyLogic(R) from FAIRCHILD Semiconductor TM
&lt;p&gt;
&lt;author&gt;Created by evgeni@eniks.com&lt;/author&gt;&lt;br&gt;
&lt;author&gt;Extended by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;&lt;p&gt;
SOT753 - Philips Semiconductors&lt;br&gt;
Source: http://www.semiconductors.philips.com/acrobat_download/datasheets/74HC_HCT1G66_3.pdf</description>
</package>
</packages>
</library>
<library name="optocoupler">
<description>&lt;b&gt;Opto Couplers&lt;/b&gt;&lt;p&gt;
Siemens, Hewlett-Packard, Texas Instuments, Sharp, Motorola&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SMD4">
<description>&lt;b&gt;SMD 4&lt;/b&gt;&lt;p&gt;
Source: http://www.vishay.com/docs/83673/sfh618.pdf</description>
</package>
</packages>
</library>
<library name="wirepad">
<description>&lt;b&gt;Single Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="4,16O1,6">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X04">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-xmultipleA">
<description>&lt;b&gt;XMULTIPLE&lt;/b&gt; Connector&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="XRJK-S-01-6-4-0-9M2">
<description>&lt;b&gt;RJ11 Connector&lt;/b&gt; without LED, 6 position, 4 contacts, shielded, thrue hole&lt;p&gt;
Source: XRJK-S-01-6-4-0-9M2(01).pdf</description>
</package>
</packages>
</library>
<library name="pinheadA">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X02">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="diode">
<description>&lt;b&gt;Diodes&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola : www.onsemi.com
&lt;li&gt;Fairchild : www.fairchildsemi.com
&lt;li&gt;Philips : www.semiconductors.com
&lt;li&gt;Vishay : www.vishay.de
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23">
<description>&lt;B&gt;DIODE&lt;/B&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U5" library="STEVES_BU" package="TO220V" value="LM314-5">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U7" library="STEVES_BU" package="TO220V" value="LM314-15">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="HS2" library="heatsink" package="SK129-HOLE" value="FA-T220-25E">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="STEVES_BU" package="1206S" value="10uF/35V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="STEVES_BU" package="1206S" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="STEVES_BU" package="0805S" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="STEVES_BU" package="0805S" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="STEVES_BU" package="0805S" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="STEVES_BU" package="0805S" value="2K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="STEVES_BU" package="0805S" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="STEVES_BU" package="0805S" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="STEVES_BU" package="0805S" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="STEVES_BU" package="0805S" value="2K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="STEVES_BU" package="0805S" value="2K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="STEVES_BU" package="0805S" value="20K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="STEVES_BU" package="0805S" value="500pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="STEVES_BU" package="0805S" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="STEVES_BU" package="0805S" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="STEVES_BU" package="0805S" value="500pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="STEVES_BU" package="0805S" value="47pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="STEVES_BU" package="3362M" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="STEVES_BU" package="3362M" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="P5" library="STEVES_BU" package="1045_TESTPOINT" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="P1" library="STEVES_BU" package="1045_TESTPOINT" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="STEVES_BU" package="3362M" value="20K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="STEVES_BU" package="3362M" value="20K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="STEVES_BU" package="0805S" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="STEVES_BU" package="0805S" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U6" library="74xx-us" package="SO16" value="74123D">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="U9" library="74xx-us" package="SO16" value="74279D">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="R26" library="STEVES_BU" package="0805S" value="2K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S100" library="STEVES_BU" package="SWITCH_7000_SPDT_VRA" value="7108P3CWAV2QE">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R19" library="STEVES_BU" package="0805S" value="20K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R25" library="STEVES_BU" package="0805S" value="20K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S104" library="STEVES_BU" package="SWITCH_NKK_MS_DPDT40" value="7201P3CWAV2SE">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PS100" library="STEVES_BU" package="ACOPIAN_ES-10" value="19E40">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J101" library="con-xmultipleA" package="XRJK-S-01-6-4-0-9M2" value="XRJK-S-01-6-4-0-9M2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J100" library="con-xmultipleA" package="XRJK-S-01-6-4-0-9M2" value="XRJK-S-01-6-4-0-9M2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R23" library="STEVES_BU" package="0805S" value="16.9K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R24" library="STEVES_BU" package="0805S" value="16.9K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C20" library="STEVES_BU" package="0805S" value="1uF/35V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C19" library="STEVES_BU" package="0805S" value="1uF/35V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R29" library="STEVES_BU" package="POT_BOURNS3590" value="50K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R28" library="STEVES_BU" package="POT_BOURNS3590" value="50K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U11" library="linear" package="SO08" value="TS922">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U10" library="STEVES_BU" package="SO-16" value="ADG436">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S103" library="STEVES_BU" package="SWITCH-3PDT-VRA" value="M2032S2A2W40">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S101" library="STEVES_BU" package="SWITCH-3PDT-VRA" value="M2032S2A2W40">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="P3" library="STEVES_BU" package="1045_TESTPOINT" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D100" library="STEVES_BU" package="LED-TRI-DIA-540-0X00" value="564-0200-132F">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R17" library="STEVES_BU" package="0805S" value="2K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R27" library="STEVES_BU" package="0805S" value="2K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U3" library="74xx-little-us" package="SOT23-5" value="74AHC1G02DBV">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U8" library="74xx-little-de" package="SOT23-5" value="74AHC1G08DBV">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="P2" library="STEVES_BU" package="1045_TESTPOINT" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="P4" library="STEVES_BU" package="1045_TESTPOINT" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="STEVES_BU" package="0805S" value="0.1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C21" library="STEVES_BU" package="0805S" value="0.1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C18" library="STEVES_BU" package="0805S" value="0.1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C17" library="STEVES_BU" package="0805S" value="0.1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="linear" package="SO08" value="TLC3702">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="linear" package="SO08" value="TLC3702">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="STEVES_BU" package="1206S" value="10uF/35V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="STEVES_BU" package="1206S" value="10uF/35V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C16" library="STEVES_BU" package="0805S" value="0.1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="STEVES_BU" package="0805S" value="0.1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="STEVES_BU" package="0805S" value="0.1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="STEVES_BU" package="0805S" value="0.1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PAD2" library="wirepad" package="4,16O1,6" value="NEUTRAL">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PAD1" library="wirepad" package="4,16O1,6" value="LINE">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PAD3" library="wirepad" package="4,16O1,6" value="WIREPAD4,16O1,6">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP3" library="pinhead" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="HS1" library="STEVES_BU" package="HEATSINK-7019B-MTG" value="HEAT_SINK_HS3597019B-MTG"/>
<element name="R22" library="STEVES_BU" package="0805S" value="2K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R18" library="STEVES_BU" package="0805S" value="2K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R21" library="STEVES_BU" package="0805S" value="0R-DNI">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R20" library="STEVES_BU" package="0805S" value="0R-DNI">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP5" library="SparkFun" package="1X12" value="M12PTH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C22" library="STEVES_BU" package="0805S" value="0.1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP4" library="SparkFun" package="1X12" value="M12PTH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J9" library="STEVES_BU" package="DUAL-BNC" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S102" library="STEVES_BU" package="SWITCH_NKK_MS_DPDT40" value="7201P3CWAV2SE">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R31" library="STEVES_BU" package="0805S" value="90K9">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R32" library="STEVES_BU" package="0805S" value="90K9">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="pinheadA" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="pinheadA" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="OK1" library="optocoupler" package="SMD4" value="SFH6186-2">
<attribute name="OC_NEWARK" value="58K2210"/>
<attribute name="MPN" value="SFH6186-2"/>
<attribute name="MF" value="VISHAY/TELEFUNKEN"/>
<attribute name="OC_FARNELL" value="1469583"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="OK2" library="optocoupler" package="SMD4" value="SFH6186-2">
<attribute name="OC_NEWARK" value="58K2210"/>
<attribute name="MPN" value="SFH6186-2"/>
<attribute name="MF" value="VISHAY/TELEFUNKEN"/>
<attribute name="OC_FARNELL" value="1469583"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R33" library="STEVES_BU" package="0805S" value="1K"/>
<element name="R34" library="STEVES_BU" package="0805S" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="OK3" library="optocoupler" package="SMD4" value="SFH6186-2">
<attribute name="OC_NEWARK" value="58K2210"/>
<attribute name="MPN" value="SFH6186-2"/>
<attribute name="MF" value="VISHAY/TELEFUNKEN"/>
<attribute name="OC_FARNELL" value="1469583"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R35" library="STEVES_BU" package="0805S" value="20K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R30" library="STEVES_BU" package="0805S" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R37" library="STEVES_BU" package="0805S" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="STEVES_BU" package="0805S" value="0.1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="STEVES_BU" package="0805S" value="0.1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="diode" package="SOT23" value="BAT54A">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R38" library="STEVES_BU" package="0805S" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="STEVES_BU" package="LOGO_JANELIA_2014" value="JFRC-LOGOLOGO_JANELIA_2014"/>
<element name="J1" library="SparkFun" package="BNC" value="BNCPTH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J4" library="SparkFun" package="BNC" value="BNCPTH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J5" library="SparkFun" package="BNC" value="BNCPTH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun" package="BNC" value="BNCPTH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="SparkFun" package="BNC" value="BNCPTH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="C2" pad="2"/>
<contactref element="R10" pad="1"/>
<contactref element="R8" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="C4" pad="2"/>
<contactref element="R14" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="D100" pad="1K"/>
<contactref element="C10" pad="2"/>
<contactref element="U5" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="PS100" pad="-"/>
<contactref element="U10" pad="6"/>
<contactref element="U10" pad="5"/>
<contactref element="U10" pad="12"/>
<contactref element="U10" pad="4"/>
<contactref element="C18" pad="2"/>
<contactref element="C17" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="S100" pad="P$2"/>
<contactref element="C14" pad="2"/>
<contactref element="U7" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="S103" pad="P$4"/>
<contactref element="S103" pad="P$1"/>
<contactref element="S101" pad="P$4"/>
<contactref element="S101" pad="P$1"/>
<contactref element="D100" pad="2K"/>
<contactref element="PAD3" pad="1"/>
<contactref element="JP3" pad="1"/>
<contactref element="JP3" pad="2"/>
<contactref element="JP3" pad="3"/>
<contactref element="JP3" pad="4"/>
<contactref element="U6" pad="9"/>
<contactref element="U6" pad="11"/>
<contactref element="U6" pad="7"/>
<contactref element="U6" pad="6"/>
<contactref element="U6" pad="10"/>
<contactref element="C19" pad="2"/>
<contactref element="R28" pad="1"/>
<contactref element="C20" pad="2"/>
<contactref element="R29" pad="1"/>
<contactref element="P3" pad="P$1"/>
<contactref element="P3" pad="P$2"/>
<contactref element="U6" pad="1"/>
<contactref element="U6" pad="14"/>
<contactref element="U6" pad="8"/>
<contactref element="U9" pad="8"/>
<contactref element="U8" pad="3"/>
<contactref element="U8" pad="3"/>
<contactref element="U3" pad="3"/>
<contactref element="C21" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="U6" pad="8"/>
<contactref element="U9" pad="8"/>
<contactref element="U11" pad="4"/>
<contactref element="C16" pad="2"/>
<contactref element="C15" pad="2"/>
<contactref element="U1" pad="4"/>
<contactref element="C5" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="U2" pad="4"/>
<contactref element="J100" pad="3"/>
<contactref element="J101" pad="3"/>
<contactref element="JP5" pad="12"/>
<contactref element="JP5" pad="3"/>
<contactref element="JP5" pad="6"/>
<contactref element="C22" pad="2"/>
<contactref element="JP4" pad="3"/>
<contactref element="JP4" pad="6"/>
<contactref element="JP4" pad="12"/>
<contactref element="JP2" pad="2"/>
<contactref element="JP1" pad="2"/>
<contactref element="OK1" pad="2"/>
<contactref element="OK2" pad="3"/>
<contactref element="R30" pad="1"/>
<contactref element="R37" pad="1"/>
<contactref element="C7" pad="2"/>
<contactref element="C12" pad="2"/>
<contactref element="D1" pad="3"/>
<contactref element="R35" pad="1"/>
<contactref element="J4" pad="GND"/>
<contactref element="J5" pad="GND"/>
</signal>
<signal name="PMT2_IN">
<contactref element="R11" pad="1"/>
<contactref element="J3" pad="S"/>
</signal>
<signal name="N$4">
<contactref element="R11" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="R10" pad="2"/>
<contactref element="U2" pad="5"/>
</signal>
<signal name="PMT1_IN">
<contactref element="R12" pad="1"/>
<contactref element="J2" pad="S"/>
</signal>
<signal name="N$12">
<contactref element="R12" pad="2"/>
<contactref element="R8" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="N$26">
<contactref element="R6" pad="2"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="P1" pad="P$1"/>
<contactref element="R1" pad="2"/>
<contactref element="U1" pad="2"/>
<contactref element="P1" pad="P$2"/>
</signal>
<signal name="N$15">
<contactref element="P5" pad="P$1"/>
<contactref element="R4" pad="2"/>
<contactref element="U2" pad="6"/>
<contactref element="P5" pad="P$2"/>
</signal>
<signal name="N$22">
<contactref element="R1" pad="3"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="R4" pad="3"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="N$33">
<contactref element="U3" pad="2"/>
<contactref element="U1" pad="7"/>
</signal>
<signal name="N$36">
<contactref element="U6" pad="2"/>
<contactref element="U9" pad="7"/>
</signal>
<signal name="N$37">
<contactref element="U9" pad="2"/>
<contactref element="U6" pad="4"/>
</signal>
<signal name="N$38">
<contactref element="U6" pad="15"/>
<contactref element="R15" pad="2"/>
<contactref element="C11" pad="1"/>
</signal>
<signal name="TRIP_OUT">
<contactref element="U9" pad="4"/>
<contactref element="D100" pad="3K"/>
<contactref element="R38" pad="2"/>
<contactref element="S104" pad="2"/>
</signal>
<signal name="N$48">
<contactref element="U9" pad="5"/>
<contactref element="S100" pad="P$3"/>
<contactref element="R19" pad="2"/>
</signal>
<signal name="N$59">
<contactref element="C20" pad="1"/>
<contactref element="S103" pad="P$5"/>
<contactref element="J101" pad="4"/>
</signal>
<signal name="MAN2GAIN">
<contactref element="R29" pad="2"/>
<contactref element="S102" pad="3"/>
</signal>
<signal name="MAN1GAIN">
<contactref element="R28" pad="2"/>
<contactref element="S102" pad="6"/>
</signal>
<signal name="N$65">
<contactref element="U11" pad="6"/>
<contactref element="U11" pad="7"/>
<contactref element="U10" pad="10"/>
</signal>
<signal name="N$69">
<contactref element="U10" pad="11"/>
<contactref element="S103" pad="P$3"/>
</signal>
<signal name="N$45">
<contactref element="R26" pad="1"/>
<contactref element="D100" pad="3A"/>
</signal>
<signal name="N$78">
<contactref element="D100" pad="2A"/>
<contactref element="R17" pad="1"/>
</signal>
<signal name="N$79">
<contactref element="D100" pad="1A"/>
<contactref element="R27" pad="1"/>
</signal>
<signal name="N$34">
<contactref element="U3" pad="4"/>
<contactref element="U9" pad="1"/>
</signal>
<signal name="N$82">
<contactref element="R17" pad="2"/>
<contactref element="U10" pad="1"/>
<contactref element="U10" pad="9"/>
<contactref element="S104" pad="5"/>
</signal>
<signal name="N$83">
<contactref element="S101" pad="P$8"/>
<contactref element="JP4" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="PS100" pad="+"/>
<contactref element="U5" pad="1"/>
<contactref element="C10" pad="1"/>
<contactref element="C13" pad="1"/>
<contactref element="U7" pad="1"/>
</signal>
<signal name="+5VD">
<contactref element="U5" pad="3"/>
<contactref element="C9" pad="1"/>
<contactref element="U10" pad="13"/>
<contactref element="R9" pad="1"/>
<contactref element="R7" pad="2"/>
<contactref element="R13" pad="1"/>
<contactref element="R16" pad="2"/>
<contactref element="U3" pad="5"/>
<contactref element="U8" pad="5"/>
<contactref element="C21" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="U6" pad="16"/>
<contactref element="U9" pad="16"/>
<contactref element="C18" pad="1"/>
<contactref element="C17" pad="1"/>
<contactref element="R15" pad="1"/>
<contactref element="R19" pad="1"/>
<contactref element="R25" pad="1"/>
<contactref element="S101" pad="P$9"/>
<contactref element="S103" pad="P$9"/>
<contactref element="U11" pad="8"/>
<contactref element="R26" pad="2"/>
<contactref element="R27" pad="2"/>
<contactref element="C16" pad="1"/>
<contactref element="C15" pad="1"/>
<contactref element="U1" pad="8"/>
<contactref element="C6" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="U2" pad="8"/>
<contactref element="R22" pad="1"/>
<contactref element="R18" pad="1"/>
<contactref element="R21" pad="1"/>
<contactref element="R20" pad="1"/>
<contactref element="U6" pad="3"/>
<contactref element="JP5" pad="1"/>
<contactref element="C22" pad="1"/>
<contactref element="JP4" pad="1"/>
<contactref element="OK3" pad="4"/>
</signal>
<signal name="N$9">
<contactref element="U9" pad="3"/>
<contactref element="R16" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="R5" pad="2"/>
<contactref element="U2" pad="7"/>
</signal>
<signal name="N$16">
<contactref element="U1" pad="6"/>
<contactref element="U2" pad="2"/>
<contactref element="R13" pad="2"/>
<contactref element="R14" pad="1"/>
</signal>
<signal name="N$20">
<contactref element="U10" pad="2"/>
<contactref element="U11" pad="2"/>
<contactref element="U11" pad="1"/>
</signal>
<signal name="POWER">
<contactref element="C19" pad="1"/>
<contactref element="S101" pad="P$5"/>
<contactref element="J100" pad="4"/>
</signal>
<signal name="GAIN">
<contactref element="S101" pad="P$2"/>
<contactref element="J100" pad="1"/>
<contactref element="JP4" pad="11"/>
</signal>
<signal name="N$17">
<contactref element="S103" pad="P$8"/>
<contactref element="JP5" pad="2"/>
</signal>
<signal name="N$23">
<contactref element="S103" pad="P$2"/>
<contactref element="J101" pad="1"/>
<contactref element="JP5" pad="11"/>
</signal>
<signal name="EXT_GND">
<contactref element="OK3" pad="2"/>
<contactref element="J1" pad="GND"/>
</signal>
<signal name="+15V">
<contactref element="U7" pad="3"/>
<contactref element="C14" pad="1"/>
<contactref element="S101" pad="P$6"/>
<contactref element="S103" pad="P$6"/>
</signal>
<signal name="N$21">
<contactref element="S101" pad="P$3"/>
<contactref element="U10" pad="3"/>
</signal>
<signal name="N$32">
<contactref element="R28" pad="3"/>
<contactref element="R24" pad="1"/>
</signal>
<signal name="N$40">
<contactref element="R29" pad="3"/>
<contactref element="R23" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="PS100" pad="AC2"/>
<contactref element="PAD1" pad="1"/>
</signal>
<signal name="N$41">
<contactref element="PS100" pad="AC1"/>
<contactref element="PAD2" pad="1"/>
</signal>
<signal name="N$1">
</signal>
<signal name="N$46">
</signal>
<signal name="N$49">
</signal>
<signal name="N$51">
</signal>
<signal name="N$56">
<contactref element="U9" pad="11"/>
<contactref element="R22" pad="2"/>
<contactref element="U9" pad="12"/>
<contactref element="U9" pad="10"/>
</signal>
<signal name="N$63">
<contactref element="U9" pad="15"/>
<contactref element="R18" pad="2"/>
<contactref element="U9" pad="14"/>
</signal>
<signal name="N$52">
<contactref element="R21" pad="2"/>
<contactref element="JP4" pad="9"/>
</signal>
<signal name="N$57">
<contactref element="R20" pad="2"/>
<contactref element="JP5" pad="9"/>
</signal>
<signal name="N$60">
<contactref element="P2" pad="P$1"/>
<contactref element="P2" pad="P$2"/>
<contactref element="R2" pad="2"/>
<contactref element="C4" pad="1"/>
<contactref element="U1" pad="5"/>
<contactref element="R2" pad="3"/>
</signal>
<signal name="N$58">
<contactref element="R3" pad="2"/>
<contactref element="P4" pad="P$1"/>
<contactref element="P4" pad="P$2"/>
<contactref element="C3" pad="1"/>
<contactref element="U2" pad="3"/>
<contactref element="R3" pad="3"/>
</signal>
<signal name="N$27">
<contactref element="R3" pad="1"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="N$66">
<contactref element="R6" pad="1"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$19">
<contactref element="U2" pad="1"/>
<contactref element="U3" pad="1"/>
</signal>
<signal name="VREF">
<contactref element="J100" pad="2"/>
<contactref element="R24" pad="2"/>
</signal>
<signal name="N$39">
<contactref element="J101" pad="2"/>
<contactref element="R23" pad="2"/>
</signal>
<signal name="N$43">
<contactref element="JP5" pad="8"/>
<contactref element="JP5" pad="7"/>
</signal>
<signal name="N$42">
<contactref element="JP4" pad="7"/>
<contactref element="JP4" pad="8"/>
</signal>
<signal name="EXT_TRIP_OUT">
<contactref element="OK1" pad="4"/>
<contactref element="J9" pad="P$1"/>
</signal>
<signal name="EXT_TRIP_RST_IN">
<contactref element="R33" pad="2"/>
<contactref element="J9" pad="P$2"/>
</signal>
<signal name="HV_CNTRL">
<contactref element="U8" pad="2"/>
<contactref element="OK3" pad="3"/>
<contactref element="R35" pad="2"/>
</signal>
<signal name="EXT_HV_CNT">
<contactref element="R34" pad="2"/>
<contactref element="J1" pad="S"/>
</signal>
<signal name="TRIP_RST">
<contactref element="OK2" pad="4"/>
<contactref element="S100" pad="P$1"/>
<contactref element="U9" pad="6"/>
<contactref element="R25" pad="2"/>
</signal>
<signal name="N$47">
<contactref element="U11" pad="3"/>
<contactref element="S102" pad="5"/>
</signal>
<signal name="PMT1_GAIN">
<contactref element="R31" pad="2"/>
<contactref element="J4" pad="S"/>
</signal>
<signal name="PMT2_GAIN">
<contactref element="R32" pad="2"/>
<contactref element="J5" pad="S"/>
</signal>
<signal name="N$71">
<contactref element="U11" pad="5"/>
<contactref element="S102" pad="2"/>
</signal>
<signal name="N$24">
<contactref element="JP2" pad="1"/>
<contactref element="J2" pad="GND"/>
</signal>
<signal name="N$7">
<contactref element="JP1" pad="1"/>
<contactref element="J3" pad="GND"/>
</signal>
<signal name="N$18">
<contactref element="OK2" pad="1"/>
<contactref element="R33" pad="1"/>
</signal>
<signal name="N$30">
<contactref element="OK3" pad="1"/>
<contactref element="R34" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="OK2" pad="2"/>
<contactref element="OK1" pad="3"/>
<contactref element="J9" pad="P$4"/>
<contactref element="J9" pad="P$3"/>
</signal>
<signal name="N$11">
<contactref element="R31" pad="1"/>
<contactref element="R30" pad="2"/>
<contactref element="S102" pad="4"/>
<contactref element="C12" pad="1"/>
<contactref element="D1" pad="1"/>
</signal>
<signal name="N$25">
<contactref element="R37" pad="2"/>
<contactref element="R32" pad="1"/>
<contactref element="S102" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="D1" pad="2"/>
</signal>
<signal name="N$31">
<contactref element="OK1" pad="1"/>
<contactref element="R38" pad="1"/>
</signal>
<signal name="N$35">
<contactref element="U8" pad="1"/>
<contactref element="S104" pad="1"/>
</signal>
<signal name="N$28">
<contactref element="S104" pad="3"/>
<contactref element="S104" pad="6"/>
</signal>
<signal name="N$44">
<contactref element="S104" pad="4"/>
<contactref element="U8" pad="4"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
