<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.4.0">
<drawing>
<board>
<plain>
<wire x1="15.367" y1="0" x2="15.367" y2="7.62" width="0" layer="20"/>
<wire x1="15.367" y1="7.62" x2="0" y2="7.62" width="0" layer="20"/>
<wire x1="0" y1="7.62" x2="0" y2="0" width="0" layer="20"/>
<text>3.3</text>
<text>GND</text>
<text>DRY</text>
<wire x1="0" y1="0" x2="15.367" y2="0" width="0" layer="20"/>
<text>ING</text>
<text>DNG</text>
<text>DA</text>
<text>CL</text>
<text>ADO</text>
<text>IN2</text>
<text>IN1</text>
<text>24LC...
Shield for
Teensy 3.1+</text>
</plain>
<libraries>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-CAP">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X06_NO_SILK">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-RES">
</package>
</packages>
</library>
<library name="microchip">
<description>&lt;b&gt;Microchip PIC Microcontrollers and other Devices&lt;/b&gt;&lt;p&gt;
Based on the following sources :
&lt;ul&gt;
&lt;li&gt;Microchip Data Book, 1993
&lt;li&gt;THE EMERGING WORLD STANDARD, 1995/1996
&lt;li&gt;Microchip, Technical Library CD-ROM, June 1998
&lt;li&gt;www.microchip.com
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SO-08">
<description>&lt;B&gt;Small Outline Narrow Plastic Gull Wing&lt;/B&gt;&lt;p&gt;
150-mil body, package type SN</description>
</package>
</packages>
</library>
<library name="own">
<description>wiebel's own</description>
<packages>
<package name="LOGO_MID">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun-Capacitors" package="0603-CAP" value="1.0uF">
<attribute name="PROD_ID" value="CAP-00868"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0603-RES" value="10k">
<attribute name="PROD_ID" value="RES-00824"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0603-RES" value="10k">
<attribute name="PROD_ID" value="RES-00824"/>
</element>
<element name="JP3" library="SparkFun-Connectors" package="1X06_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="JP4" library="SparkFun-Connectors" package="1X06_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="IC1" library="microchip" package="SO-08" value="24LC256SN">
<attribute name="MPN" value="24LC256-I/SN"/>
<attribute name="OC_NEWARK" value="27C9144"/>
<attribute name="MF" value="MICROCHIP"/>
<attribute name="OC_FARNELL" value="9757996"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="own" package="LOGO_MID" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="C1" pad="2"/>
<contactref element="IC1" pad="1"/>
<contactref element="IC1" pad="2"/>
<contactref element="IC1" pad="3"/>
<contactref element="IC1" pad="7"/>
<contactref element="IC1" pad="4"/>
<contactref element="JP4" pad="5"/>
</signal>
<signal name="VCC">
<contactref element="C1" pad="1"/>
<contactref element="IC1" pad="8"/>
<contactref element="R2" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="JP3" pad="5"/>
</signal>
<signal name="SCL">
<contactref element="R2" pad="1"/>
<contactref element="JP3" pad="1"/>
<contactref element="IC1" pad="6"/>
</signal>
<signal name="SDA">
<contactref element="R1" pad="1"/>
<contactref element="JP3" pad="2"/>
<contactref element="IC1" pad="5"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
