<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="15.8625" y2="0" width="0" layer="20"/>
<wire x1="15.8625" y1="0" x2="15.8625" y2="15.8904" width="0" layer="20"/>
<wire x1="15.8625" y1="15.8904" x2="0" y2="15.8904" width="0" layer="20"/>
<wire x1="0" y1="15.8904" x2="0" y2="0" width="0" layer="20"/>
<text>USB-HID-KB-EMU
Rev 2016B
UNTESTED!</text>
<text>100nf</text>
<text>10uf</text>
<text>ATTINY85</text>
<text>68Ω</text>
<text>68Ω</text>
<text>2K2Ω</text>
<text>3V6</text>
<text>3V6</text>
</plain>
<libraries>
<library name="rcl">
<packages>
<package name="C0805">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="M0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.10 W</description>
</package>
</packages>
</library>
<library name="zetex">
<description>&lt;b&gt;Zetex Power MOS FETs, Bridges, Diodes&lt;/b&gt;&lt;p&gt;
http://www.zetex.com&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOD323">
<description>&lt;b&gt;Small Outline Diode&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="USB-A-H">
<description>&lt;b&gt;USB Series A Hole Mounted&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SO08-EIAJ">
<description>Fits EIAJ packages (wide version of the SOIC-8).</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="rcl" package="C0805" value="100nf"/>
<element name="C2" library="rcl" package="C0805" value="10uf"/>
<element name="D1" library="zetex" package="SOD323" value="3V6">
<attribute name="OC_FARNELL" value="1824860"/>
<attribute name="OC_NEWARK" value="79R6078"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value="CDSOD323-T05C"/>
</element>
<element name="D2" library="zetex" package="SOD323" value="3V6">
<attribute name="OC_FARNELL" value="1824860"/>
<attribute name="OC_NEWARK" value="79R6078"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value="CDSOD323-T05C"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="USB-A-H" value="USB-A-H">
<attribute name="PROD_ID" value="CONN-08367"/>
</element>
<element name="R1" library="rcl" package="M0805" value="68R"/>
<element name="R2" library="rcl" package="M0805" value="68R"/>
<element name="R3" library="rcl" package="M0805" value="2k2"/>
<element name="U1" library="SparkFun-DigitalIC" package="SO08-EIAJ" value="Tiny85-20-SMT">
<attribute name="PROD_ID" value="IC-09092"/>
</element>
</elements>
<signals>
<signal name="N$3">
<contactref element="R1" pad="2"/>
<contactref element="D1" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="J1" pad="D-"/>
</signal>
<signal name="N$4">
<contactref element="R2" pad="2"/>
<contactref element="D2" pad="1"/>
<contactref element="J1" pad="D+"/>
</signal>
<signal name="GND">
<contactref element="D1" pad="2"/>
<contactref element="D2" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="U1" pad="4"/>
<contactref element="C1" pad="2"/>
<contactref element="J1" pad="GND"/>
</signal>
<signal name="VCC">
<contactref element="C2" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="J1" pad="VBUS"/>
<contactref element="U1" pad="8"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="R2" pad="1"/>
<contactref element="U1" pad="7"/>
</signal>
<signal name="N$1">
<contactref element="R1" pad="1"/>
<contactref element="U1" pad="5"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
