<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="32.004" y2="0" width="0" layer="20"/>
<wire x1="32.004" y1="0" x2="32.004" y2="19.812" width="0" layer="20"/>
<wire x1="32.004" y1="19.812" x2="0" y2="19.812" width="0" layer="20"/>
<wire x1="0" y1="19.812" x2="0" y2="0" width="0" layer="20"/>
<text>J001332REVA</text>
<text>CABLE SIDE</text>
<text>LCD SIDE</text>
<text>20140815</text>
</plain>
<libraries>
<library name="STEVES">
<packages>
<package name="DMS-20LCD">
</package>
</packages>
</library>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X12">
</package>
</packages>
</library>
<library name="STEVES1">
<packages>
<package name="0805S">
</package>
</packages>
</library>
<library name="STEVES_BU">
<packages>
<package name="0805S">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="LCD2" library="STEVES" package="DMS-20LCD" value="DMS-20LCDDMS-20LCD-RA"/>
<element name="JP9" library="SparkFun" package="1X12" value="PPTC121LGBN-RC">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="STEVES1" package="0805S" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="STEVES_BU" package="0805S" value="0.1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L2" library="STEVES1" package="0805S" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L3" library="STEVES1" package="0805S" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$15">
<contactref element="LCD2" pad="P$6"/>
<contactref element="JP9" pad="6"/>
</signal>
<signal name="N$17">
<contactref element="JP9" pad="5"/>
<contactref element="LCD2" pad="P$5"/>
</signal>
<signal name="N$19">
<contactref element="LCD2" pad="P$4"/>
<contactref element="JP9" pad="4"/>
</signal>
<signal name="N$21">
<contactref element="LCD2" pad="P$3"/>
<contactref element="JP9" pad="3"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="N$22">
<contactref element="JP9" pad="2"/>
<contactref element="LCD2" pad="P$2"/>
</signal>
<signal name="N$23">
<contactref element="JP9" pad="1"/>
<contactref element="L1" pad="1"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="N$24">
<contactref element="LCD2" pad="P$7"/>
<contactref element="JP9" pad="7"/>
</signal>
<signal name="N$25">
<contactref element="JP9" pad="8"/>
<contactref element="LCD2" pad="P$8"/>
</signal>
<signal name="N$26">
<contactref element="LCD2" pad="P$9"/>
<contactref element="JP9" pad="9"/>
</signal>
<signal name="N$29">
<contactref element="JP9" pad="10"/>
<contactref element="LCD2" pad="P$10"/>
</signal>
<signal name="N$35">
<contactref element="JP9" pad="11"/>
<contactref element="L2" pad="2"/>
</signal>
<signal name="N$37">
<contactref element="JP9" pad="12"/>
<contactref element="L3" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="LCD2" pad="P$1"/>
<contactref element="L1" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="LCD2" pad="P$11"/>
<contactref element="L2" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="LCD2" pad="P$12"/>
<contactref element="L3" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
