<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="2.54" x2="0" y2="29.21" width="0" layer="20"/>
<wire x1="0" y1="29.21" x2="2.54" y2="31.75" width="0" layer="20" curve="-90"/>
<wire x1="2.54" y1="31.75" x2="19.05" y2="31.75" width="0" layer="20"/>
<wire x1="19.05" y1="31.75" x2="21.59" y2="29.21" width="0" layer="20" curve="-90"/>
<wire x1="21.59" y1="29.21" x2="21.59" y2="2.54" width="0" layer="20"/>
<wire x1="21.59" y1="2.54" x2="19.05" y2="0" width="0" layer="20" curve="-90"/>
<wire x1="19.05" y1="0" x2="2.54" y2="0" width="0" layer="20"/>
<wire x1="2.54" y1="0" x2="0" y2="2.54" width="0" layer="20" curve="-90"/>
<text>VIN</text>
<text>3V3</text>
<text>SDA</text>
<text>SCL</text>
<text>GND</text>
<text>INT</text>
<text>FIX</text>
<text>Technoblogy</text>
</plain>
<libraries>
<library name="microbuilder">
<packages>
<package name="FGPMMOPA6H">
</package>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt; - 5 Pin</description>
</package>
<package name="CHIPLED_0805_NOOUTLINE">
</package>
<package name="0805-NO">
</package>
</packages>
</library>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SO14">
</package>
</packages>
</library>
<library name="SparkFun-FreqCtrl">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find crystals and oscillators and other things that go "tick".&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CRYSTAL-SMD-5X3">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="1X06-CLEANBIG">
</package>
</packages>
</library>
</libraries>
<attributes>
<attribute name="REV" value="E"/>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="microbuilder" package="FGPMMOPA6H" value="FGPMMOPA6H">
<attribute name="VALUE"/>
</element>
<element name="U2" library="microbuilder" package="SOT23-5" value="MIC5225-3.3"/>
<element name="LED1" library="microbuilder" package="CHIPLED_0805_NOOUTLINE" value="RED"/>
<element name="R1" library="microbuilder" package="0805-NO" value="1K"/>
<element name="C1" library="microbuilder" package="0805-NO" value="0.1uF"/>
<element name="C2" library="microbuilder" package="0805-NO" value="10uF"/>
<element name="C3" library="microbuilder" package="0805-NO" value="10uF"/>
<element name="U$14" library="SparkFun-DigitalIC" package="SO14" value="ATTINY841">
<attribute name="PROD_ID" value="IC-11285"/>
<attribute name="VALUE"/>
</element>
<element name="Y1" library="SparkFun-FreqCtrl" package="CRYSTAL-SMD-5X3" value="8MHz">
<attribute name="PROD_ID" value="XTAL-08297"/>
</element>
<element name="JP3" library="adafruit" package="1X06-CLEANBIG" value="">
<attribute name="VALUE"/>
</element>
<element name="C4" library="microbuilder" package="0805-NO" value="10pf"/>
<element name="C5" library="microbuilder" package="0805-NO" value="10pf"/>
</elements>
<signals>
<signal name="FIX">
<contactref element="U1" pad="P$5"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$2">
<contactref element="LED1" pad="C"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="GND">
<contactref element="R1" pad="1"/>
<contactref element="U1" pad="P$8"/>
<contactref element="U1" pad="P$3"/>
<contactref element="U2" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="U1" pad="P$12"/>
<contactref element="U1" pad="P$19"/>
<contactref element="U$14" pad="14"/>
<contactref element="JP3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="3.3V">
<contactref element="U1" pad="P$1"/>
<contactref element="U2" pad="5"/>
<contactref element="C2" pad="1"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="VIN">
<contactref element="U2" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="U2" pad="3"/>
<contactref element="U$14" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="JP3" pad="3"/>
</signal>
<signal name="TX">
<contactref element="U1" pad="P$9"/>
<contactref element="U$14" pad="11"/>
</signal>
<signal name="SCL">
<contactref element="U$14" pad="9"/>
<contactref element="JP3" pad="6"/>
</signal>
<signal name="SDA">
<contactref element="U$14" pad="7"/>
<contactref element="JP3" pad="5"/>
</signal>
<signal name="N$3">
<contactref element="Y1" pad="3"/>
<contactref element="U$14" pad="3"/>
<contactref element="C5" pad="1"/>
</signal>
<signal name="INT">
<contactref element="U$14" pad="13"/>
<contactref element="JP3" pad="4"/>
</signal>
<signal name="N$1">
<contactref element="C4" pad="1"/>
<contactref element="Y1" pad="1"/>
<contactref element="U$14" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
