<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.4.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="50.978" y2="0" width="0" layer="20"/>
<wire x1="50.978" y1="0" x2="50.978" y2="35.55" width="0" layer="20"/>
<wire x1="50.978" y1="35.55" x2="0" y2="35.55" width="0" layer="20"/>
<wire x1="0" y1="35.55" x2="0" y2="0" width="0" layer="20"/>
<text>Implicit Gatekeeper</text>
<text>©2019 Implicit Technologies, LLC
www.implicittech.com</text>
<text>v1.1</text>
<text>MADE IN USA</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X03">
<description>&lt;h3&gt;Plated Through Hole - 3 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Capacitors&lt;/h3&gt;
This library contains capacitors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CPOL-RADIAL-2.5MM-5MM">
<description>2.5 mm spaced PTHs with 5 mm diameter outline and standard solder mask</description>
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Discrete Semiconductors&lt;/h3&gt;
This library contains diodes, optoisolators, TRIACs, MOSFETs, transistors, etc. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DIODE-1N4148">
</package>
</packages>
</library>
<library name="Omron - G5V-1-DC3">
<description>Upverter Parts Library

Created by Upverter.com</description>
<packages>
<package name="OMRON_G5V-1-DC3_0">
<description>SIGNAL RELAY SPDT 3VDC, 1A, THROUGH HOLE</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.3">
<description>&lt;h3&gt;AXIAL-0.3&lt;/h3&gt;
&lt;p&gt;Commonly used for 1/4W through-hole resistors. 0.3" pitch between holes.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="adafruit_tj">
<packages>
<package name="FEATHERWING">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="TO92-EBC-OVAL">
<description>&lt;b&gt;TO-92&lt;/b&gt;&lt;p&gt;
grid 5.08 mm</description>
</package>
</packages>
</library>
<library name="282837-8_TJ">
<packages>
<package name="5EHDRC">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="12VSTEPUP" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="CPOL-RADIAL-2.5MM-5MM" value="10uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08440"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="CPOL-RADIAL-2.5MM-5MM" value="10uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08440"/>
</element>
<element name="D1" library="SparkFun-DiscreteSemi" package="DIODE-1N4148" value="4148">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="DIO-08378"/>
</element>
<element name="J1" library="282837-8_TJ" package="5EHDRC" value="5EHDRC">
<attribute name="AVAILABILITY" value="Unavailable"/>
<attribute name="COMMENT" value="282837-8"/>
<attribute name="DESCRIPTION" value=" TERMI-BLOK PCB MOUNT 8P  "/>
<attribute name="MF" value="TE Connectivity"/>
<attribute name="MP" value="282837-8"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PRICE" value="None"/>
<attribute name="TE_PURCHASE_URL" value="https://www.te.com/usa-en/product-282837-8.html?te_bu=Cor&amp;te_type=disp&amp;te_campaign=seda_glo_cor-seda-global-disp-prtnr-fy19-seda-model-bom-cta_sma-317_1&amp;elqCampaignId=32493"/>
</element>
<element name="K1" library="Omron - G5V-1-DC3" package="OMRON_G5V-1-DC3_0" value="RELAY">
<attribute name="AMBIENT_TEMPERATURE_RANGE_HIGH" value="+70°C"/>
<attribute name="AMBIENT_TEMPERATURE_RANGE_LOW" value="-40°C"/>
<attribute name="CENTROID_NOT_SPECIFIED" value="No"/>
<attribute name="COIL_CURRENT" value="50mA"/>
<attribute name="COIL_POWER" value="150mW"/>
<attribute name="COIL_RESISTANCE" value="60Ω"/>
<attribute name="COIL_TYPE" value="Non-Latching"/>
<attribute name="CURRENT_RATING" value="2A"/>
<attribute name="DATASHEET" value="https://omronfs.omron.com/en_US/ecb/products/pdf/en-g5v_1.pdf"/>
<attribute name="DEVICE_CLASS_L1" value="Electromechanical"/>
<attribute name="DEVICE_CLASS_L2" value="Relays"/>
<attribute name="DEVICE_CLASS_L3" value="Signal Relays"/>
<attribute name="DIGIKEY_DESCRIPTION" value="RELAY GEN PURPOSE SPDT 1A 125V"/>
<attribute name="DIGIKEY_PART_NUMBER" value="Z2204-ND"/>
<attribute name="HEIGHT" value="10mm"/>
<attribute name="LEAD_FREE" value="yes"/>
<attribute name="MF" value="Omron"/>
<attribute name="MFG_PACKAGE_IDENT" value="G5V-1-DC3"/>
<attribute name="MFG_PACKAGE_IDENT_DATE" value="0"/>
<attribute name="MFG_PACKAGE_IDENT_REV" value="0"/>
<attribute name="MOUSER_DESCRIPTION" value="Low Signal Relays - PCB ThruHole Hi-Sens SPDT 3DC 150mW Seal"/>
<attribute name="MOUSER_PART_NUMBER" value="653-G5V-1-DC3"/>
<attribute name="MPN" value="G5V-1-DC3"/>
<attribute name="NAME"/>
<attribute name="NUMBER_OF_CONTACTS" value="1"/>
<attribute name="PACKAGE" value="PTH_SPDT_RELAY_15MM5_7MM5"/>
<attribute name="PREFIX" value="K"/>
<attribute name="ROHS" value="yes"/>
<attribute name="STANDOFF_HEIGHT" value="0.5mm"/>
<attribute name="SWITCHING_CURRENT" value="1A"/>
<attribute name="TEMPERATURE_RANGE_HIGH" value="+70°C"/>
<attribute name="TEMPERATURE_RANGE_LOW" value="-40°C"/>
<attribute name="THROW_CONFIGURATION" value="SPDT"/>
<attribute name="VERIFICATION_VERSION" value="0.0.0.1"/>
<attribute name="VOLTAGE_RATING_AC" value="125V"/>
<attribute name="VOLTAGE_RATING_DC" value="24V"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="AXIAL-0.3" value="10k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-12183"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="AXIAL-0.3" value="680R">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-12183"/>
<attribute name="VALUE"/>
</element>
<element name="MS1" library="adafruit_tj" package="FEATHERWING" value="FEATHERWING"/>
<element name="T1" library="adafruit" package="TO92-EBC-OVAL" value="2N2222">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="R2" pad="P$2"/>
<contactref element="R1" pad="P$2"/>
<contactref element="T1" pad="B"/>
</signal>
<signal name="N$2">
<contactref element="D1" pad="A"/>
<contactref element="K1" pad="9"/>
<contactref element="T1" pad="C"/>
</signal>
<signal name="GND">
<contactref element="R1" pad="P$1"/>
<contactref element="12VSTEPUP" pad="2"/>
<contactref element="J1" pad="1"/>
<contactref element="J1" pad="5"/>
<contactref element="J1" pad="8"/>
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="MS1" pad="4"/>
<contactref element="T1" pad="E"/>
</signal>
<signal name="12V">
<contactref element="C2" pad="1"/>
<contactref element="K1" pad="6"/>
<contactref element="K1" pad="5"/>
<contactref element="12VSTEPUP" pad="1"/>
</signal>
<signal name="5V">
<contactref element="12VSTEPUP" pad="3"/>
<contactref element="J1" pad="2"/>
<contactref element="MS1" pad="26"/>
</signal>
<signal name="RLYCTL">
<contactref element="R2" pad="P$1"/>
<contactref element="MS1" pad="6"/>
</signal>
<signal name="DOORSENSOR">
<contactref element="J1" pad="7"/>
<contactref element="MS1" pad="5"/>
</signal>
<signal name="DATA1">
<contactref element="J1" pad="4"/>
<contactref element="MS1" pad="25"/>
</signal>
<signal name="DATA0">
<contactref element="J1" pad="3"/>
<contactref element="MS1" pad="23"/>
</signal>
<signal name="LATCH">
<contactref element="J1" pad="6"/>
<contactref element="K1" pad="10"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="3.3V">
<contactref element="MS1" pad="2"/>
<contactref element="D1" pad="C"/>
<contactref element="K1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
