<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.6.2">
<drawing>
<board>
<plain>
<text>evilgeniuslabs.org</text>
<text>Level Shifter FeatherWing v0.1</text>
<text>evilgeniuslabs.org</text>
<text>Level
Shifter
FeatherWing
v0.1</text>
<text>GND</text>
<text>5V</text>
<text>R1</text>
<text>R2</text>
<text>R3</text>
<text>R4</text>
<text>R5</text>
<text>R6</text>
<text>R7</text>
<text>R8</text>
<text>300-
500Ω</text>
<text>R1</text>
<text>R2</text>
<text>R3</text>
<text>R4</text>
<text>R5</text>
<text>R6</text>
<text>R7</text>
<text>R8</text>
<text>R1</text>
<text>R2</text>
<text>R3</text>
<text>R4</text>
<text>R5</text>
<text>R6</text>
<text>R7</text>
<text>R8</text>
</plain>
<libraries>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CAP-PTH-SMALL">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.1">
</package>
</packages>
</library>
<library name="EH DIC-00289 - SN74HCT245 OCTAL BUS TRANSCEIVERS WITH 3-STATE OUTPUTS">
<packages>
<package name="DIL20">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="FEATHERWING">
</package>
<package name="1X08-CLEANBIG">
</package>
<package name="PJ-102A">
</package>
<package name="1X06-CLEANBIG">
</package>
<package name="1X01-CLEANBIG">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R3" library="SparkFun-Resistors" package="AXIAL-0.1" value="300-500Ω">
<attribute name="NAME"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="AXIAL-0.1" value="300-500Ω">
<attribute name="NAME"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="AXIAL-0.1" value="300-500Ω">
<attribute name="NAME"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="AXIAL-0.1" value="300-500Ω">
<attribute name="NAME"/>
</element>
<element name="U$2" library="EH DIC-00289 - SN74HCT245 OCTAL BUS TRANSCEIVERS WITH 3-STATE OUTPUTS" package="DIL20" value="SN74HCT245">
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="CAP-PTH-SMALL" value="0.1uF">
<attribute name="VALUE"/>
</element>
<element name="MS1" library="adafruit" package="FEATHERWING" value="FEATHERWING"/>
<element name="R5" library="SparkFun-Resistors" package="AXIAL-0.1" value="300-500Ω">
<attribute name="NAME"/>
</element>
<element name="R6" library="SparkFun-Resistors" package="AXIAL-0.1" value="300-500Ω">
<attribute name="NAME"/>
</element>
<element name="R7" library="SparkFun-Resistors" package="AXIAL-0.1" value="300-500Ω">
<attribute name="NAME"/>
</element>
<element name="R8" library="SparkFun-Resistors" package="AXIAL-0.1" value="300-500Ω">
<attribute name="NAME"/>
</element>
<element name="JP1" library="adafruit" package="1X08-CLEANBIG" value="">
<attribute name="VALUE"/>
</element>
<element name="U$1" library="adafruit" package="PJ-102A" value="2.1MMJACKTHM"/>
<element name="GND" library="adafruit" package="1X08-CLEANBIG" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="5V" library="adafruit" package="1X06-CLEANBIG" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP5" library="adafruit" package="1X01-CLEANBIG" value="">
<attribute name="VALUE"/>
</element>
<element name="JP6" library="adafruit" package="1X01-CLEANBIG" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="VCC">
<contactref element="U$2" pad="20"/>
<contactref element="C1" pad="1"/>
<contactref element="MS1" pad="26"/>
<contactref element="U$1" pad="TIP"/>
<contactref element="5V" pad="1"/>
<contactref element="5V" pad="2"/>
<contactref element="5V" pad="3"/>
<contactref element="5V" pad="4"/>
<contactref element="5V" pad="5"/>
<contactref element="5V" pad="6"/>
<contactref element="JP5" pad="1"/>
<contactref element="JP6" pad="1"/>
</signal>
<signal name="GND">
<contactref element="U$2" pad="10"/>
<contactref element="U$2" pad="19"/>
<contactref element="U$2" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="MS1" pad="4"/>
<contactref element="U$1" pad="RING_SW"/>
<contactref element="U$1" pad="RING"/>
<contactref element="GND" pad="8"/>
<contactref element="GND" pad="7"/>
<contactref element="GND" pad="6"/>
<contactref element="GND" pad="5"/>
<contactref element="GND" pad="4"/>
<contactref element="GND" pad="3"/>
<contactref element="GND" pad="2"/>
<contactref element="GND" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="R1" pad="P$1"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="R2" pad="P$1"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="B1">
<contactref element="U$2" pad="18"/>
<contactref element="MS1" pad="25"/>
</signal>
<signal name="B2">
<contactref element="U$2" pad="17"/>
<contactref element="MS1" pad="24"/>
</signal>
<signal name="B3">
<contactref element="U$2" pad="16"/>
<contactref element="MS1" pad="23"/>
</signal>
<signal name="B4">
<contactref element="U$2" pad="15"/>
<contactref element="MS1" pad="22"/>
</signal>
<signal name="A1">
<contactref element="U$2" pad="2"/>
<contactref element="R1" pad="P$2"/>
</signal>
<signal name="A2">
<contactref element="U$2" pad="3"/>
<contactref element="R2" pad="P$2"/>
</signal>
<signal name="A3">
<contactref element="U$2" pad="4"/>
<contactref element="R3" pad="P$2"/>
</signal>
<signal name="A4">
<contactref element="U$2" pad="5"/>
<contactref element="R4" pad="P$2"/>
</signal>
<signal name="N$1">
<contactref element="R3" pad="P$1"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="A5">
<contactref element="U$2" pad="6"/>
<contactref element="R5" pad="P$2"/>
</signal>
<signal name="A6">
<contactref element="U$2" pad="7"/>
<contactref element="R6" pad="P$2"/>
</signal>
<signal name="A8">
<contactref element="U$2" pad="9"/>
<contactref element="R8" pad="P$2"/>
</signal>
<signal name="B8">
<contactref element="U$2" pad="11"/>
<contactref element="MS1" pad="18"/>
</signal>
<signal name="B7">
<contactref element="U$2" pad="12"/>
<contactref element="MS1" pad="19"/>
</signal>
<signal name="B6">
<contactref element="U$2" pad="13"/>
<contactref element="MS1" pad="20"/>
</signal>
<signal name="B5">
<contactref element="U$2" pad="14"/>
<contactref element="MS1" pad="21"/>
</signal>
<signal name="A7">
<contactref element="U$2" pad="8"/>
<contactref element="R7" pad="P$2"/>
</signal>
<signal name="N$2">
<contactref element="R5" pad="P$1"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="N$3">
<contactref element="R7" pad="P$1"/>
<contactref element="JP1" pad="7"/>
</signal>
<signal name="R6">
<contactref element="R6" pad="P$1"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="N$7">
<contactref element="R8" pad="P$1"/>
<contactref element="JP1" pad="8"/>
</signal>
<signal name="N$8">
<contactref element="R4" pad="P$1"/>
<contactref element="JP1" pad="4"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
