<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="28.5625" y2="0" width="0" layer="20"/>
<wire x1="28.5625" y1="0" x2="28.5625" y2="36.185" width="0" layer="20"/>
<wire x1="28.5625" y1="36.185" x2="0" y2="36.185" width="0" layer="20"/>
<wire x1="0" y1="36.185" x2="0" y2="0" width="0" layer="20"/>
<text>1 GND</text>
<text>2 3V3</text>
<text>3 EN</text>
<text>4 SENSOR_VP</text>
<text>5 SENSOR_VN</text>
<text>6 IO34</text>
<text>7 IO35</text>
<text>8 IO32</text>
<text>9 IO33</text>
<text>10 IO25</text>
<text>11 IO26</text>
<text>12 IO27</text>
<text>13 IO14</text>
<text>14 IO12</text>
<text>16 I013</text>
<text>17 SD2</text>
<text>18 SD3</text>
<text>19 CMD</text>
<text>20 CLK</text>
<text>21 SD0</text>
<text>22 SD1</text>
<text>23 IO15</text>
<text>24 IO2</text>
<text>IO0 25</text>
<text>IO4 26</text>
<text>IO16 27</text>
<text>IO17 28</text>
<text>IO5 29</text>
<text>IO18 30</text>
<text>IO19 31</text>
<text>IO21 33</text>
<text>RXD0 34</text>
<text>TXD0 35</text>
<text>IO22 36</text>
<text>IO23 37</text>
<text>esp-32s
breakout</text>
<text>(c)
packom.net
2016</text>
<text>esp-32s breakout
(c) packom.net 2016</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X14">
<description>&lt;h3&gt;Plated Through Hole -14 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:14&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_14&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X12">
<description>&lt;h3&gt;Plated Through Hole -12 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:12&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_12&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X09">
<description>&lt;h3&gt;Plated Through Hole -9 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:9&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_09&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="Piers's library">
<packages>
<package name="ESP-32S">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="SparkFun-Connectors" package="1X14" value="">
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X12" value="">
<attribute name="VALUE"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="1X09" value="">
<attribute name="VALUE"/>
</element>
<element name="U$1" library="Piers's library" package="ESP-32S" value="ESP-32S"/>
</elements>
<signals>
<signal name="N$2">
<contactref element="U$1" pad="3V3"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="U$1" pad="EN"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="U$1" pad="SENSOR_VP"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="N$5">
<contactref element="U$1" pad="SENSOR_VN"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="N$6">
<contactref element="U$1" pad="IO34"/>
<contactref element="J1" pad="6"/>
</signal>
<signal name="N$7">
<contactref element="U$1" pad="IO35"/>
<contactref element="J1" pad="7"/>
</signal>
<signal name="N$8">
<contactref element="U$1" pad="IO32"/>
<contactref element="J1" pad="8"/>
</signal>
<signal name="N$9">
<contactref element="U$1" pad="IO33"/>
<contactref element="J1" pad="9"/>
</signal>
<signal name="N$10">
<contactref element="U$1" pad="IO25"/>
<contactref element="J1" pad="10"/>
</signal>
<signal name="N$11">
<contactref element="U$1" pad="IO26"/>
<contactref element="J1" pad="11"/>
</signal>
<signal name="N$12">
<contactref element="U$1" pad="IO27"/>
<contactref element="J1" pad="12"/>
</signal>
<signal name="N$13">
<contactref element="U$1" pad="IO14"/>
<contactref element="J1" pad="13"/>
</signal>
<signal name="N$14">
<contactref element="U$1" pad="IO12"/>
<contactref element="J1" pad="14"/>
</signal>
<signal name="N$15">
<contactref element="J3" pad="1"/>
<contactref element="U$1" pad="IO13"/>
</signal>
<signal name="N$16">
<contactref element="J3" pad="2"/>
<contactref element="U$1" pad="SD2"/>
</signal>
<signal name="N$17">
<contactref element="J3" pad="3"/>
<contactref element="U$1" pad="SD3"/>
</signal>
<signal name="N$18">
<contactref element="J3" pad="4"/>
<contactref element="U$1" pad="CMD"/>
</signal>
<signal name="N$19">
<contactref element="J3" pad="5"/>
<contactref element="U$1" pad="CLK"/>
</signal>
<signal name="N$20">
<contactref element="J3" pad="6"/>
<contactref element="U$1" pad="SD0"/>
</signal>
<signal name="N$21">
<contactref element="J3" pad="7"/>
<contactref element="U$1" pad="SD1"/>
</signal>
<signal name="N$22">
<contactref element="J3" pad="8"/>
<contactref element="U$1" pad="IO15"/>
</signal>
<signal name="N$23">
<contactref element="J3" pad="9"/>
<contactref element="U$1" pad="IO2"/>
</signal>
<signal name="N$24">
<contactref element="J2" pad="1"/>
<contactref element="U$1" pad="IO0"/>
</signal>
<signal name="N$25">
<contactref element="J2" pad="2"/>
<contactref element="U$1" pad="IO4"/>
</signal>
<signal name="N$26">
<contactref element="J2" pad="3"/>
<contactref element="U$1" pad="IO16"/>
</signal>
<signal name="N$27">
<contactref element="J2" pad="4"/>
<contactref element="U$1" pad="IO17"/>
</signal>
<signal name="N$28">
<contactref element="J2" pad="5"/>
<contactref element="U$1" pad="IO5"/>
</signal>
<signal name="N$29">
<contactref element="J2" pad="6"/>
<contactref element="U$1" pad="IO18"/>
</signal>
<signal name="N$30">
<contactref element="J2" pad="7"/>
<contactref element="U$1" pad="IO19"/>
</signal>
<signal name="N$31">
<contactref element="J2" pad="8"/>
<contactref element="U$1" pad="IO21"/>
</signal>
<signal name="N$32">
<contactref element="J2" pad="9"/>
<contactref element="U$1" pad="RXD0"/>
</signal>
<signal name="N$33">
<contactref element="J2" pad="10"/>
<contactref element="U$1" pad="TXD0"/>
</signal>
<signal name="N$34">
<contactref element="J2" pad="11"/>
<contactref element="U$1" pad="IO22"/>
</signal>
<signal name="N$35">
<contactref element="J2" pad="12"/>
<contactref element="U$1" pad="IO23"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="GND_PAD"/>
<contactref element="U$1" pad="VIA1"/>
<contactref element="U$1" pad="VIA2"/>
<contactref element="U$1" pad="VIA3"/>
<contactref element="U$1" pad="VIA4"/>
<contactref element="U$1" pad="VIA5"/>
<contactref element="U$1" pad="VIA6"/>
<contactref element="U$1" pad="VIA7"/>
<contactref element="U$1" pad="VIA8"/>
<contactref element="U$1" pad="VIA9"/>
<contactref element="U$1" pad="VIA10"/>
<contactref element="U$1" pad="VIA11"/>
<contactref element="U$1" pad="VIA12"/>
<contactref element="U$1" pad="VIA13"/>
<contactref element="U$1" pad="VIA14"/>
<contactref element="U$1" pad="VIA15"/>
<contactref element="U$1" pad="VIA16"/>
<contactref element="U$1" pad="GND38"/>
<contactref element="U$1" pad="GND"/>
<contactref element="U$1" pad="GND15"/>
<contactref element="J1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
