<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.2.0">
<drawing>
<board>
<plain>
<wire x1="25.654" y1="0" x2="25.654" y2="41.148" width="0" layer="20"/>
<wire x1="25.654" y1="41.148" x2="0" y2="41.148" width="0" layer="20"/>
<wire x1="0" y1="41.148" x2="0" y2="0" width="0" layer="20"/>
<wire x1="0" y1="0" x2="25.654" y2="0" width="0" layer="20"/>
<text>ESP-07</text>
<text>RX  TX</text>
<text>IO15</text>
<text>IO5</text>
<text>IO4</text>
<text>CuriousTech.net</text>
<text>IO13</text>
<text>IO16</text>
<text>DS18B20
IO14</text>
<text>Slave
IO12</text>
<text>IO2</text>
<text>3V3</text>
<text>ADC</text>
<text>Waterbed Heater</text>
<text>WiFi Smart</text>
<text>GND</text>
<text>SDA</text>
<text>SCL</text>
<text>GND</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X04">
</package>
<package name="1X02">
</package>
<package name="1X06">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805-CAP">
</package>
</packages>
</library>
<library name="CuriousTech">
<description>CuriousTech custom misc parts</description>
<packages>
<package name="OMROM_TH">
</package>
<package name="SMD-PAD1">
<description>SMD pad 0.2x0.1</description>
</package>
<package name="SIDE-TACT">
</package>
</packages>
</library>
<library name="ESP-07_12">
<packages>
<package name="ESP-07/12">
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23-3">
</package>
<package name="SOD-323">
</package>
</packages>
</library>
<library name="wirepad">
<description>&lt;b&gt;Single Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1,6/0,8">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Sensors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find sensors- accelerometers, gyros, compasses, magnetometers, light sensors, imagers, temp sensors, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="PHOTOCELL">
</package>
</packages>
</library>
<library name="jumper">
<description>&lt;b&gt;Jumpers&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SJ_2">
<description>&lt;b&gt;Solder jumper&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R2" library="SparkFun-Resistors" package="0805" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="0805" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="ESP-07_12" package="ESP-07/12" value="ESP-07/12"/>
<element name="R1" library="SparkFun-Resistors" package="0805" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="OLED" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="." library="SparkFun-Connectors" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="SparkFun-DiscreteSemi" package="SOT23-3" value="P-FET">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LEFT" library="CuriousTech" package="OMROM_TH" value="OMROM_TH"/>
<element name="RIGHT" library="CuriousTech" package="OMROM_TH" value="OMROM_TH"/>
<element name="U$10" library="CuriousTech" package="SMD-PAD1" value="SMD-PAD1"/>
<element name="U$2" library="CuriousTech" package="SMD-PAD1" value="SMD-PAD1"/>
<element name="U$3" library="CuriousTech" package="SMD-PAD1" value="SMD-PAD1"/>
<element name="U$6" library="CuriousTech" package="SMD-PAD1" value="SMD-PAD1"/>
<element name="U$11" library="CuriousTech" package="SMD-PAD1" value="SMD-PAD1"/>
<element name="Q2" library="SparkFun-DiscreteSemi" package="SOT23-3" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="TRANS-08049"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="SparkFun-Resistors" package="0805" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="+" library="wirepad" package="1,6/0,8" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="-" library="wirepad" package="1,6/0,8" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="SparkFun-DiscreteSemi" package="SOD-323" value="250mA/100V">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="DIO-09646"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="SparkFun-Resistors" package="0805" value="4K7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$8" library="CuriousTech" package="SMD-PAD1" value="SMD-PAD1"/>
<element name="C2" library="SparkFun-Capacitors" package="0805-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="0805" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="0805" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="0805-CAP" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="0805-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="SparkFun-Sensors" package="PHOTOCELL" value="PHOTOCELLPTH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="SparkFun-Resistors" package="0805" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="SparkFun-Resistors" package="0805" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$5" library="CuriousTech" package="SIDE-TACT" value="SIDE-TACT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$7" library="CuriousTech" package="SIDE-TACT" value="SIDE-TACT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="1X06" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-08437"/>
<attribute name="VALUE"/>
</element>
<element name="SJ1" library="jumper" package="SJ_2" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="IO15">
<contactref element="U$1" pad="GPIO15"/>
<contactref element="R1" pad="2"/>
<contactref element="SJ1" pad="3"/>
</signal>
<signal name="N$11">
<contactref element="R2" pad="1"/>
<contactref element="U$1" pad="CH_PD"/>
</signal>
<signal name="3V3">
<contactref element="R2" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="U$1" pad="VCC"/>
<contactref element="U$3" pad="&gt;NAME"/>
<contactref element="Q1" pad="2"/>
<contactref element="+" pad="1"/>
<contactref element="D1" pad="C"/>
<contactref element="R9" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="R4" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="OLED" pad="2"/>
<contactref element="U$8" pad="&gt;NAME"/>
<contactref element="R8" pad="2"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="N$25">
</signal>
<signal name="N$24">
</signal>
<signal name="N$27">
</signal>
<signal name="N$29">
</signal>
<signal name="REST">
<contactref element="R3" pad="1"/>
<contactref element="U$1" pad="REST"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="GND"/>
<contactref element="R1" pad="1"/>
<contactref element="RIGHT" pad="P4"/>
<contactref element="LEFT" pad="P4"/>
<contactref element="RIGHT" pad="P2"/>
<contactref element="U$6" pad="&gt;NAME"/>
<contactref element="U$11" pad="&gt;NAME"/>
<contactref element="Q2" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="OLED" pad="1"/>
<contactref element="R10" pad="1"/>
<contactref element="U$5" pad="3"/>
<contactref element="U$5" pad="4"/>
<contactref element="U$7" pad="3"/>
<contactref element="U$7" pad="4"/>
<contactref element="J1" pad="6"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="TXD">
<contactref element="U$1" pad="TXD"/>
<contactref element="." pad="1"/>
<contactref element="U$7" pad="2"/>
<contactref element="U$7" pad="1"/>
</signal>
<signal name="RXD">
<contactref element="U$1" pad="RXD"/>
<contactref element="." pad="2"/>
<contactref element="SJ1" pad="1"/>
</signal>
<signal name="ADC">
<contactref element="U$1" pad="ADC"/>
<contactref element="R7" pad="1"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="IO2">
<contactref element="U$1" pad="GPIO2"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="IO12">
<contactref element="U$1" pad="GPIO12"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="IO14">
<contactref element="U$1" pad="GPIO14"/>
<contactref element="U$10" pad="&gt;NAME"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="IO13">
<contactref element="U$1" pad="GPIO13"/>
<contactref element="RIGHT" pad="P1"/>
</signal>
<signal name="IO16">
<contactref element="U$1" pad="GPIO16"/>
<contactref element="R4" pad="1"/>
<contactref element="LEFT" pad="P3"/>
</signal>
<signal name="IO0">
<contactref element="U$1" pad="GPIO0"/>
<contactref element="U$5" pad="1"/>
<contactref element="U$5" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="U$2" pad="&gt;NAME"/>
<contactref element="Q1" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="Q2" pad="3"/>
<contactref element="-" pad="1"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="N$2">
<contactref element="Q2" pad="1"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="Q1" pad="1"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="SDA">
<contactref element="OLED" pad="4"/>
<contactref element="U$1" pad="GPIO5"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="SCL">
<contactref element="OLED" pad="3"/>
<contactref element="U$1" pad="GPIO4"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="R7" pad="2"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="SJ1" pad="2"/>
<contactref element="R6" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
