<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.7.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="19.03" y2="0" width="0" layer="20"/>
<wire x1="19.03" y1="0" x2="19.03" y2="16.18" width="0" layer="20"/>
<wire x1="19.03" y1="16.18" x2="0" y2="16.18" width="0" layer="20"/>
<wire x1="0" y1="16.18" x2="0" y2="0" width="0" layer="20"/>
<text>L6362 Breakout board</text>
<text>Designed in Thailand
By Tinlethax</text>
<text>24V
C/Q</text>
<text>GND</text>
<text>rev1.0</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="C0603K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 0603 Reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 1608</description>
</package>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="Wurth_Connectors_WR-PHD">
<description>&lt;BR&gt;Wurth Elektronik - Connectors - Board-to-Board Connectors - WR-PHD &lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2021a, 2021-11-04&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="61300311121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54mm Pin Header, 3 Pin</description>
</package>
<package name="61300611121">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt; 2.54mm Pin Header, 6 Pin</description>
</package>
</packages>
</library>
<library name="L6362A">
<packages>
<package name="VFDFPN12L_3X3X0P9_STM">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="adafruit" package="C0603K" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="adafruit" package="C0603K" value="1pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="adafruit" package="C0603K" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="Wurth_Connectors_WR-PHD" package="61300311121" value=" 61300311121 ">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/61300311121.pdf"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="NAME"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value=" 61300311121 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="Wurth_Connectors_WR-PHD" package="61300611121" value=" 61300611121 ">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/61300611121.pdf"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="NAME"/>
<attribute name="PACKAGING" value="Bag"/>
<attribute name="PART-NUMBER" value=" 61300611121 "/>
<attribute name="PINS" value=" 6 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="ROWS" value="Single"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="adafruit" package="R0603" value="2k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="adafruit" package="R0603" value="10R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="adafruit" package="R0603" value="100R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U101" library="L6362A" package="VFDFPN12L_3X3X0P9_STM" value="L6362ATRVFDFPN12L_3X3X0P9_STM">
<attribute name="COPYRIGHT" value="Copyright (C) 2024 Ultra Librarian. All rights reserved."/>
<attribute name="MANUFACTURER_PART_NUMBER" value="L6362ATR"/>
<attribute name="MFR_NAME" value="STMicroelectronics"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="I/Q">
<contactref element="U101" pad="10"/>
<contactref element="R3" pad="1"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="C/Q">
<contactref element="U101" pad="11"/>
<contactref element="R3" pad="2"/>
<contactref element="U101" pad="9"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="OL">
<contactref element="U101" pad="6"/>
<contactref element="R1" pad="1"/>
<contactref element="J2" pad="5"/>
</signal>
<signal name="VIOL">
<contactref element="U101" pad="12"/>
<contactref element="J1" pad="1"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="GNDIO">
<contactref element="U101" pad="7"/>
<contactref element="C2" pad="2"/>
<contactref element="J1" pad="3"/>
<contactref element="C1" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="UART_RX">
<contactref element="U101" pad="3"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="UART_TX">
<contactref element="U101" pad="5"/>
<contactref element="J2" pad="4"/>
</signal>
<signal name="VREG">
<contactref element="C3" pad="1"/>
<contactref element="U101" pad="1"/>
<contactref element="U101" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="U101" pad="8"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="EN/DIAG">
<contactref element="U101" pad="4"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="GND">
<contactref element="R2" pad="1"/>
<contactref element="J2" pad="6"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
