<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.3.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="19.05" x2="53.28" y2="19.05" width="0" layer="20"/>
<wire x1="53.28" y1="19.05" x2="53.28" y2="80" width="0" layer="20"/>
<wire x1="53.28" y1="80" x2="0" y2="80" width="0" layer="20"/>
<wire x1="0" y1="80" x2="0" y2="19.05" width="0" layer="20"/>
<text>5V Power</text>
<text>GND</text>
<text>GND</text>
<text>+5Vin</text>
<text>Arduino Nano</text>
<text>Plipbox Nano by lallafah</text>
<text>Board design by Aaron Morris 2015</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="POWER_JACK_PTH">
</package>
</packages>
</library>
<library name="jet-lib">
<packages>
<package name="PDIP-32">
</package>
</packages>
</library>
<library name="con-subd">
<description>&lt;b&gt;SUB-D Connectors&lt;/b&gt;&lt;p&gt;
Harting&lt;br&gt;
NorComp&lt;br&gt;
&lt;p&gt;
PREFIX :&lt;br&gt;
H = High density&lt;br&gt;
F = Female&lt;br&gt;
M = Male&lt;p&gt;
NUMBER: Number of pins&lt;p&gt;
SUFFIX :&lt;br&gt;
H = Horizontal&lt;br&gt;
V = Vertical &lt;br&gt;
P = Shield pin on housing&lt;br&gt;
B = No mounting holes&lt;br&gt;
S = Pins individually placeable (Single)&lt;br&gt;
D = Direct mounting &lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="M25HP">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="SparkFun-Connectors" package="POWER_JACK_PTH" value="POWER_JACKPTH">
<attribute name="PROD_ID" value="CONN-08197"/>
</element>
<element name="1" library="jet-lib" package="PDIP-32" value="1"/>
<element name="X1" library="con-subd" package="M25HP" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="D0">
<contactref element="X1" pad="2"/>
<contactref element="1" pad="A7"/>
</signal>
<signal name="D1">
<contactref element="X1" pad="3"/>
<contactref element="1" pad="A6"/>
</signal>
<signal name="D2">
<contactref element="X1" pad="4"/>
<contactref element="1" pad="A5"/>
</signal>
<signal name="D3">
<contactref element="X1" pad="5"/>
<contactref element="1" pad="A4"/>
</signal>
<signal name="D4">
<contactref element="X1" pad="6"/>
<contactref element="1" pad="A3"/>
</signal>
<signal name="D5">
<contactref element="X1" pad="7"/>
<contactref element="1" pad="A2"/>
</signal>
<signal name="D6">
<contactref element="X1" pad="8"/>
<contactref element="1" pad="D6"/>
</signal>
<signal name="D7">
<contactref element="X1" pad="9"/>
<contactref element="1" pad="D7"/>
</signal>
<signal name="/ACK">
<contactref element="X1" pad="10"/>
<contactref element="1" pad="D8"/>
</signal>
<signal name="BUSY">
<contactref element="X1" pad="11"/>
<contactref element="1" pad="D4"/>
</signal>
<signal name="POUT">
<contactref element="X1" pad="12"/>
<contactref element="1" pad="D5"/>
</signal>
<signal name="SELECT">
<contactref element="X1" pad="13"/>
<contactref element="1" pad="D9"/>
</signal>
<signal name="GND">
<contactref element="X1" pad="17"/>
<contactref element="X1" pad="18"/>
<contactref element="X1" pad="19"/>
<contactref element="X1" pad="20"/>
<contactref element="X1" pad="21"/>
<contactref element="X1" pad="22"/>
<contactref element="1" pad="GND"/>
<contactref element="1" pad="GND1"/>
<contactref element="JP1" pad="GNDBREAK"/>
<contactref element="JP1" pad="GND"/>
</signal>
<signal name="/STROBE">
<contactref element="X1" pad="1"/>
<contactref element="1" pad="D3"/>
</signal>
<signal name="VCC">
<contactref element="JP1" pad="PWR"/>
<contactref element="1" pad="VIN"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
