<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.2">
<drawing>
<board>
<plain>
<wire x1="0.254" y1="0" x2="7.366" y2="0" width="0" layer="20"/>
<wire x1="7.366" y1="0" x2="7.366" y2="17.78" width="0" layer="20"/>
<wire x1="7.366" y1="17.78" x2="0.254" y2="17.78" width="0" layer="20"/>
<wire x1="0.254" y1="17.78" x2="0.254" y2="0" width="0" layer="20"/>
<text>GND</text>
<text>3-5V</text>
<text>SDA</text>
<text>SCL</text>
<text>A0</text>
<text>A1</text>
<text>A2</text>
</plain>
<libraries>
<library name="0CBW">
<description>&lt;b&gt;PCB Libraries Packages&lt;/b&gt;&lt;p&gt;
\</description>
<packages>
<package name="CC0805N-L">
</package>
<package name="MSOP8_NARROW_PADS">
</package>
<package name="SJ">
<description>&lt;b&gt;Solder jumper&lt;/b&gt;</description>
</package>
<package name=".060-.150">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
<description>&lt;p&gt;&lt;b&gt;Generic 2012 (0805) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="0CBW" package="CC0805N-L" value="C0805C225K4RACTUCC0805N-L">
<attribute name="MANUFACTURER_PART_NUMBER" value="C0805C225K4RACTU"/>
<attribute name="VENDOR" value="Kemet"/>
</element>
<element name="PAD1" library="0CBW" package=".060-.150" value="WIREPAD.060-.150">
<attribute name="VALUE"/>
</element>
<element name="PAD2" library="0CBW" package=".060-.150" value="WIREPAD.060-.150">
<attribute name="VALUE"/>
</element>
<element name="PAD3" library="0CBW" package=".060-.150" value="WIREPAD.060-.150">
<attribute name="VALUE"/>
</element>
<element name="PAD4" library="0CBW" package=".060-.150" value="WIREPAD.060-.150">
<attribute name="VALUE"/>
</element>
<element name="SJ1" library="0CBW" package="SJ" value="">
<attribute name="VALUE"/>
</element>
<element name="SJ2" library="0CBW" package="SJ" value="">
<attribute name="VALUE"/>
</element>
<element name="SJ3" library="0CBW" package="SJ" value="">
<attribute name="VALUE"/>
</element>
<element name="U1" library="0CBW" package="MSOP8_NARROW_PADS" value="MCP9808T-E/MC">
<attribute name="BUILT_BY" value="EMA_UL_Team"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="MCP9808T-E/MC"/>
<attribute name="SOURCELIBRARY" value="Microchip_2014-11-20"/>
<attribute name="VENDOR" value="Microchip"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0805" value=" ">
<attribute name="NAME"/>
<attribute name="PROD_ID" value=" "/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0805" value=" ">
<attribute name="NAME"/>
<attribute name="PROD_ID" value=" "/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="0805" value=" ">
<attribute name="NAME"/>
<attribute name="PROD_ID" value=" "/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U1" pad="4"/>
<contactref element="PAD4" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="SJ1" pad="1"/>
<contactref element="U1" pad="5"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="SJ2" pad="1"/>
<contactref element="U1" pad="6"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="SJ3" pad="1"/>
<contactref element="U1" pad="7"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="VDD">
<contactref element="SJ3" pad="2"/>
<contactref element="SJ2" pad="2"/>
<contactref element="SJ1" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="PAD1" pad="1"/>
<contactref element="U1" pad="8"/>
</signal>
<signal name="N$7">
<contactref element="U1" pad="2"/>
<contactref element="PAD3" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="U1" pad="1"/>
<contactref element="PAD2" pad="1"/>
</signal>
<signal name="N$4">
</signal>
<signal name="N$5">
</signal>
<signal name="N$6">
</signal>
<signal name="N$10">
</signal>
</signals>
</board>
</drawing>
</eagle>
