<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.1.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="12.624" y2="0" width="0" layer="20"/>
<wire x1="12.624" y1="0" x2="12.624" y2="24.12" width="0" layer="20"/>
<wire x1="12.624" y1="24.12" x2="0" y2="24.12" width="0" layer="20"/>
<wire x1="0" y1="24.12" x2="0" y2="0" width="0" layer="20"/>
<hole x="3.175" y="17.78" drill="3.2"/>
<hole x="9.525" y="17.78" drill="3.2"/>
<text>WS</text>
<text>Gnd</text>
<text>5v</text>
<text>Sig</text>
<hole x="6.35" y="10.16" drill="3.2"/>
<text>'16</text>
</plain>
<libraries>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-CAP">
</package>
<package name="0603-RES">
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-0603">
</package>
</packages>
</library>
<library name="TPS5430">
<packages>
<package name="US5881-HALL-EFFECT">
</package>
</packages>
</library>
<library name="jst_eph">
<description>JST PH series crimp-style 2mm connectors</description>
<packages>
<package name="B3B-PH-K-S">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun-Passives" package="0603-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Passives" package="0603-CAP" value="4.7nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="SparkFun-LED" package="LED-0603" value="Power">
<attribute name="VALUE"/>
</element>
<element name="LED2" library="SparkFun-LED" package="LED-0603" value="Sig">
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Passives" package="0603-RES" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Passives" package="0603-RES" value="2k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun-Passives" package="0603-RES" value="2k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="TPS5430" package="US5881-HALL-EFFECT" value="US5881-HALL-EFFECT"/>
<element name="JP1" library="jst_eph" package="B3B-PH-K-S" value="3PIN"/>
</elements>
<signals>
<signal name="VDD">
<contactref element="C1" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="U$1" pad="VDD"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="GND">
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="LED1" pad="C"/>
<contactref element="U$1" pad="GND"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="SIGNAL">
<contactref element="C2" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="LED2" pad="C"/>
<contactref element="U$1" pad="VOUT"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="N$6">
<contactref element="R2" pad="2"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$7">
<contactref element="R3" pad="1"/>
<contactref element="LED2" pad="A"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
