<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="2" x2="0" y2="12.732" width="0.0762" layer="20"/>
<wire x1="0" y1="12.732" x2="2" y2="14.732" width="0.0762" layer="20" curve="-90"/>
<wire x1="2" y1="14.732" x2="13.748" y2="14.732" width="0.0762" layer="20"/>
<wire x1="13.748" y1="14.732" x2="15.748" y2="12.732" width="0.0762" layer="20" curve="-90"/>
<wire x1="15.748" y1="12.732" x2="15.748" y2="2" width="0.0762" layer="20"/>
<wire x1="15.748" y1="2" x2="13.748" y2="0" width="0.0762" layer="20" curve="-90"/>
<wire x1="13.748" y1="0" x2="2" y2="0" width="0.0762" layer="20"/>
<wire x1="2" y1="0" x2="0" y2="2" width="0.0762" layer="20" curve="-90"/>
<text>DPDT
BREADBOARD PCB</text>
<text>ZERO G IOD</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>5</text>
<text>6</text>
</plain>
<libraries>
<library name="switches">
<packages>
<package name="DPDT_SOLDER_LUG">
<description>&lt;b&gt;Taiway 1MD1T1B1C0M1QE&lt;/b&gt;
&lt;br&gt;
 &lt;a href="http://smallbear-electronics.mybigcommerce.com/dpdt-on-on-solder-term/"&gt;http://smallbear-electronics.mybigcommerce.com/dpdt-on-on-solder-term/&lt;/a&gt;</description>
</package>
</packages>
</library>
<library name="supply pins">
<packages>
<package name="UNLABELED2">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="SW1" library="switches" package="DPDT_SOLDER_LUG" value="dpdt"/>
<element name="U$1" library="supply pins" package="UNLABELED2" value="PADSQ"/>
<element name="U$2" library="supply pins" package="UNLABELED2" value="PADSQ"/>
<element name="U$3" library="supply pins" package="UNLABELED2" value="PADSQ"/>
<element name="U$4" library="supply pins" package="UNLABELED2" value="PADSQ"/>
<element name="U$5" library="supply pins" package="UNLABELED2" value="PADSQ"/>
<element name="U$6" library="supply pins" package="UNLABELED2" value="PADSQ"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="SW1" pad="A2"/>
<contactref element="U$1" pad="P$1"/>
</signal>
<signal name="N$2">
<contactref element="SW1" pad="B2"/>
<contactref element="U$2" pad="P$1"/>
</signal>
<signal name="N$3">
<contactref element="SW1" pad="A1"/>
<contactref element="U$3" pad="P$1"/>
</signal>
<signal name="N$4">
<contactref element="SW1" pad="A3"/>
<contactref element="U$4" pad="P$1"/>
</signal>
<signal name="N$5">
<contactref element="SW1" pad="B1"/>
<contactref element="U$5" pad="P$1"/>
</signal>
<signal name="N$6">
<contactref element="SW1" pad="B3"/>
<contactref element="U$6" pad="P$1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
