<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="30.48" y2="0" width="0.1524" layer="20"/>
<wire x1="30.48" y1="0" x2="30.48" y2="50.8" width="0.1524" layer="20"/>
<wire x1="0" y1="50.8" x2="0" y2="0" width="0.1524" layer="20"/>
<wire x1="0" y1="50.8" x2="30.48" y2="50.8" width="0.1524" layer="20"/>
</plain>
<libraries>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Aesthetics&lt;/h3&gt;
This library contiains non-functional items such as logos, build/ordering notes, frame blocks, etc. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CREATIVE_COMMONS">
<description>&lt;h3&gt;Creative Commons License Template&lt;/h3&gt;
&lt;p&gt;CC BY-SA 4.0 License with &lt;a href="https://creativecommons.org/licenses/by-sa/4.0/"&gt;link to license&lt;/a&gt; and placeholder for designer name.&lt;/p&gt;
&lt;p&gt;Devices using:
&lt;ul&gt;&lt;li&gt;FRAME_LEDGER&lt;/li&gt;
&lt;li&gt;FRAME_LETTER&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SFE_LOGO_NAME_FLAME_.2">
<description>&lt;h3&gt;SparkFun Font Logo w/ Flame - 0.2" Height - Silkscreen&lt;/h3&gt;
&lt;p&gt;SparkFun font logo with flame logo&lt;/p&gt;
&lt;p&gt;Devices using:
&lt;ul&gt;&lt;li&gt;SFE_LOGO_NAME_FLAME&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="OSHW-LOGO-S_COPPER">
<description>&lt;h3&gt;Open-Source Hardware (OSHW) Logo - Small - Top Copper&lt;/h3&gt;
&lt;p&gt;Exposed copper logo for open-source hardware designs.&lt;/p&gt;
&lt;p&gt;Devices using:
&lt;ul&gt;&lt;li&gt;OSHW_LOGO&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SFE_LOGO_FLAME_COPPER_.1">
<description>&lt;h3&gt;SparkFun Flame Logo - 0.1" Height - Top Copper&lt;/h3&gt;
&lt;p&gt;SparkFun Flame Logo&lt;/p&gt;
&lt;p&gt;Devices using:
&lt;ul&gt;&lt;li&gt;SFE_LOGO_FLAME&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SFE_LOGO_FLAME_.1">
<description>&lt;h3&gt;SparkFun Flame Logo - 0.1" Height - Silkscreen&lt;/h3&gt;
&lt;p&gt;SparkFun Flame Logo&lt;/p&gt;
&lt;p&gt;Devices using:
&lt;ul&gt;&lt;li&gt;SFE_LOGO_FLAME&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="OSHW-LOGO-S">
<description>&lt;h3&gt;Open-Source Hardware (OSHW) Logo - Small - Silkscreen&lt;/h3&gt;
&lt;p&gt;Silkscreen logo for open-source hardware designs.&lt;/p&gt;
&lt;p&gt;Devices using:
&lt;ul&gt;&lt;li&gt;OSHW_LOGO&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-IC-Microcontroller">
<description>&lt;h3&gt;SparkFun Microcontrollers&lt;/h3&gt;
This library contains microcontrollers.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="QFN-44-NOPAD_1:1">
</package>
</packages>
</library>
<library name="SparkFun-Displays">
<description>&lt;h3&gt;SparkFun Displays&lt;/h3&gt;
This library contains LCDs, OLEDs, etc. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OLED-0.66-64X48">
<description>&lt;h3&gt;OLDE display, 0.66 inch&lt;/h3&gt;
&lt;p&gt;For MicroView.&lt;/p&gt;

&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 28&lt;/li&gt;
&lt;li&gt;Pin pitch: &lt;/li&gt;
&lt;li&gt;Area: &lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Datasheet referenced for footprint:&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;Example device(s): 
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13003"&gt;Microview breakout&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Discrete Semiconductors&lt;/h3&gt;
This library contains diodes, optoisolators, TRIACs, MOSFETs, transistors, etc. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SMA-DIODE">
<description>&lt;B&gt;Diode&lt;/B&gt;
&lt;p&gt;Basic SMA packaged diode. Good for reverse polarization protection. Common part #: MBRA140&lt;/p&gt;
&lt;p&gt;SMA is the smallest package in the DO-214 standard (DO-214AC)&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-IC-Power">
<description>&lt;h3&gt;SparkFun Power Driver and Management ICs&lt;/h3&gt;
In this library you'll find anything that has to do with power delivery, or making power supplies.
&lt;p&gt;Contents:
&lt;ul&gt;&lt;li&gt;LDOs&lt;/li&gt;
&lt;li&gt;Boost/Buck controllers&lt;/li&gt;
&lt;li&gt;Charge pump controllers&lt;/li&gt;
&lt;li&gt;Power sequencers&lt;/li&gt;
&lt;li&gt;Power switches&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X3_TEST_POINTS">
<description>&lt;h3&gt;Plated Through Hole - 2x3 Test Point Header&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X04_1MM_RA">
<description>&lt;h3&gt;SMD- 4 Pin Right Angle &lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="JST-2-SMD">
<description>&lt;h3&gt;JST-Right Angle Male Header SMT&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 2mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://www.4uconnector.com/online/object/4udrawing/20404.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;li&gt;JST_2MM_MALE&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X02_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole - No Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X09_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole -9 Pin No Silk&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:9&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_09&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X07_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole -7 Pin  No Silk&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:7&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_07&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X06_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole - 6 Pin No Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X04_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole - 4 Pin No Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="USB-B-MICRO-SMD_RED_PASTE">
<description>&lt;h3&gt;USB - microB SMD Reduced Paste&lt;/h3&gt;
 70% paste area under D+ D- USBID pins for applications where those pins aren't required, to reduce the likelihood of bridges.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:5&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Micro-USB.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;USB_MICRO-B&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Fuses">
<description>&lt;h3&gt;SparkFun Fuses&lt;/h3&gt;
In this library you'll find fuses, or fuse like components such as PTCs. Reference designator F.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1206">
<description>&lt;p&gt;&lt;b&gt;Generic 3216 (1206) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603">
<description>&lt;p&gt;&lt;b&gt;Generic 1608 (0603) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun LEDs&lt;/h3&gt;
This library contains discrete LEDs for illumination or indication, but no displays.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-0603">
<description>&lt;B&gt;LED 0603 SMT&lt;/B&gt;&lt;p&gt;
0603, surface mount.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.075inch &lt;/li&gt;
&lt;li&gt;Area: 0.06" x 0.03"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;LED - BLUE&lt;/li&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Switches">
<description>&lt;h3&gt;SparkFun Switches, Buttons, Encoders&lt;/h3&gt;
In this library you'll find switches, buttons, joysticks, and anything that moves to create or disrupt an electrical connection.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SWITCH_SPST_SMD_A">
<description>&lt;h3&gt;SPDT Slide Switch - SMD&lt;/h3&gt;
&lt;p&gt;Single-pole, double-throw (SPDT) switch.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://cdn.sparkfun.com/datasheets/Components/Switches/SLIDE.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="TACTILE_SWITCH_SMD_4.6X2.8MM">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - SMD, 4.6 x 2.8mm&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.ck-components.com/media/1479/kmr2.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Capacitors&lt;/h3&gt;
This library contains capacitors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603">
<description>&lt;p&gt;&lt;b&gt;Generic 1608 (0603) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
<package name="1206">
<description>&lt;p&gt;&lt;b&gt;Generic 3216 (1206) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
<package name="0805">
<description>&lt;p&gt;&lt;b&gt;Generic 2012 (0805) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Jumpers">
<description>&lt;h3&gt;SparkFun Jumpers&lt;/h3&gt;
In this library you'll find jumpers, or other semipermanent means of changing current paths. The least permanent form is the solder jumper. These can be changed by adding, removing, or moving solder. In cases that are less likely to be changed we have jumpers that are connected with traces. These can be cut with a razor, or reconnected with solder. Reference designator JP.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SMT-JUMPER_3_2-NC_TRACE_SILK">
</package>
<package name="SMT-JUMPER_2_NC_PASTE_SILK">
</package>
</packages>
</library>
<library name="SparkFun-Clocks">
<description>&lt;h3&gt;SparkFun Clocks, Oscillators and Resonators&lt;/h3&gt;
This library contains the real-time clocks, oscillators, resonators, and crystals we use. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CRYSTAL-SMD-5X3.2-4PAD">
<description>&lt;h3&gt;5x3.2mm SMD Crystal&lt;/h3&gt;
&lt;p&gt;Example: &lt;a href="https://www.sparkfun.com/products/94"&gt;16MHz SMD Crystal&lt;/a&gt; (&lt;a href="https://www.sparkfun.com/datasheets/Components/SPK-5032-16MHZ.pdf"&gt;Datasheet&lt;/a&gt;)&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Hardware">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
This library contains board components that are not electrical in nature, such as stand-offs, magnets, and Actobotics. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="STAND-OFF">
<description>&lt;h3&gt;Standoff (#4 Screw)&lt;/h3&gt;
&lt;p&gt;This is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components.&lt;/p&gt;
&lt;h4&gt;Devices Using&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;STAND-OFF&lt;/li&gt;&lt;/ul&gt;</description>
</package>
</packages>
</library>
<library name="buzzard_labels">
<packages>
<package name="3V317">
</package>
<package name="RAW15">
</package>
<package name="RST16">
</package>
<package name="D120">
</package>
<package name="D111">
</package>
<package name="D102">
</package>
<package name="D93">
</package>
<package name="D84">
</package>
<package name="D75">
</package>
<package name="D66">
</package>
<package name="D57">
</package>
<package name="D48">
</package>
<package name="SCL18">
</package>
<package name="SDA19">
</package>
<package name="TX20">
</package>
<package name="RX21">
</package>
<package name="MISO22">
</package>
<package name="MOSI28">
</package>
<package name="SCK23">
</package>
<package name="A59">
</package>
<package name="A410">
</package>
<package name="A311">
</package>
<package name="A212">
</package>
<package name="A113">
</package>
<package name="A014">
</package>
<package name="GND38">
</package>
<package name="GND39">
</package>
<package name="RX36">
</package>
<package name="TX34">
</package>
<package name="STAT35">
</package>
<package name="CHG30">
</package>
<package name="BATT29">
</package>
<package name="#32">
</package>
<package name="#31">
</package>
<package name="_______39">
</package>
<package name="I2C_ADDR40">
</package>
<package name="I2C_PU39">
</package>
<package name="OP__##__0X3C42">
</package>
<package name="CL__##__0X3D41">
</package>
<package name="CHG#ON41">
</package>
<package name="V1044">
</package>
<package name="PRO_MICRO43">
</package>
<package name="MICRO_OLED42">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="FRAME1" library="SparkFun-Aesthetics" package="CREATIVE_COMMONS" value="FRAME-LETTER"/>
<element name="U1" library="SparkFun-IC-Microcontroller" package="QFN-44-NOPAD_1:1" value="32U4">
<attribute name="PROD_ID" value="IC-10828"/>
</element>
<element name="OLED1" library="SparkFun-Displays" package="OLED-0.66-64X48" value="OLED0.66">
<attribute name="PROD_ID" value="LCD-12019"/>
</element>
<element name="D5" library="SparkFun-DiscreteSemi" package="SMA-DIODE" value="3A/40V/500mV">
<attribute name="PROD_ID" value="DIO-09886"/>
</element>
<element name="3.3V_REG" library="SparkFun-IC-Power" package="SOT23-5" value="MIC5219 3.3V">
<attribute name="PROD_ID" value="VREG-09872"/>
</element>
<element name="BAT_CHARGE" library="SparkFun-IC-Power" package="SOT23-5" value="MCP73831">
<attribute name="PROD_ID" value="IC-09995"/>
</element>
<element name="ISP" library="SparkFun-Connectors" package="2X3_TEST_POINTS" value="AVR_SPI_PROG_3X2TESTPOINTS"/>
<element name="QWIIC" library="SparkFun-Connectors" package="1X04_1MM_RA" value="">
<attribute name="PROD_ID" value="CONN-13694"/>
<attribute name="VALUE"/>
</element>
<element name="F1" library="SparkFun-Fuses" package="1206" value="6V/0.5A">
<attribute name="PROD_ID" value="RES-08585"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="0603" value="330">
<attribute name="PROD_ID" value="RES-00818"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="0603" value="330">
<attribute name="PROD_ID" value="RES-00818"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="0603" value="330">
<attribute name="PROD_ID" value="RES-00818"/>
</element>
<element name="R6" library="SparkFun-Resistors" package="0603" value="330">
<attribute name="PROD_ID" value="RES-00818"/>
</element>
<element name="D1" library="SparkFun-LED" package="LED-0603" value="RED">
<attribute name="PROD_ID" value="DIO-00819"/>
</element>
<element name="D2" library="SparkFun-LED" package="LED-0603" value="RED">
<attribute name="PROD_ID" value="DIO-00819"/>
</element>
<element name="D3" library="SparkFun-LED" package="LED-0603" value="RED">
<attribute name="PROD_ID" value="DIO-00819"/>
</element>
<element name="D4" library="SparkFun-LED" package="LED-0603" value="RED">
<attribute name="PROD_ID" value="DIO-00819"/>
</element>
<element name="R7" library="SparkFun-Resistors" package="0603" value="10k">
<attribute name="PROD_ID" value="RES-00824"/>
</element>
<element name="R9" library="SparkFun-Resistors" package="0603" value="10k">
<attribute name="PROD_ID" value="RES-00824"/>
</element>
<element name="R8" library="SparkFun-Resistors" package="0603" value="10k">
<attribute name="PROD_ID" value="RES-00824"/>
</element>
<element name="S1" library="SparkFun-Switches" package="SWITCH_SPST_SMD_A" value="">
<attribute name="PROD_ID" value="SWCH-10651"/>
<attribute name="SF_SKU" value="COM-10860"/>
<attribute name="VALUE"/>
</element>
<element name="S2" library="SparkFun-Switches" package="TACTILE_SWITCH_SMD_4.6X2.8MM" value="MOMENTARY-SWITCH-SPST-SMD-4.6X2.8MM">
<attribute name="PROD_ID" value="SWCH-13065"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0603" value="22">
<attribute name="PROD_ID" value="RES-08698"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0603" value="22">
<attribute name="PROD_ID" value="RES-08698"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="0603" value="470pF">
<attribute name="PROD_ID" value="CAP-07884"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="1206" value="4.7uF">
<attribute name="PROD_ID" value="CAP-10300"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="1206" value="4.7uF">
<attribute name="PROD_ID" value="CAP-10300"/>
</element>
<element name="C12" library="SparkFun-Capacitors" package="1206" value="4.7uF">
<attribute name="PROD_ID" value="CAP-10300"/>
</element>
<element name="JST" library="SparkFun-Connectors" package="JST-2-SMD" value="">
<attribute name="PROD_ID" value="CONN-11443"/>
<attribute name="SF_ID" value="PRT-08612"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="SparkFun-Capacitors" package="0603" value="0.1uF">
<attribute name="PROD_ID" value="CAP-00810"/>
</element>
<element name="C13" library="SparkFun-Capacitors" package="0603" value="0.1uF">
<attribute name="PROD_ID" value="CAP-00810"/>
</element>
<element name="C10" library="SparkFun-Capacitors" package="0603" value="1.0uF">
<attribute name="PROD_ID" value="CAP-00868"/>
</element>
<element name="C14" library="SparkFun-Capacitors" package="0603" value="1.0uF">
<attribute name="PROD_ID" value="CAP-00868"/>
</element>
<element name="C7" library="SparkFun-Capacitors" package="0603" value="1.0uF">
<attribute name="PROD_ID" value="CAP-00868"/>
</element>
<element name="C5" library="SparkFun-Capacitors" package="0805" value="1.0uF">
<attribute name="PROD_ID" value="CAP-08064"/>
</element>
<element name="C6" library="SparkFun-Capacitors" package="0805" value="1.0uF">
<attribute name="PROD_ID" value="CAP-08064"/>
</element>
<element name="R13" library="SparkFun-Resistors" package="0603" value="390k">
<attribute name="PROD_ID" value="RES-12024"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="0805" value="2.2uF">
<attribute name="PROD_ID" value="CAP-11624"/>
</element>
<element name="JP1" library="SparkFun-Jumpers" package="SMT-JUMPER_3_2-NC_TRACE_SILK" value="JUMPER-SMT_3_2-NC_TRACE_SILK"/>
<element name="R11" library="SparkFun-Resistors" package="0603" value="4.7k">
<attribute name="PROD_ID" value="RES-07857"/>
</element>
<element name="R12" library="SparkFun-Resistors" package="0603" value="4.7k">
<attribute name="PROD_ID" value="RES-07857"/>
</element>
<element name="JP2" library="SparkFun-Jumpers" package="SMT-JUMPER_2_NC_PASTE_SILK" value="JUMPER-SMT_2_NC_PASTE_SILK"/>
<element name="R10" library="SparkFun-Resistors" package="0603" value="10k">
<attribute name="PROD_ID" value="RES-00824"/>
</element>
<element name="PTH" library="SparkFun-Connectors" package="1X02_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="DIG" library="SparkFun-Connectors" package="1X09_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="DIG_GND" library="SparkFun-Connectors" package="1X09_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="COMM" library="SparkFun-Connectors" package="1X07_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="COMM_GND" library="SparkFun-Connectors" package="1X07_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="ANALOG" library="SparkFun-Connectors" package="1X06_NO_SILK" value="">
<attribute name="PROD_ID" value="CONN-08437"/>
<attribute name="VALUE"/>
</element>
<element name="ANALOG_GND" library="SparkFun-Connectors" package="1X06_NO_SILK" value="">
<attribute name="PROD_ID" value="CONN-08437"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="SparkFun-Capacitors" package="0603" value="22pF">
<attribute name="PROD_ID" value="CAP-07876"/>
</element>
<element name="C8" library="SparkFun-Capacitors" package="0603" value="22pF">
<attribute name="PROD_ID" value="CAP-07876"/>
</element>
<element name="Y1" library="SparkFun-Clocks" package="CRYSTAL-SMD-5X3.2-4PAD" value="8MHz">
<attribute name="PROD_ID" value="XTAL-09431"/>
</element>
<element name="LOGO1" library="SparkFun-Aesthetics" package="SFE_LOGO_NAME_FLAME_.2" value="SFE_LOGO_NAME_FLAME.2_INCH"/>
<element name="LOGO2" library="SparkFun-Aesthetics" package="OSHW-LOGO-S_COPPER" value="OSHW-LOGOS-COPPER"/>
<element name="LOGO3" library="SparkFun-Aesthetics" package="SFE_LOGO_FLAME_COPPER_.1" value="SFE_LOGO_FLAME.1COP"/>
<element name="H1" library="SparkFun-Hardware" package="STAND-OFF" value="STAND-OFF"/>
<element name="H2" library="SparkFun-Hardware" package="STAND-OFF" value="STAND-OFF"/>
<element name="PWR" library="SparkFun-Connectors" package="1X04_NO_SILK" value="">
<attribute name="PROD_ID" value="CONN-09696"/>
<attribute name="VALUE"/>
</element>
<element name="PWR_GND" library="SparkFun-Connectors" package="1X04_NO_SILK" value="">
<attribute name="PROD_ID" value="CONN-09696"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="USB-B-MICRO-SMD_RED_PASTE" value="">
<attribute name="PROD_ID" value="CONN-11752"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="buzzard_labels" package="3V317" value="3V317"/>
<element name="U$2" library="buzzard_labels" package="3V317" value="3V317"/>
<element name="U$3" library="buzzard_labels" package="3V317" value="3V317"/>
<element name="U$4" library="buzzard_labels" package="3V317" value="3V317"/>
<element name="U$5" library="buzzard_labels" package="RAW15" value="RAW15"/>
<element name="U$6" library="buzzard_labels" package="RAW15" value="RAW15"/>
<element name="U$7" library="buzzard_labels" package="RST16" value="RST16"/>
<element name="U$8" library="buzzard_labels" package="RST16" value="RST16"/>
<element name="U$9" library="buzzard_labels" package="D120" value="D120"/>
<element name="U$10" library="buzzard_labels" package="D120" value="D120"/>
<element name="U$11" library="buzzard_labels" package="D111" value="D111"/>
<element name="U$12" library="buzzard_labels" package="D111" value="D111"/>
<element name="U$13" library="buzzard_labels" package="D102" value="D102"/>
<element name="U$14" library="buzzard_labels" package="D102" value="D102"/>
<element name="U$15" library="buzzard_labels" package="D93" value="D93"/>
<element name="U$16" library="buzzard_labels" package="D93" value="D93"/>
<element name="U$17" library="buzzard_labels" package="D84" value="D84"/>
<element name="U$18" library="buzzard_labels" package="D84" value="D84"/>
<element name="U$19" library="buzzard_labels" package="D75" value="D75"/>
<element name="U$20" library="buzzard_labels" package="D75" value="D75"/>
<element name="U$21" library="buzzard_labels" package="D66" value="D66"/>
<element name="U$22" library="buzzard_labels" package="D66" value="D66"/>
<element name="U$23" library="buzzard_labels" package="D57" value="D57"/>
<element name="U$24" library="buzzard_labels" package="D57" value="D57"/>
<element name="U$25" library="buzzard_labels" package="D48" value="D48"/>
<element name="U$26" library="buzzard_labels" package="D48" value="D48"/>
<element name="U$27" library="buzzard_labels" package="SCL18" value="SCL18"/>
<element name="U$28" library="buzzard_labels" package="SCL18" value="SCL18"/>
<element name="U$29" library="buzzard_labels" package="SDA19" value="SDA19"/>
<element name="U$30" library="buzzard_labels" package="SDA19" value="SDA19"/>
<element name="U$31" library="buzzard_labels" package="TX20" value="TX20"/>
<element name="U$32" library="buzzard_labels" package="TX20" value="TX20"/>
<element name="U$33" library="buzzard_labels" package="RX21" value="RX21"/>
<element name="U$34" library="buzzard_labels" package="RX21" value="RX21"/>
<element name="U$35" library="buzzard_labels" package="MISO22" value="MISO22"/>
<element name="U$36" library="buzzard_labels" package="MISO22" value="MISO22"/>
<element name="U$37" library="buzzard_labels" package="MOSI28" value="MOSI28"/>
<element name="U$38" library="buzzard_labels" package="MOSI28" value="MOSI28"/>
<element name="U$39" library="buzzard_labels" package="SCK23" value="SCK23"/>
<element name="U$40" library="buzzard_labels" package="SCK23" value="SCK23"/>
<element name="U$41" library="buzzard_labels" package="A59" value="A59"/>
<element name="U$42" library="buzzard_labels" package="A59" value="A59"/>
<element name="U$43" library="buzzard_labels" package="A410" value="A410"/>
<element name="U$44" library="buzzard_labels" package="A410" value="A410"/>
<element name="U$45" library="buzzard_labels" package="A311" value="A311"/>
<element name="U$46" library="buzzard_labels" package="A311" value="A311"/>
<element name="U$47" library="buzzard_labels" package="A212" value="A212"/>
<element name="U$48" library="buzzard_labels" package="A212" value="A212"/>
<element name="U$49" library="buzzard_labels" package="A113" value="A113"/>
<element name="U$50" library="buzzard_labels" package="A113" value="A113"/>
<element name="U$51" library="buzzard_labels" package="A014" value="A014"/>
<element name="U$52" library="buzzard_labels" package="A014" value="A014"/>
<element name="U$53" library="buzzard_labels" package="GND38" value="GND38"/>
<element name="U$54" library="buzzard_labels" package="GND38" value="GND38"/>
<element name="U$55" library="buzzard_labels" package="GND39" value="GND39"/>
<element name="U$56" library="buzzard_labels" package="GND39" value="GND39"/>
<element name="U$57" library="buzzard_labels" package="RX36" value="RX36"/>
<element name="U$58" library="buzzard_labels" package="TX34" value="TX34"/>
<element name="U$59" library="buzzard_labels" package="STAT35" value="STAT35"/>
<element name="U$60" library="buzzard_labels" package="CHG30" value="CHG30"/>
<element name="U$61" library="buzzard_labels" package="BATT29" value="BATT29"/>
<element name="U$62" library="buzzard_labels" package="#32" value="#32"/>
<element name="U$63" library="buzzard_labels" package="#31" value="#31"/>
<element name="U$66" library="buzzard_labels" package="_______39" value="_______39"/>
<element name="U$67" library="buzzard_labels" package="_______39" value="_______39"/>
<element name="U$68" library="buzzard_labels" package="_______39" value="_______39"/>
<element name="U$69" library="buzzard_labels" package="_______39" value="_______39"/>
<element name="U$70" library="buzzard_labels" package="_______39" value="_______39"/>
<element name="U$71" library="buzzard_labels" package="_______39" value="_______39"/>
<element name="U$72" library="buzzard_labels" package="_______39" value="_______39"/>
<element name="U$73" library="buzzard_labels" package="_______39" value="_______39"/>
<element name="U$74" library="buzzard_labels" package="_______39" value="_______39"/>
<element name="U$75" library="buzzard_labels" package="_______39" value="_______39"/>
<element name="U$76" library="buzzard_labels" package="_______39" value="_______39"/>
<element name="U$77" library="buzzard_labels" package="_______39" value="_______39"/>
<element name="U$78" library="buzzard_labels" package="_______39" value="_______39"/>
<element name="U$79" library="buzzard_labels" package="_______39" value="_______39"/>
<element name="U$80" library="buzzard_labels" package="_______39" value="_______39"/>
<element name="U$81" library="buzzard_labels" package="_______39" value="_______39"/>
<element name="U$82" library="buzzard_labels" package="_______39" value="_______39"/>
<element name="U$83" library="buzzard_labels" package="_______39" value="_______39"/>
<element name="U$84" library="buzzard_labels" package="_______39" value="_______39"/>
<element name="U$85" library="buzzard_labels" package="_______39" value="_______39"/>
<element name="U$86" library="buzzard_labels" package="_______39" value="_______39"/>
<element name="U$87" library="buzzard_labels" package="_______39" value="_______39"/>
<element name="U$88" library="buzzard_labels" package="_______39" value="_______39"/>
<element name="U$89" library="buzzard_labels" package="_______39" value="_______39"/>
<element name="U$90" library="buzzard_labels" package="_______39" value="_______39"/>
<element name="U$91" library="buzzard_labels" package="_______39" value="_______39"/>
<element name="U$92" library="buzzard_labels" package="_______39" value="_______39"/>
<element name="U$93" library="buzzard_labels" package="_______39" value="_______39"/>
<element name="U$94" library="buzzard_labels" package="_______39" value="_______39"/>
<element name="U$95" library="buzzard_labels" package="_______39" value="_______39"/>
<element name="U$96" library="buzzard_labels" package="_______39" value="_______39"/>
<element name="U$97" library="buzzard_labels" package="_______39" value="_______39"/>
<element name="U$98" library="buzzard_labels" package="_______39" value="_______39"/>
<element name="U$99" library="buzzard_labels" package="_______39" value="_______39"/>
<element name="U$100" library="buzzard_labels" package="_______39" value="_______39"/>
<element name="U$101" library="buzzard_labels" package="_______39" value="_______39"/>
<element name="U$102" library="buzzard_labels" package="_______39" value="_______39"/>
<element name="U$103" library="buzzard_labels" package="_______39" value="_______39"/>
<element name="U$104" library="buzzard_labels" package="_______39" value="_______39"/>
<element name="U$105" library="buzzard_labels" package="_______39" value="_______39"/>
<element name="U$106" library="buzzard_labels" package="_______39" value="_______39"/>
<element name="U$107" library="buzzard_labels" package="_______39" value="_______39"/>
<element name="U$108" library="buzzard_labels" package="_______39" value="_______39"/>
<element name="U$109" library="buzzard_labels" package="_______39" value="_______39"/>
<element name="U$110" library="buzzard_labels" package="_______39" value="_______39"/>
<element name="U$111" library="buzzard_labels" package="_______39" value="_______39"/>
<element name="U$112" library="buzzard_labels" package="_______39" value="_______39"/>
<element name="U$113" library="buzzard_labels" package="_______39" value="_______39"/>
<element name="U$114" library="buzzard_labels" package="_______39" value="_______39"/>
<element name="U$115" library="buzzard_labels" package="_______39" value="_______39"/>
<element name="U$116" library="buzzard_labels" package="_______39" value="_______39"/>
<element name="U$117" library="buzzard_labels" package="_______39" value="_______39"/>
<element name="U$118" library="buzzard_labels" package="I2C_ADDR40" value="I2C_ADDR40"/>
<element name="U$119" library="buzzard_labels" package="I2C_PU39" value="I2C_PU39"/>
<element name="U$120" library="buzzard_labels" package="OP__##__0X3C42" value="OP__##__0X3C42"/>
<element name="U$121" library="buzzard_labels" package="CL__##__0X3D41" value="CL__##__0X3D41"/>
<element name="U$123" library="buzzard_labels" package="RST16" value="RST16"/>
<element name="U$122" library="buzzard_labels" package="CHG#ON41" value="CHG#ON41"/>
<element name="U$124" library="buzzard_labels" package="V1044" value="V1044"/>
<element name="U$64" library="buzzard_labels" package="PRO_MICRO43" value="PRO_MICRO43"/>
<element name="U$65" library="buzzard_labels" package="MICRO_OLED42" value="MICRO_OLED42"/>
<element name="LOGO4" library="SparkFun-Aesthetics" package="SFE_LOGO_FLAME_.1" value="SFE_LOGO_FLAME.1_INCH"/>
<element name="LOGO5" library="SparkFun-Aesthetics" package="OSHW-LOGO-S" value="OSHW-LOGOS"/>
</elements>
<signals>
<signal name="N$2">
<contactref element="BAT_CHARGE" pad="4"/>
<contactref element="R3" pad="2"/>
<contactref element="F1" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="R3" pad="1"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="N$4">
<contactref element="D1" pad="C"/>
<contactref element="BAT_CHARGE" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="3.3V_REG" pad="3"/>
<contactref element="S1" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="R2" pad="1"/>
<contactref element="J1" pad="D+"/>
</signal>
<signal name="N$10">
<contactref element="R1" pad="1"/>
<contactref element="J1" pad="D-"/>
</signal>
<signal name="V_USB">
<contactref element="F1" pad="1"/>
<contactref element="U1" pad="7"/>
<contactref element="U1" pad="2"/>
<contactref element="C13" pad="1"/>
<contactref element="J1" pad="VBUS"/>
<contactref element="S1" pad="3"/>
<contactref element="D5" pad="C"/>
<contactref element="3.3V_REG" pad="1"/>
<contactref element="PWR" pad="4"/>
</signal>
<signal name="D-">
<contactref element="R1" pad="2"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="D+">
<contactref element="R2" pad="2"/>
<contactref element="U1" pad="4"/>
</signal>
<signal name="GND">
<contactref element="S1" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="S2" pad="4"/>
<contactref element="S2" pad="3"/>
<contactref element="C11" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="U1" pad="33"/>
<contactref element="U1" pad="5"/>
<contactref element="U1" pad="15"/>
<contactref element="U1" pad="23"/>
<contactref element="U1" pad="35"/>
<contactref element="U1" pad="43"/>
<contactref element="D4" pad="C"/>
<contactref element="D3" pad="C"/>
<contactref element="D2" pad="C"/>
<contactref element="ISP" pad="6"/>
<contactref element="C7" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="R13" pad="1"/>
<contactref element="JST" pad="1"/>
<contactref element="C12" pad="2"/>
<contactref element="QWIIC" pad="1"/>
<contactref element="C14" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="JP2" pad="1"/>
<contactref element="PTH" pad="2"/>
<contactref element="OLED1" pad="10"/>
<contactref element="OLED1" pad="1"/>
<contactref element="OLED1" pad="28"/>
<contactref element="OLED1" pad="27"/>
<contactref element="OLED1" pad="7"/>
<contactref element="ANALOG_GND" pad="1"/>
<contactref element="ANALOG_GND" pad="2"/>
<contactref element="ANALOG_GND" pad="3"/>
<contactref element="ANALOG_GND" pad="4"/>
<contactref element="ANALOG_GND" pad="5"/>
<contactref element="ANALOG_GND" pad="6"/>
<contactref element="COMM_GND" pad="1"/>
<contactref element="COMM_GND" pad="2"/>
<contactref element="COMM_GND" pad="3"/>
<contactref element="COMM_GND" pad="4"/>
<contactref element="COMM_GND" pad="5"/>
<contactref element="COMM_GND" pad="6"/>
<contactref element="COMM_GND" pad="7"/>
<contactref element="DIG_GND" pad="1"/>
<contactref element="DIG_GND" pad="2"/>
<contactref element="DIG_GND" pad="3"/>
<contactref element="DIG_GND" pad="4"/>
<contactref element="DIG_GND" pad="5"/>
<contactref element="DIG_GND" pad="6"/>
<contactref element="DIG_GND" pad="7"/>
<contactref element="DIG_GND" pad="8"/>
<contactref element="DIG_GND" pad="9"/>
<contactref element="C9" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="PWR_GND" pad="4"/>
<contactref element="PWR_GND" pad="3"/>
<contactref element="PWR_GND" pad="2"/>
<contactref element="PWR_GND" pad="1"/>
<contactref element="J1" pad="GND"/>
</signal>
<signal name="V_BAT">
<contactref element="BAT_CHARGE" pad="3"/>
<contactref element="D5" pad="A"/>
<contactref element="JST" pad="2"/>
<contactref element="C12" pad="1"/>
<contactref element="PTH" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="3.3V_REG" pad="4"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="3.3V">
<contactref element="3.3V_REG" pad="5"/>
<contactref element="C2" pad="1"/>
<contactref element="U1" pad="44"/>
<contactref element="R9" pad="2"/>
<contactref element="ISP" pad="2"/>
<contactref element="OLED1" pad="6"/>
<contactref element="OLED1" pad="8"/>
<contactref element="R8" pad="2"/>
<contactref element="OLED1" pad="9"/>
<contactref element="QWIIC" pad="2"/>
<contactref element="C14" pad="1"/>
<contactref element="JP1" pad="2"/>
<contactref element="R10" pad="2"/>
<contactref element="U1" pad="24"/>
<contactref element="U1" pad="14"/>
<contactref element="U1" pad="34"/>
<contactref element="PWR" pad="2"/>
<contactref element="PWR" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="BAT_CHARGE" pad="5"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="BAT_CHARGE" pad="2"/>
<contactref element="R7" pad="2"/>
<contactref element="3.3V_REG" pad="2"/>
</signal>
<signal name="!RESET">
<contactref element="S2" pad="1"/>
<contactref element="S2" pad="2"/>
<contactref element="R9" pad="1"/>
<contactref element="U1" pad="13"/>
<contactref element="ISP" pad="5"/>
<contactref element="PWR" pad="3"/>
</signal>
<signal name="N$11">
<contactref element="U1" pad="42"/>
<contactref element="C11" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="U1" pad="6"/>
<contactref element="C10" pad="1"/>
</signal>
<signal name="A0">
<contactref element="U1" pad="36"/>
<contactref element="ANALOG" pad="1"/>
</signal>
<signal name="A1">
<contactref element="U1" pad="37"/>
<contactref element="ANALOG" pad="2"/>
</signal>
<signal name="A2">
<contactref element="U1" pad="38"/>
<contactref element="ANALOG" pad="3"/>
</signal>
<signal name="A3">
<contactref element="U1" pad="39"/>
<contactref element="ANALOG" pad="4"/>
</signal>
<signal name="A4">
<contactref element="U1" pad="40"/>
<contactref element="ANALOG" pad="5"/>
</signal>
<signal name="A5">
<contactref element="U1" pad="41"/>
<contactref element="ANALOG" pad="6"/>
</signal>
<signal name="RXI">
<contactref element="U1" pad="20"/>
<contactref element="COMM" pad="4"/>
</signal>
<signal name="TXO">
<contactref element="U1" pad="21"/>
<contactref element="COMM" pad="5"/>
</signal>
<signal name="SDA">
<contactref element="U1" pad="19"/>
<contactref element="OLED1" pad="18"/>
<contactref element="OLED1" pad="17"/>
<contactref element="QWIIC" pad="3"/>
<contactref element="R11" pad="1"/>
<contactref element="COMM" pad="6"/>
</signal>
<signal name="SCL">
<contactref element="U1" pad="18"/>
<contactref element="OLED1" pad="16"/>
<contactref element="QWIIC" pad="4"/>
<contactref element="R12" pad="1"/>
<contactref element="COMM" pad="7"/>
</signal>
<signal name="D4">
<contactref element="U1" pad="25"/>
<contactref element="DIG" pad="9"/>
</signal>
<signal name="D5">
<contactref element="U1" pad="31"/>
<contactref element="DIG" pad="8"/>
</signal>
<signal name="D6">
<contactref element="U1" pad="27"/>
<contactref element="DIG" pad="7"/>
</signal>
<signal name="D7">
<contactref element="U1" pad="1"/>
<contactref element="DIG" pad="6"/>
</signal>
<signal name="SCK">
<contactref element="U1" pad="9"/>
<contactref element="ISP" pad="3"/>
<contactref element="COMM" pad="1"/>
</signal>
<signal name="MOSI">
<contactref element="U1" pad="10"/>
<contactref element="ISP" pad="4"/>
<contactref element="COMM" pad="2"/>
</signal>
<signal name="MISO">
<contactref element="U1" pad="11"/>
<contactref element="ISP" pad="1"/>
<contactref element="COMM" pad="3"/>
</signal>
<signal name="N$17">
<contactref element="U1" pad="22"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$18">
<contactref element="U1" pad="8"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="N$19">
<contactref element="U1" pad="32"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="N$20">
<contactref element="R4" pad="1"/>
<contactref element="D2" pad="A"/>
</signal>
<signal name="N$21">
<contactref element="R5" pad="1"/>
<contactref element="D3" pad="A"/>
</signal>
<signal name="N$22">
<contactref element="R6" pad="1"/>
<contactref element="D4" pad="A"/>
</signal>
<signal name="D12">
<contactref element="U1" pad="26"/>
<contactref element="DIG" pad="1"/>
</signal>
<signal name="D8">
<contactref element="U1" pad="28"/>
<contactref element="DIG" pad="5"/>
</signal>
<signal name="D/!C">
<contactref element="OLED1" pad="13"/>
<contactref element="JP2" pad="2"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="OLED1" pad="12"/>
<contactref element="R8" pad="1"/>
<contactref element="C7" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="OLED1" pad="26"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="OLED1" pad="25"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="N$23">
<contactref element="OLED1" pad="24"/>
<contactref element="R13" pad="2"/>
</signal>
<signal name="N$24">
<contactref element="OLED1" pad="3"/>
<contactref element="C5" pad="2"/>
</signal>
<signal name="N$25">
<contactref element="OLED1" pad="2"/>
<contactref element="C5" pad="1"/>
</signal>
<signal name="N$26">
<contactref element="OLED1" pad="4"/>
<contactref element="C6" pad="1"/>
</signal>
<signal name="N$27">
<contactref element="OLED1" pad="5"/>
<contactref element="C6" pad="2"/>
</signal>
<signal name="R/!W">
<contactref element="OLED1" pad="14"/>
</signal>
<signal name="E/!RD">
<contactref element="OLED1" pad="15"/>
</signal>
<signal name="O_D3">
<contactref element="OLED1" pad="19"/>
</signal>
<signal name="O_D4">
<contactref element="OLED1" pad="20"/>
</signal>
<signal name="O_D5">
<contactref element="OLED1" pad="21"/>
</signal>
<signal name="O_D6">
<contactref element="OLED1" pad="22"/>
</signal>
<signal name="O_D7">
<contactref element="OLED1" pad="23"/>
</signal>
<signal name="N$28">
<contactref element="JP1" pad="1"/>
<contactref element="R12" pad="2"/>
</signal>
<signal name="N$29">
<contactref element="JP1" pad="3"/>
<contactref element="R11" pad="2"/>
</signal>
<signal name="D11">
<contactref element="U1" pad="12"/>
<contactref element="DIG" pad="2"/>
</signal>
<signal name="D10">
<contactref element="U1" pad="30"/>
<contactref element="DIG" pad="3"/>
</signal>
<signal name="D9">
<contactref element="U1" pad="29"/>
<contactref element="DIG" pad="4"/>
</signal>
<signal name="N$8">
<contactref element="U1" pad="17"/>
<contactref element="Y1" pad="3"/>
<contactref element="C9" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="Y1" pad="1"/>
<contactref element="U1" pad="16"/>
<contactref element="C8" pad="2"/>
</signal>
<signal name="N$30">
</signal>
<signal name="!CS">
<contactref element="OLED1" pad="11"/>
</signal>
<signal name="N$32">
</signal>
<signal name="N$35">
</signal>
<signal name="N$36">
</signal>
<signal name="N$37">
</signal>
<signal name="N$38">
</signal>
<signal name="N$39">
</signal>
<signal name="N$40">
</signal>
<signal name="N$41">
</signal>
<signal name="N$44">
</signal>
<signal name="N$45">
</signal>
<signal name="SHIELD">
<contactref element="J1" pad="SHIELD2"/>
<contactref element="J1" pad="SHIELD1"/>
<contactref element="J1" pad="SHIELD3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
