<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="56.94325" y1="33.019340625" x2="4.01228125" y2="33.010659375" width="0" layer="20"/>
<wire x1="4.01228125" y1="33.010659375" x2="0" y2="28.99771875" width="0" layer="20" curve="89.893424"/>
<wire x1="0" y1="28.99771875" x2="0" y2="3.81" width="0" layer="20"/>
<wire x1="0" y1="3.81" x2="3.81" y2="0" width="0" layer="20" curve="90"/>
<wire x1="3.81" y1="0" x2="57.15" y2="0" width="0" layer="20"/>
<wire x1="57.15" y1="0" x2="60.96" y2="3.81" width="0" layer="20" curve="90"/>
<wire x1="60.96" y1="3.81" x2="60.96" y2="29.00325" width="0" layer="20"/>
<wire x1="60.96" y1="29.00325" x2="56.94325" y2="33.019340625" width="0" layer="20" curve="90.009407"/>
<hole x="3.81" y="3.81" drill="3.175"/>
<hole x="57.15" y="3.81" drill="3.175"/>
<hole x="3.81" y="29.21" drill="3.175"/>
<hole x="57.15" y="29.21" drill="3.175"/>
<text>ATtiny85</text>
<text>ATtiny84</text>
<text>ATtiny2313</text>
<text>ATmega328p</text>
<text>ATmega328p</text>
<text>ATmega328p</text>
<text>ATtiny2313</text>
<text>ATtiny84</text>
<text>ATtiny85</text>
<text>Pin 1 -&gt;</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DIL28-3-ZIF_SOCKET">
</package>
<package name="FTDI_DEVICE_SIDE">
<description>Package for devices meant to mate to an FTDI connector.</description>
</package>
</packages>
</library>
<library name="barbary_enterprises">
<packages>
<package name="2X3-NS">
</package>
<package name="CAP-PTH-SMALL">
</package>
<package name="AXIAL-0.3">
</package>
</packages>
</library>
<library name="SparkFun-FreqCtrl">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find crystals and oscillators and other things that go "tick".&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="RESONATOR-PTH">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="SparkFun-Connectors" package="DIL28-3-ZIF_SOCKET" value="ZIFSOCKET-28-3ZIFFSOCKET-28-3"/>
<element name="ATMEGA328" library="barbary_enterprises" package="2X3-NS" value="AVR_SPI_PRG_6LABELED"/>
<element name="JP1" library="SparkFun-Connectors" package="FTDI_DEVICE_SIDE" value="FTDI_DEVICE"/>
<element name="C1" library="barbary_enterprises" package="CAP-PTH-SMALL" value=""/>
<element name="R1" library="barbary_enterprises" package="AXIAL-0.3" value=""/>
<element name="Y1" library="SparkFun-FreqCtrl" package="RESONATOR-PTH" value=""/>
<element name="ATTINY85" library="barbary_enterprises" package="2X3-NS" value="AVR_SPI_PRG_6LABELED"/>
<element name="ATTINY84" library="barbary_enterprises" package="2X3-NS" value="AVR_SPI_PRG_6LABELED"/>
<element name="ATTINY2313" library="barbary_enterprises" package="2X3-NS" value="AVR_SPI_PRG_6LABELED"/>
</elements>
<signals>
<signal name="P15">
<contactref element="U$1" pad="15"/>
</signal>
<signal name="P16">
<contactref element="U$1" pad="16"/>
</signal>
<signal name="P21">
<contactref element="U$1" pad="21"/>
</signal>
<signal name="P23">
<contactref element="U$1" pad="23"/>
<contactref element="ATTINY84" pad="3"/>
</signal>
<signal name="P24">
<contactref element="U$1" pad="24"/>
</signal>
<signal name="P25">
<contactref element="U$1" pad="25"/>
<contactref element="ATTINY85" pad="4"/>
<contactref element="ATTINY2313" pad="4"/>
</signal>
<signal name="P27">
<contactref element="U$1" pad="27"/>
<contactref element="ATTINY85" pad="3"/>
<contactref element="ATTINY2313" pad="3"/>
</signal>
<signal name="P28">
<contactref element="U$1" pad="28"/>
<contactref element="ATTINY85" pad="2"/>
<contactref element="ATTINY84" pad="6"/>
<contactref element="ATTINY2313" pad="2"/>
</signal>
<signal name="P2">
<contactref element="U$1" pad="2"/>
<contactref element="JP1" pad="P$3"/>
</signal>
<signal name="P4">
<contactref element="U$1" pad="4"/>
<contactref element="ATTINY85" pad="6"/>
<contactref element="ATTINY84" pad="5"/>
</signal>
<signal name="P5">
<contactref element="U$1" pad="5"/>
</signal>
<signal name="P6">
<contactref element="U$1" pad="6"/>
</signal>
<signal name="P12">
<contactref element="U$1" pad="12"/>
</signal>
<signal name="P13">
<contactref element="U$1" pad="13"/>
</signal>
<signal name="P14">
<contactref element="U$1" pad="14"/>
</signal>
<signal name="P17">
<contactref element="ATMEGA328" pad="4"/>
<contactref element="U$1" pad="17"/>
</signal>
<signal name="P7">
<contactref element="ATMEGA328" pad="2"/>
<contactref element="U$1" pad="7"/>
<contactref element="JP1" pad="P$4"/>
<contactref element="R1" pad="P$2"/>
<contactref element="ATTINY84" pad="4"/>
</signal>
<signal name="P18">
<contactref element="ATMEGA328" pad="1"/>
<contactref element="U$1" pad="18"/>
</signal>
<signal name="P19">
<contactref element="ATMEGA328" pad="3"/>
<contactref element="U$1" pad="19"/>
</signal>
<signal name="P1">
<contactref element="ATMEGA328" pad="5"/>
<contactref element="U$1" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="R1" pad="P$1"/>
<contactref element="ATTINY85" pad="5"/>
<contactref element="ATTINY84" pad="2"/>
<contactref element="ATTINY2313" pad="5"/>
</signal>
<signal name="DTR">
<contactref element="JP1" pad="P$1"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="P3">
<contactref element="U$1" pad="3"/>
<contactref element="JP1" pad="P$2"/>
</signal>
<signal name="P8">
<contactref element="U$1" pad="8"/>
<contactref element="ATMEGA328" pad="6"/>
<contactref element="JP1" pad="P$5"/>
<contactref element="Y1" pad="2"/>
<contactref element="JP1" pad="P$6"/>
</signal>
<signal name="P9">
<contactref element="U$1" pad="9"/>
<contactref element="Y1" pad="1"/>
</signal>
<signal name="P10">
<contactref element="U$1" pad="10"/>
<contactref element="ATTINY2313" pad="6"/>
<contactref element="Y1" pad="3"/>
</signal>
<signal name="P11">
<contactref element="U$1" pad="11"/>
</signal>
<signal name="P20">
<contactref element="U$1" pad="20"/>
</signal>
<signal name="P22">
<contactref element="U$1" pad="22"/>
<contactref element="ATTINY84" pad="1"/>
</signal>
<signal name="P26">
<contactref element="U$1" pad="26"/>
<contactref element="ATTINY85" pad="1"/>
<contactref element="ATTINY2313" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
