<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="8.55" y1="11.176" x2="29.55" y2="11.176" width="0" layer="20"/>
<wire x1="29.55" y1="11.176" x2="29.55" y2="45.51" width="0" layer="20"/>
<wire x1="29.55" y1="45.51" x2="8.55" y2="45.51" width="0" layer="20"/>
<wire x1="8.55" y1="45.51" x2="8.55" y2="11.176" width="0" layer="20"/>
<text>1A</text>
<text>2A</text>
<text>VCC</text>
<text>GND</text>
<text>3A</text>
<text>4A</text>
<text>3,4
EN</text>
<text>1,2
EN</text>
<text>2Y</text>
<text>1Y</text>
<text>3Y</text>
<text>4Y</text>
<text>GND</text>
<text>VCC2</text>
<text>L293NE
Quad Half-H Driver
Breakout v1</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SCREWTERMINAL-3.5MM-2">
</package>
<package name="1X08_ROUND">
</package>
</packages>
</library>
<library name="Darryl">
<packages>
<package name="DIP254P762X508-16">
</package>
<package name="DIODE-STICKUP">
</package>
</packages>
</library>
<library name="Pictures">
<packages>
<package name="CREATIVE_COMMONS">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-2" value="M023.5MM"/>
<element name="JP2" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-2" value="M023.5MM"/>
<element name="JP3" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-2" value="M023.5MM"/>
<element name="U1" library="Darryl" package="DIP254P762X508-16" value="L293NE">
<attribute name="PACKAGE" value="PDIP-16"/>
<attribute name="OC_NEWARK" value="06F9524"/>
<attribute name="MPN" value="L293NE"/>
<attribute name="SUPPLIER" value="Texas Instruments"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="Darryl" package="DIODE-STICKUP" value="DIODE-SCHOTTKY">
<attribute name="NAME"/>
</element>
<element name="D2" library="Darryl" package="DIODE-STICKUP" value="DIODE-SCHOTTKY">
<attribute name="NAME"/>
</element>
<element name="D4" library="Darryl" package="DIODE-STICKUP" value="DIODE-SCHOTTKY">
<attribute name="NAME"/>
</element>
<element name="D3" library="Darryl" package="DIODE-STICKUP" value="DIODE-SCHOTTKY">
<attribute name="NAME"/>
</element>
<element name="D5" library="Darryl" package="DIODE-STICKUP" value="DIODE-SCHOTTKY">
<attribute name="NAME"/>
</element>
<element name="D6" library="Darryl" package="DIODE-STICKUP" value="DIODE-SCHOTTKY">
<attribute name="NAME"/>
</element>
<element name="D8" library="Darryl" package="DIODE-STICKUP" value="DIODE-SCHOTTKY">
<attribute name="NAME"/>
</element>
<element name="D7" library="Darryl" package="DIODE-STICKUP" value="DIODE-SCHOTTKY">
<attribute name="NAME"/>
</element>
<element name="JP4" library="SparkFun-Connectors" package="1X08_ROUND" value="">
<attribute name="VALUE"/>
</element>
<element name="FRAME1" library="Pictures" package="CREATIVE_COMMONS" value="FRAME-LETTER"/>
</elements>
<signals>
<signal name="5V">
<contactref element="U1" pad="16"/>
<contactref element="JP4" pad="4"/>
</signal>
<signal name="12V">
<contactref element="U1" pad="8"/>
<contactref element="JP1" pad="1"/>
<contactref element="D1" pad="C"/>
<contactref element="D4" pad="C"/>
<contactref element="D5" pad="C"/>
<contactref element="D8" pad="C"/>
</signal>
<signal name="GND">
<contactref element="U1" pad="12"/>
<contactref element="U1" pad="5"/>
<contactref element="U1" pad="4"/>
<contactref element="U1" pad="13"/>
<contactref element="JP1" pad="2"/>
<contactref element="D2" pad="A"/>
<contactref element="D3" pad="A"/>
<contactref element="D6" pad="A"/>
<contactref element="D7" pad="A"/>
<contactref element="JP4" pad="5"/>
</signal>
<signal name="1A">
<contactref element="U1" pad="2"/>
<contactref element="JP4" pad="2"/>
</signal>
<signal name="2A">
<contactref element="U1" pad="7"/>
<contactref element="JP4" pad="3"/>
</signal>
<signal name="3A">
<contactref element="U1" pad="10"/>
<contactref element="JP4" pad="6"/>
</signal>
<signal name="4A">
<contactref element="U1" pad="15"/>
<contactref element="JP4" pad="7"/>
</signal>
<signal name="34EN">
<contactref element="U1" pad="9"/>
<contactref element="JP4" pad="8"/>
</signal>
<signal name="12EN">
<contactref element="U1" pad="1"/>
<contactref element="JP4" pad="1"/>
</signal>
<signal name="4Y">
<contactref element="U1" pad="14"/>
<contactref element="JP3" pad="1"/>
<contactref element="D8" pad="A"/>
<contactref element="D7" pad="C"/>
</signal>
<signal name="3Y">
<contactref element="U1" pad="11"/>
<contactref element="JP3" pad="2"/>
<contactref element="D5" pad="A"/>
<contactref element="D6" pad="C"/>
</signal>
<signal name="2Y">
<contactref element="U1" pad="6"/>
<contactref element="JP2" pad="1"/>
<contactref element="D4" pad="A"/>
<contactref element="D3" pad="C"/>
</signal>
<signal name="1Y">
<contactref element="U1" pad="3"/>
<contactref element="JP2" pad="2"/>
<contactref element="D1" pad="A"/>
<contactref element="D2" pad="C"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
