<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.3.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="53.32" y2="0" width="0" layer="20"/>
<wire x1="53.32" y1="0" x2="53.32" y2="39.04" width="0" layer="20"/>
<wire x1="53.32" y1="39.04" x2="0" y2="39.04" width="0" layer="20"/>
<wire x1="0" y1="39.04" x2="0" y2="0" width="0" layer="20"/>
<text>FL/FR
A</text>
<text>FL/FR
B</text>
<text>RL/RR
A</text>
<text>RL/RR
B</text>
<text>FC/LFE
A</text>
<text>FC/LFE
B</text>
<text>FL/FR
OUT</text>
<text>RL/RR
OUT</text>
<text>FC/LFE
OUT</text>
<text>6-Channel A/B Switch
(c) 2017 Nadia Clawson</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AUDIO-JACK">
<description>&lt;h3&gt;3.5mm Stereo Audio Jack&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:5&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Audio-3.5mm.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;Audio_Jack&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="switch">
<description>&lt;b&gt;Switches&lt;/b&gt;&lt;p&gt;
Marquardt, Siemens, C&amp;K, ITT, and others&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL18">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="FLRA" library="SparkFun-Connectors" package="AUDIO-JACK" value="AUDIO_JACK_3.5MM_PTH">
<attribute name="PROD_ID" value="CONN-08774"/>
<attribute name="SF_ID" value="PRT-08032"/>
</element>
<element name="RLRA" library="SparkFun-Connectors" package="AUDIO-JACK" value="AUDIO_JACK_3.5MM_PTH">
<attribute name="PROD_ID" value="CONN-08774"/>
<attribute name="SF_ID" value="PRT-08032"/>
</element>
<element name="FCSA" library="SparkFun-Connectors" package="AUDIO-JACK" value="AUDIO_JACK_3.5MM_PTH">
<attribute name="PROD_ID" value="CONN-08774"/>
<attribute name="SF_ID" value="PRT-08032"/>
</element>
<element name="FLRB" library="SparkFun-Connectors" package="AUDIO-JACK" value="AUDIO_JACK_3.5MM_PTH">
<attribute name="PROD_ID" value="CONN-08774"/>
<attribute name="SF_ID" value="PRT-08032"/>
</element>
<element name="RLRB" library="SparkFun-Connectors" package="AUDIO-JACK" value="AUDIO_JACK_3.5MM_PTH">
<attribute name="PROD_ID" value="CONN-08774"/>
<attribute name="SF_ID" value="PRT-08032"/>
</element>
<element name="FCSB" library="SparkFun-Connectors" package="AUDIO-JACK" value="AUDIO_JACK_3.5MM_PTH">
<attribute name="PROD_ID" value="CONN-08774"/>
<attribute name="SF_ID" value="PRT-08032"/>
</element>
<element name="FLR" library="SparkFun-Connectors" package="AUDIO-JACK" value="AUDIO_JACK_3.5MM_PTH">
<attribute name="PROD_ID" value="CONN-08774"/>
<attribute name="SF_ID" value="PRT-08032"/>
</element>
<element name="RLR" library="SparkFun-Connectors" package="AUDIO-JACK" value="AUDIO_JACK_3.5MM_PTH">
<attribute name="PROD_ID" value="CONN-08774"/>
<attribute name="SF_ID" value="PRT-08032"/>
</element>
<element name="FCS" library="SparkFun-Connectors" package="AUDIO-JACK" value="AUDIO_JACK_3.5MM_PTH">
<attribute name="PROD_ID" value="CONN-08774"/>
<attribute name="SF_ID" value="PRT-08032"/>
</element>
<element name="S1" library="switch" package="DIL18" value="6PDT"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="S1" pad="2"/>
<contactref element="FLR" pad="TIP"/>
</signal>
<signal name="N$2">
<contactref element="S1" pad="17"/>
<contactref element="FLR" pad="RING"/>
</signal>
<signal name="N$3">
<contactref element="S1" pad="5"/>
<contactref element="RLR" pad="TIP"/>
</signal>
<signal name="N$4">
<contactref element="S1" pad="14"/>
<contactref element="RLR" pad="RING"/>
</signal>
<signal name="N$7">
<contactref element="FLRA" pad="TIP"/>
<contactref element="S1" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="FLRA" pad="RING"/>
<contactref element="S1" pad="18"/>
</signal>
<signal name="N$9">
<contactref element="FLRB" pad="TIP"/>
<contactref element="S1" pad="3"/>
</signal>
<signal name="N$10">
<contactref element="FLRB" pad="RING"/>
<contactref element="S1" pad="16"/>
</signal>
<signal name="N$11">
<contactref element="RLRA" pad="TIP"/>
<contactref element="S1" pad="4"/>
</signal>
<signal name="N$12">
<contactref element="RLRA" pad="RING"/>
<contactref element="S1" pad="15"/>
</signal>
<signal name="N$13">
<contactref element="RLRB" pad="TIP"/>
<contactref element="S1" pad="6"/>
</signal>
<signal name="N$14">
<contactref element="RLRB" pad="RING"/>
<contactref element="S1" pad="13"/>
</signal>
<signal name="N$5">
<contactref element="S1" pad="8"/>
<contactref element="FCS" pad="RING"/>
</signal>
<signal name="N$6">
<contactref element="FCS" pad="TIP"/>
<contactref element="S1" pad="11"/>
</signal>
<signal name="N$15">
<contactref element="FCSA" pad="RING"/>
<contactref element="S1" pad="7"/>
</signal>
<signal name="N$16">
<contactref element="FCSA" pad="TIP"/>
<contactref element="S1" pad="12"/>
</signal>
<signal name="N$17">
<contactref element="FCSB" pad="RING"/>
<contactref element="S1" pad="9"/>
</signal>
<signal name="N$18">
<contactref element="FCSB" pad="TIP"/>
<contactref element="S1" pad="10"/>
</signal>
<signal name="GND">
<contactref element="FLR" pad="SLEEVE"/>
<contactref element="RLR" pad="SLEEVE"/>
<contactref element="FCS" pad="SLEEVE"/>
<contactref element="FCSB" pad="SLEEVE"/>
<contactref element="RLRB" pad="SLEEVE"/>
<contactref element="FLRB" pad="SLEEVE"/>
<contactref element="FCSA" pad="SLEEVE"/>
<contactref element="RLRA" pad="SLEEVE"/>
<contactref element="FLRA" pad="SLEEVE"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
