<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.1.1">
<drawing>
<board>
<plain>
<wire x1="6" y1="7" x2="6" y2="55.04" width="0.1524" layer="20"/>
<wire x1="6" y1="55.04" x2="33.5" y2="55.04" width="0.1524" layer="20"/>
<wire x1="33.5" y1="55.04" x2="33.5" y2="7" width="0.1524" layer="20"/>
<wire x1="6" y1="7" x2="14.5" y2="7" width="0.1524" layer="20"/>
<wire x1="33.5" y1="7" x2="25" y2="7" width="0.1524" layer="20"/>
<wire x1="14.5" y1="7" x2="14.5" y2="11.5" width="0.1524" layer="20"/>
<wire x1="14.5" y1="11.5" x2="25" y2="11.5" width="0.1524" layer="20"/>
<wire x1="25" y1="11.5" x2="25" y2="7" width="0.1524" layer="20"/>
<text>LadybugFC</text>
<text>VL53L1X</text>
<text>PMW3901</text>
<text>3.3V</text>
</plain>
<libraries>
<library name="headers(2mm)">
<packages>
<package name="1X9">
</package>
<package name="1X6">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X03">
<description>&lt;h3&gt;Plated Through Hole - 3 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X04">
<description>&lt;h3&gt;Plated Through Hole - 4 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X02">
<description>&lt;h3&gt;Plated Through Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="LBLFT" library="headers(2mm)" package="1X9" value="1X9"/>
<element name="LBRGT" library="headers(2mm)" package="1X6" value="1X6"/>
<element name="VLLFT" library="SparkFun-Connectors" package="1X03" value=""/>
<element name="VLRGT2" library="SparkFun-Connectors" package="1X03" value=""/>
<element name="PMLFT" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="PROD_ID" value="CONN-09696"/>
</element>
<element name="PMRGT" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="PROD_ID" value="CONN-09696"/>
</element>
<element name="PWPWR" library="SparkFun-Connectors" package="1X02" value=""/>
</elements>
<signals>
<signal name="5V">
<contactref element="LBLFT" pad="7"/>
</signal>
<signal name="TX2/INT">
<contactref element="LBLFT" pad="6"/>
<contactref element="VLLFT" pad="3"/>
</signal>
<signal name="RX2">
<contactref element="LBLFT" pad="5"/>
</signal>
<signal name="A4">
<contactref element="LBLFT" pad="4"/>
</signal>
<signal name="A1/SCK">
<contactref element="LBLFT" pad="3"/>
<contactref element="PMRGT" pad="4"/>
</signal>
<signal name="GND">
<contactref element="LBLFT" pad="2"/>
<contactref element="LBRGT" pad="1"/>
<contactref element="VLLFT" pad="2"/>
<contactref element="PWPWR" pad="2"/>
</signal>
<signal name="3.3V">
<contactref element="LBLFT" pad="1"/>
<contactref element="VLLFT" pad="1"/>
<contactref element="PWPWR" pad="1"/>
</signal>
<signal name="TX1">
<contactref element="LBRGT" pad="6"/>
</signal>
<signal name="A0">
<contactref element="LBRGT" pad="4"/>
</signal>
<signal name="SDA">
<contactref element="LBRGT" pad="3"/>
<contactref element="VLRGT2" pad="1"/>
</signal>
<signal name="SCL">
<contactref element="LBRGT" pad="2"/>
<contactref element="VLRGT2" pad="2"/>
</signal>
<signal name="D5/MOSI">
<contactref element="LBRGT" pad="5"/>
<contactref element="PMLFT" pad="3"/>
</signal>
<signal name="D4/MISO">
<contactref element="LBLFT" pad="9"/>
<contactref element="PMLFT" pad="4"/>
</signal>
<signal name="D10/CS">
<contactref element="LBLFT" pad="8"/>
<contactref element="PMLFT" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
