<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.4.0">
<drawing>
<board>
<plain>
<wire x1="19.05" y1="0" x2="1.27" y2="0" width="0" layer="20"/>
<wire x1="1.27" y1="0" x2="0" y2="1.27" width="0" layer="20" curve="-90"/>
<wire x1="0" y1="1.27" x2="0" y2="19.03125" width="0" layer="20"/>
<wire x1="0" y1="19.03125" x2="1.26875" y2="20.30125" width="0" layer="20" curve="-89.943607"/>
<wire x1="1.26875" y1="20.30125" x2="19.04875" y2="20.31875" width="0" layer="20"/>
<wire x1="19.04875" y1="20.31875" x2="20.32" y2="19.04875" width="0" layer="20" curve="-90.052583"/>
<wire x1="20.32" y1="19.04875" x2="20.32" y2="1.27" width="0" layer="20"/>
<wire x1="20.32" y1="1.27" x2="19.05" y2="0" width="0" layer="20" curve="-90"/>
<text>Out4</text>
<text>Out3</text>
<text>Out2</text>
<text>Out1</text>
<text>+</text>
<text>-</text>
<text>-</text>
<text>-</text>
<text>-</text>
<text>-</text>
<text>-</text>
<text>+</text>
<text>In4</text>
<text>st3/4</text>
<text>In3</text>
<text>In2</text>
<text>st1/2</text>
<text>In1</text>
<text>BTS716G
Breakout
V1.0 2015</text>
<text>Optional Power
Screw Terminal</text>
<text>-</text>
<text>+</text>
<text>+</text>
<text>-</text>
<text>-</text>
<text>-</text>
<text>-</text>
<text>-</text>
<text>4</text>
<text>3</text>
<text>2</text>
<text>1</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>In</text>
<text>Out</text>
</plain>
<libraries>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="EMPTY">
</package>
</packages>
</library>
<library name="infineon">
<description>&lt;b&gt;Infineon Technologies&lt;/b&gt;&lt;p&gt;
http://www.infineon.comp&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="PG-DSO-20">
<description>&lt;b&gt;PG-DSO-20&lt;/b&gt; Plastic Dual Small Outline Package&lt;p&gt;
Source: http://www.infineon.com/products .. BTS176G.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X08_NO_SILK">
</package>
<package name="SCREWTERMINAL-5MM-2">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="FRAME1" library="SparkFun-Aesthetics" package="EMPTY" value="FRAME-LETTERNO_PACKAGE"/>
<element name="IC1" library="infineon" package="PG-DSO-20" value="BTS716G">
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="1X08_NO_SILK" value=""/>
<element name="JP3" library="SparkFun-Connectors" package="SCREWTERMINAL-5MM-2" value="M025MM">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP4" library="SparkFun-Connectors" package="1X08_NO_SILK" value=""/>
</elements>
<signals>
<signal name="VCC">
<contactref element="JP3" pad="1"/>
<contactref element="IC1" pad="1"/>
<contactref element="IC1" pad="10"/>
<contactref element="IC1" pad="11"/>
<contactref element="IC1" pad="12"/>
<contactref element="IC1" pad="15"/>
<contactref element="IC1" pad="16"/>
<contactref element="IC1" pad="19"/>
<contactref element="IC1" pad="20"/>
<contactref element="JP4" pad="8"/>
</signal>
<signal name="GND">
<contactref element="IC1" pad="2"/>
<contactref element="IC1" pad="6"/>
<contactref element="JP3" pad="2"/>
<contactref element="JP1" pad="2"/>
<contactref element="JP1" pad="4"/>
<contactref element="JP1" pad="6"/>
<contactref element="JP1" pad="8"/>
<contactref element="JP4" pad="1"/>
</signal>
<signal name="IN1">
<contactref element="IC1" pad="3"/>
<contactref element="JP4" pad="7"/>
</signal>
<signal name="ST1/2">
<contactref element="IC1" pad="4"/>
<contactref element="JP4" pad="6"/>
</signal>
<signal name="IN2">
<contactref element="IC1" pad="5"/>
<contactref element="JP4" pad="5"/>
</signal>
<signal name="IN3">
<contactref element="IC1" pad="7"/>
<contactref element="JP4" pad="4"/>
</signal>
<signal name="ST3/4">
<contactref element="IC1" pad="8"/>
<contactref element="JP4" pad="3"/>
</signal>
<signal name="IN4">
<contactref element="IC1" pad="9"/>
<contactref element="JP4" pad="2"/>
</signal>
<signal name="OUT1">
<contactref element="JP1" pad="1"/>
<contactref element="IC1" pad="18"/>
</signal>
<signal name="OUT2">
<contactref element="IC1" pad="17"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="OUT3">
<contactref element="JP1" pad="5"/>
<contactref element="IC1" pad="14"/>
</signal>
<signal name="OUT4">
<contactref element="JP1" pad="7"/>
<contactref element="IC1" pad="13"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
