<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="81.73" y1="0" x2="81.73" y2="95" width="0" layer="20"/>
<wire x1="81.73" y1="95" x2="77.73" y2="99" width="0" layer="20" curve="90"/>
<wire x1="77.73" y1="99" x2="4" y2="99" width="0" layer="20"/>
<wire x1="4" y1="99" x2="0" y2="95" width="0" layer="20" curve="90"/>
<wire x1="0" y1="95" x2="0" y2="0" width="0" layer="20"/>
<wire x1="0" y1="0" x2="9.25" y2="0" width="0" layer="20"/>
<wire x1="10.55" y1="-1.3" x2="10.55" y2="-3" width="0" layer="20"/>
<wire x1="10.55" y1="-3" x2="34.415" y2="-3" width="0" layer="20"/>
<wire x1="47.315" y1="-3" x2="71.18" y2="-3" width="0" layer="20"/>
<wire x1="71.18" y1="-3" x2="71.18" y2="-1.3" width="0" layer="20"/>
<wire x1="72.48" y1="0" x2="81.73" y2="0" width="0" layer="20"/>
<wire x1="9.25" y1="0" x2="10.55" y2="-1.3" width="0" layer="20" curve="-90"/>
<wire x1="35.715" y1="0" x2="46.015" y2="0" width="0" layer="20"/>
<wire x1="34.415" y1="-1.3" x2="34.415" y2="-3" width="0" layer="20"/>
<wire x1="47.315" y1="-1.3" x2="47.315" y2="-3" width="0" layer="20"/>
<wire x1="34.415" y1="-1.3" x2="35.715" y2="0" width="0" layer="20" curve="-90"/>
<wire x1="46.015" y1="0" x2="47.315" y2="-1.3" width="0" layer="20" curve="-90"/>
<wire x1="71.18" y1="-1.3" x2="72.48" y2="0" width="0" layer="20" curve="-90"/>
<hole x="5" y="94" drill="3.2"/>
<hole x="76.73" y="94" drill="3.2"/>
</plain>
<libraries>
<library name="phonesat">
<packages>
<package name="SOLAR_CELL">
</package>
<package name="SB_DIODE">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="MOLEX-1X3_LOCK">
</package>
</packages>
</library>
<library name="Burner">
<packages>
<package name="BURNER">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="S3" library="phonesat" package="SOLAR_CELL" value="SOLAR_CELL">
<attribute name="NAME"/>
</element>
<element name="D2" library="phonesat" package="SB_DIODE" value="SB_DIODE">
<attribute name="NAME"/>
</element>
<element name="S18" library="phonesat" package="SOLAR_CELL" value="SOLAR_CELL">
<attribute name="NAME"/>
</element>
<element name="S17" library="phonesat" package="SOLAR_CELL" value="SOLAR_CELL">
<attribute name="NAME"/>
</element>
<element name="S2" library="phonesat" package="SOLAR_CELL" value="SOLAR_CELL">
<attribute name="NAME"/>
</element>
<element name="S19" library="phonesat" package="SOLAR_CELL" value="SOLAR_CELL">
<attribute name="NAME"/>
</element>
<element name="S20" library="phonesat" package="SOLAR_CELL" value="SOLAR_CELL">
<attribute name="NAME"/>
</element>
<element name="S1" library="phonesat" package="SOLAR_CELL" value="SOLAR_CELL">
<attribute name="NAME"/>
</element>
<element name="S15" library="phonesat" package="SOLAR_CELL" value="SOLAR_CELL">
<attribute name="NAME"/>
</element>
<element name="S4" library="phonesat" package="SOLAR_CELL" value="SOLAR_CELL">
<attribute name="NAME"/>
</element>
<element name="S8" library="phonesat" package="SOLAR_CELL" value="SOLAR_CELL">
<attribute name="NAME"/>
</element>
<element name="S7" library="phonesat" package="SOLAR_CELL" value="SOLAR_CELL">
<attribute name="NAME"/>
</element>
<element name="S9" library="phonesat" package="SOLAR_CELL" value="SOLAR_CELL">
<attribute name="NAME"/>
</element>
<element name="S10" library="phonesat" package="SOLAR_CELL" value="SOLAR_CELL">
<attribute name="NAME"/>
</element>
<element name="S5" library="phonesat" package="SOLAR_CELL" value="SOLAR_CELL">
<attribute name="NAME"/>
</element>
<element name="S6" library="phonesat" package="SOLAR_CELL" value="SOLAR_CELL">
<attribute name="NAME"/>
</element>
<element name="D1" library="phonesat" package="SB_DIODE" value="SB_DIODE">
<attribute name="NAME"/>
</element>
<element name="D3" library="phonesat" package="SB_DIODE" value="SB_DIODE">
<attribute name="NAME"/>
</element>
<element name="D4" library="phonesat" package="SB_DIODE" value="SB_DIODE">
<attribute name="NAME"/>
</element>
<element name="D5" library="phonesat" package="SB_DIODE" value="SB_DIODE">
<attribute name="NAME"/>
</element>
<element name="D6" library="phonesat" package="SB_DIODE" value="SB_DIODE">
<attribute name="NAME"/>
</element>
<element name="D7" library="phonesat" package="SB_DIODE" value="SB_DIODE">
<attribute name="NAME"/>
</element>
<element name="D8" library="phonesat" package="SB_DIODE" value="SB_DIODE">
<attribute name="NAME"/>
</element>
<element name="D9" library="phonesat" package="SB_DIODE" value="SB_DIODE">
<attribute name="NAME"/>
</element>
<element name="D10" library="phonesat" package="SB_DIODE" value="SB_DIODE">
<attribute name="NAME"/>
</element>
<element name="D11" library="phonesat" package="SB_DIODE" value="SB_DIODE">
<attribute name="NAME"/>
</element>
<element name="D12" library="phonesat" package="SB_DIODE" value="SB_DIODE">
<attribute name="NAME"/>
</element>
<element name="S11" library="phonesat" package="SOLAR_CELL" value="SOLAR_CELL">
<attribute name="NAME"/>
</element>
<element name="S16" library="phonesat" package="SOLAR_CELL" value="SOLAR_CELL">
<attribute name="NAME"/>
</element>
<element name="S12" library="phonesat" package="SOLAR_CELL" value="SOLAR_CELL">
<attribute name="NAME"/>
</element>
<element name="S14" library="phonesat" package="SOLAR_CELL" value="SOLAR_CELL">
<attribute name="NAME"/>
</element>
<element name="S13" library="phonesat" package="SOLAR_CELL" value="SOLAR_CELL">
<attribute name="NAME"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="MOLEX-1X3_LOCK" value=""/>
<element name="U$1" library="Burner" package="BURNER" value="BURNER"/>
<element name="U$2" library="Burner" package="BURNER" value="BURNER"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="D6" pad="POS"/>
<contactref element="D7" pad="NEG"/>
<contactref element="S12" pad="1"/>
<contactref element="S14" pad="2"/>
<contactref element="S11" pad="1"/>
<contactref element="S13" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="D7" pad="POS"/>
<contactref element="D8" pad="NEG"/>
<contactref element="S14" pad="1"/>
<contactref element="S13" pad="1"/>
<contactref element="S16" pad="2"/>
<contactref element="S15" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="S1" pad="2"/>
<contactref element="D1" pad="NEG"/>
<contactref element="D11" pad="POS"/>
<contactref element="S2" pad="2"/>
</signal>
<signal name="V_SOLAR">
<contactref element="D12" pad="NEG"/>
<contactref element="D11" pad="NEG"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="GND">
<contactref element="D5" pad="POS"/>
<contactref element="D10" pad="POS"/>
<contactref element="S9" pad="1"/>
<contactref element="S10" pad="1"/>
<contactref element="S20" pad="1"/>
<contactref element="S19" pad="1"/>
<contactref element="JP1" pad="1"/>
<contactref element="U$2" pad="H1"/>
<contactref element="U$2" pad="H2"/>
<contactref element="U$2" pad="H3"/>
</signal>
<signal name="N$36">
<contactref element="D8" pad="POS"/>
<contactref element="D9" pad="NEG"/>
<contactref element="S16" pad="1"/>
<contactref element="S18" pad="2"/>
<contactref element="S15" pad="1"/>
<contactref element="S17" pad="2"/>
</signal>
<signal name="N$37">
<contactref element="D2" pad="POS"/>
<contactref element="S3" pad="1"/>
<contactref element="D3" pad="NEG"/>
<contactref element="S4" pad="1"/>
<contactref element="S5" pad="2"/>
<contactref element="S6" pad="2"/>
</signal>
<signal name="N$39">
<contactref element="D3" pad="POS"/>
<contactref element="D4" pad="NEG"/>
<contactref element="S5" pad="1"/>
<contactref element="S6" pad="1"/>
<contactref element="S7" pad="2"/>
<contactref element="S8" pad="2"/>
</signal>
<signal name="N$41">
<contactref element="D9" pad="POS"/>
<contactref element="D10" pad="NEG"/>
<contactref element="S18" pad="1"/>
<contactref element="S20" pad="2"/>
<contactref element="S17" pad="1"/>
<contactref element="S19" pad="2"/>
</signal>
<signal name="N$45">
<contactref element="S1" pad="1"/>
<contactref element="D1" pad="POS"/>
<contactref element="D2" pad="NEG"/>
<contactref element="S3" pad="2"/>
<contactref element="S2" pad="1"/>
<contactref element="S4" pad="2"/>
</signal>
<signal name="N$50">
<contactref element="D4" pad="POS"/>
<contactref element="D5" pad="NEG"/>
<contactref element="S7" pad="1"/>
<contactref element="S9" pad="2"/>
<contactref element="S8" pad="1"/>
<contactref element="S10" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="D6" pad="NEG"/>
<contactref element="D12" pad="POS"/>
<contactref element="S12" pad="2"/>
<contactref element="S11" pad="2"/>
</signal>
<signal name="N$3">
</signal>
<signal name="N$4">
</signal>
<signal name="N$8">
</signal>
<signal name="N$31">
</signal>
<signal name="N$35">
</signal>
<signal name="V_BURN">
<contactref element="JP1" pad="3"/>
<contactref element="U$1" pad="H1"/>
<contactref element="U$1" pad="H2"/>
<contactref element="U$1" pad="H3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
