<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="17.78" y1="17.78" x2="87.3" y2="17.78" width="0" layer="20"/>
<wire x1="87.3" y1="17.78" x2="87.3" y2="49.52" width="0" layer="20"/>
<wire x1="87.3" y1="49.52" x2="17.78" y2="49.52" width="0" layer="20"/>
<wire x1="17.78" y1="49.52" x2="17.78" y2="17.78" width="0" layer="20"/>
<text>ATTINY85</text>
<text>ATTINY84</text>
<text>1</text>
<text>1</text>
<text>1</text>
<hole x="24.13" y="21.59" drill="3.2"/>
<hole x="81.28" y="45.72" drill="3.2"/>
<hole x="24.13" y="45.72" drill="3.2"/>
<hole x="81.28" y="21.59" drill="3.2"/>
<text>ZIF Socket</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X3">
</package>
<package name="DIL28-3-ZIF_SOCKET">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="SparkFun-Connectors" package="2X3" value="AVR_SPI_PRG_6PTH"/>
<element name="U$2" library="SparkFun-Connectors" package="DIL28-3-ZIF_SOCKET" value="ZIFSOCKET-28-3ZIFFSOCKET-28-3"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="U$2" pad="26"/>
<contactref element="J1" pad="1"/>
<contactref element="U$2" pad="17"/>
</signal>
<signal name="N$2">
<contactref element="U$2" pad="25"/>
<contactref element="J1" pad="4"/>
<contactref element="U$2" pad="12"/>
</signal>
<signal name="N$3">
<contactref element="U$2" pad="27"/>
<contactref element="J1" pad="3"/>
<contactref element="U$2" pad="18"/>
</signal>
<signal name="5V">
<contactref element="U$2" pad="28"/>
<contactref element="J1" pad="2"/>
<contactref element="U$2" pad="6"/>
</signal>
<signal name="N$4">
<contactref element="U$2" pad="1"/>
<contactref element="J1" pad="5"/>
<contactref element="U$2" pad="9"/>
</signal>
<signal name="GND">
<contactref element="U$2" pad="4"/>
<contactref element="J1" pad="6"/>
<contactref element="U$2" pad="23"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
